## Profile Comparison between http://hl7.org/fhir/us/core/StructureDefinition/us-core-implantable-device vs http://hl7.org/fhir/us/qicore/StructureDefinition/qicore-device

Left: | US Core Implantable Device Profile (http://hl7.org/fhir/us/core/StructureDefinition/us-core-implantable-device)
Right: | QICore Device (http://hl7.org/fhir/us/qicore/StructureDefinition/qicore-device)

### Messages

Error | StructureDefinition.url | Values for url differ: 'http://hl7.org/fhir/us/core/StructureDefinition/us-core-implantable-device' vs 'http://hl7.org/fhir/us/qicore/StructureDefinition/qicore-device'
Error | StructureDefinition.version | Values for version differ: '8.0.1' vs '7.0.2'
Information | StructureDefinition.name | Values for name differ: 'USCoreImplantableDeviceProfile' vs 'QICoreDevice'
Information | StructureDefinition.title | Values for title differ: 'US Core Implantable Device Profile' vs 'QICore Device'
Information | StructureDefinition.date | Values for date differ: '2023-10-17' vs '2018-08-22'
Information | StructureDefinition.publisher | Values for publisher differ: 'HL7 International / Cross-Group Projects' vs 'HL7 International / Clinical Quality Information'
Information | StructureDefinition.comment | Values for comment differ: 'Some devices may not have UDI information (for example. historical data or patient reported data).' vs 'UDI may identify an unique instance of a device, or it may only identify the type of the device. See [UDI mappings](http://hl7.org/fhir/R4/device-mappings.html#udi) for a complete mapping of UDI parts to Device.'
Warning | Device.udiCarrier | Elements differ in definition for mustSupport: 'true' vs 'false'
Information | Device.udiCarrier | Element maximum cardinalities differ: '1' vs '2147483647'
Warning | Device.udiCarrier.deviceIdentifier | Elements differ in definition for mustSupport: 'true' vs 'false'
Information | Device.udiCarrier.deviceIdentifier | Element minimum cardinalities differ: '1' vs '0'
Warning | Device.udiCarrier.carrierHRF | Elements differ in definition for mustSupport: 'true' vs 'false'
Warning | Device.distinctIdentifier | Elements differ in definition for mustSupport: 'true' vs 'false'
Warning | Device.manufactureDate | Elements differ in definition for mustSupport: 'true' vs 'false'
Warning | Device.expirationDate | Elements differ in definition for mustSupport: 'true' vs 'false'
Warning | Device.lotNumber | Elements differ in definition for mustSupport: 'true' vs 'false'
Warning | Device.serialNumber | Elements differ in definition for mustSupport: 'true' vs 'false'
Warning | Device.type | Elements differ in definition for mustSupport: 'true' vs 'false'
Information | Device.type | Element minimum cardinalities differ: '1' vs '0'
Information | StructureDefinition.short | Values for short differ: 'Patient to whom Device is affixed' vs '(QI) Patient to whom Device is affixed'
Warning | Device.patient | Elements differ in definition for mustSupport: 'true' vs 'false'

### Metadata

Name | Value | Comments
--- | --- | ---
abstract | false |
baseDefinition | http://hl7.org/fhir/StructureDefinition/Device |
copyright | Used by permission of HL7 International, all rights reserved Creative Commons License |  | Removed the item 'Used by permission of HL7 International, all rights reserved Creative Commons License'
date | 2023-10-17 | 2018-08-22 | Values Differ
description | The US Core Device Profile inherits from the FHIR [Device](https://hl7.org/fhir/R4/device.html) resource; refer to it for scope and usage definitions. This profile meets the requirements of the U.S. Core Data for Interoperability (USCDI) *Unique Device Identifier - Implantable* Data Element. It sets minimum expectations for the Device resource to record, search, and fetch UDI information associated with a patient's implantable device(s). It specifies which core elements, extensions, vocabularies, and value sets **SHALL** be present in the resource and constrains how the elements are used. Providing the floor for standards development for specific use cases promotes interoperability and adoption. | Profile of Device for decision support/quality metrics. Defines the core set of elements and extensions for quality rule and measure authors. | Values Differ
experimental | false |
fhirVersion | 4.0.1 |
jurisdiction |  |
jurisdiction[0] | urn:iso:std:iso:3166#US |
kind | resource |
name | USCoreImplantableDeviceProfile | QICoreDevice | Values Differ
publisher | HL7 International / Cross-Group Projects | HL7 International / Clinical Quality Information | Values Differ
purpose |  |
status | active |
title | US Core Implantable Device Profile | QICore Device | Values Differ
type | Device |
url | http://hl7.org/fhir/us/core/StructureDefinition/us-core-implantable-device | http://hl7.org/fhir/us/qicore/StructureDefinition/qicore-device | Values Differ
version | 8.0.1 | 7.0.2 | Values Differ

### Structure

Name | L Flags | L Card. | L Type | L Description & Constraints | R Flags | R Card. | R Type | R Description & Constraints | Comments
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare |  | 0..* | Device | Item used in healthcare |
id | Σ | 0..1 | id | Logical id of this artifact | Σ | 0..1 | id | Logical id of this artifact |
meta | Σ | 0..1 | Meta | Metadata about the resource | Σ | 0..1 | Meta | Metadata about the resource |
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created | ?!Σ | 0..1 | uri | A set of rules under which this content was created |
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
|  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements |
contained |  | 0..* | Resource | Contained, inline Resources |  | 0..* | Resource | Contained, inline Resources |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored | ?! | 0..* | Extension | Extensions that cannot be ignored |
identifier |  | 0..* | Identifier | Instance identifier |  | 0..* | Identifier | Instance identifier |
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device |
udiCarrier | S Σ | 0..1 | BackboneElement | Unique Device Identifier (UDI) Barcode string | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string | Elements differ in definition for mustSupport: 'true' vs 'false' Element maximum cardinalities differ: '1' vs '2147483647'
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
deviceIdentifier | S Σ | 1..1 | string | Mandatory fixed portion of UDI | Σ | 0..1 | string | Mandatory fixed portion of UDI | Elements differ in definition for mustSupport: 'true' vs 'false' Element minimum cardinalities differ: '1' vs '0'
issuer |  | 0..1 | uri | UDI Issuing Organization |  | 0..1 | uri | UDI Issuing Organization |
jurisdiction |  | 0..1 | uri | Regional UDI authority |  | 0..1 | uri | Regional UDI authority |
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String |
carrierHRF | S Σ | 0..1 | string | UDI Human Readable Barcode String | Σ | 0..1 | string | UDI Human Readable Barcode String | Elements differ in definition for mustSupport: 'true' vs 'false'
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered. |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered. |
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device. | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device. |
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device. |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device. |
distinctIdentifier | S | 0..1 | string | The distinct identification string |  | 0..1 | string | The distinct identification string | Elements differ in definition for mustSupport: 'true' vs 'false'
manufacturer |  | 0..1 | string | Name of device manufacturer |  | 0..1 | string | Name of device manufacturer |
manufactureDate | S | 0..1 | dateTime | Date when the device was made |  | 0..1 | dateTime | Date when the device was made | Elements differ in definition for mustSupport: 'true' vs 'false'
expirationDate | S | 0..1 | dateTime | Date and time of expiry of this device (if applicable) |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable) | Elements differ in definition for mustSupport: 'true' vs 'false'
lotNumber | S | 0..1 | string | Lot number of manufacture |  | 0..1 | string | Lot number of manufacture | Elements differ in definition for mustSupport: 'true' vs 'false'
serialNumber | S | 0..1 | string | Serial number assigned by the manufacturer |  | 0..1 | string | Serial number assigned by the manufacturer | Elements differ in definition for mustSupport: 'true' vs 'false'
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer |  | 0..* | BackboneElement | The name of the device as given by the manufacturer |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
name |  | 1..1 | string | The name of the device |  | 1..1 | string | The name of the device |
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by. |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by. |
modelNumber |  | 0..1 | string | The model number for the device |  | 0..1 | string | The model number for the device |
partNumber |  | 0..1 | string | The part number of the device |  | 0..1 | string | The part number of the device |
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: ?? (extensible): Codes to identify medical devices |  | 0..1 | CodeableConcept | The kind or type of device Binding: ?? (example): Codes to identify medical devices. | Elements differ in definition for mustSupport: 'true' vs 'false' Element minimum cardinalities differ: '1' vs '0'
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate |
version |  | 0..1 | string | The version of the standard that is used to operate and communicate |  | 0..1 | string | The version of the standard that is used to operate and communicate |
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device |  | 0..* | BackboneElement | The actual design of the device or software version running on the device |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
type |  | 0..1 | CodeableConcept | The type of the device version |  | 0..1 | CodeableConcept | The type of the device version |
component |  | 0..1 | Identifier | A single component of the device version |  | 0..1 | Identifier | A single component of the device version |
value |  | 1..1 | string | The version text |  | 1..1 | string | The version text |
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible) |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible) |
valueQuantity |  | 0..* | Quantity | Property value as a quantity |  | 0..* | Quantity | Property value as a quantity |
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP) |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP) |
patient | S | 1..1 | Reference(US Core Patient Profile) | Patient to whom Device is affixed |  | 1..1 | Reference(QICore Patient) | (QI) Patient to whom Device is affixed | Elements differ in definition for mustSupport: 'true' vs 'false'
owner |  | 0..1 | Reference(Organization) | Organization responsible for device |  | 0..1 | Reference(Organization) | Organization responsible for device |
contact |  | 0..* | ContactPoint | Details for human/organization for support |  | 0..* | ContactPoint | Details for human/organization for support |
location |  | 0..1 | Reference(Location) | Where the device is found |  | 0..1 | Reference(Location) | Where the device is found |
url |  | 0..1 | uri | Network address to contact device |  | 0..1 | uri | Network address to contact device |
note |  | 0..* | Annotation | Device notes and comments |  | 0..* | Annotation | Device notes and comments |
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device | Σ | 0..* | CodeableConcept | Safety Characteristics of Device |
parent |  | 0..1 | Reference(Device) | The parent device |  | 0..1 | Reference(Device) | The parent device |
Documentation for this format