## Profile Comparison between http://hl7.org/fhir/uv/radiation-dose-summary/StructureDefinition/modality-device vs http://hl7.org/fhir/uv/radiation-dose-summary/StructureDefinition/modality-device

Left: | Modality Device (http://hl7.org/fhir/uv/radiation-dose-summary/StructureDefinition/modality-device)
Right: | Modality Device (http://hl7.org/fhir/uv/radiation-dose-summary/StructureDefinition/modality-device)

### Messages

Error | StructureDefinition.version | Values for version differ: '0.1.0' vs '1.0.0'
Information | StructureDefinition.status | Values for status differ: 'draft' vs 'active'
Warning | StructureDefinition.experimental | Values for experimental differ: 'true' vs 'false'
Information | StructureDefinition.date | Values for date differ: '2021-12-08T15:51:18+00:00' vs '2025-10-29T17:37:08+00:00'
Information | StructureDefinition.publisher | Values for publisher differ: 'HL7 Imaging Integration Working Group' vs 'HL7 International / Imaging Integration'
Information | Device.language | Example/preferred bindings differ at Device.language using binding from ModalityDevice

### Metadata

Name | Value | Comments
--- | --- | ---
abstract | false |
baseDefinition | http://hl7.org/fhir/StructureDefinition/Device |
copyright |  |
date | 2021-12-08T15:51:18+00:00 | 2025-10-29T17:37:08+00:00 | Values Differ
description | Modality profiling as a Device resource |
experimental | true | false | Values Differ
fhirVersion | 4.0.1 |
jurisdiction |  |
jurisdiction[0] | http://unstats.un.org/unsd/methods/m49/m49.htm#001 |
kind | resource |
name | ModalityDevice |
publisher | HL7 Imaging Integration Working Group | HL7 International / Imaging Integration | Values Differ
purpose |  |
status | draft | active | Values Differ
title | Modality Device |
type | Device |
url | http://hl7.org/fhir/uv/radiation-dose-summary/StructureDefinition/modality-device |
version | 0.1.0 | 1.0.0 | Values Differ

### Structure

Name | L Flags | L Card. | L Type | L Description & Constraints | R Flags | R Card. | R Type | R Description & Constraints | Comments
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare |  | 0..* | Device | Item used in healthcare |
id | Σ | 0..1 | string | Logical id of this artifact | Σ | 0..1 | id | Logical id of this artifact |
meta | Σ | 0..1 | Meta | Metadata about the resource | Σ | 0..1 | Meta | Metadata about the resource |
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created | ?!Σ | 0..1 | uri | A set of rules under which this content was created |
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
|  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
| Example/preferred bindings differ at Device.language using binding from ModalityDevice
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements |
contained |  | 0..* | Resource | Contained, inline Resources |  | 0..* | Resource | Contained, inline Resources |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored | ?! | 0..* | Extension | Extensions that cannot be ignored |
Slices for identifier |  | 1..* | Identifier | Instance identifier Slice: Unordered, Open by pattern:type |  | 1..* | Identifier | Instance identifier Slice: Unordered, Open by pattern:type |
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device |
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI | Σ | 0..1 | string | Mandatory fixed portion of UDI |
issuer |  | 0..1 | uri | UDI Issuing Organization |  | 0..1 | uri | UDI Issuing Organization |
jurisdiction |  | 0..1 | uri | Regional UDI authority |  | 0..1 | uri | Regional UDI authority |
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String |
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String | Σ | 0..1 | string | UDI Human Readable Barcode String |
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered. |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered. |
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device. | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device. |
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device. |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device. |
distinctIdentifier |  | 0..1 | string | The distinct identification string |  | 0..1 | string | The distinct identification string |
manufacturer | S | 0..1 | string | The manufacturer of the modality, related to tag(0008,0070) manufacturer | S | 0..1 | string | The manufacturer of the modality, related to tag(0008,0070) manufacturer |
manufactureDate |  | 0..1 | dateTime | Date when the device was made |  | 0..1 | dateTime | Date when the device was made |
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable) |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable) |
lotNumber |  | 0..1 | string | Lot number of manufacture |  | 0..1 | string | Lot number of manufacture |
serialNumber | S | 0..1 | string | The serial number of the modality, which is the Device Serial Number | S | 0..1 | string | The serial number of the modality, which is the Device Serial Number |
Slices for deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer Slice: Unordered, Open by value:type |  | 0..* | BackboneElement | The name of the device as given by the manufacturer Slice: Unordered, Open by value:type |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
name |  | 1..1 | string | The name of the device |  | 1..1 | string | The name of the device |
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by. |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by. |
modelNumber |  | 0..1 | string | The model number for the device |  | 0..1 | string | The model number for the device |
partNumber |  | 0..1 | string | The part number of the device |  | 0..1 | string | The part number of the device |
type | S | 1..1 | CodeableConcept | Describes the main modality type (CT, MG, etc.) Binding: ?? (required) | S | 1..1 | CodeableConcept | Describes the main modality type (CT, MG, etc.) Binding: ?? (required) |
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate |
version |  | 0..1 | string | The version of the standard that is used to operate and communicate |  | 0..1 | string | The version of the standard that is used to operate and communicate |
version |  | 0..* | BackboneElement | Describes the Software Versions of the device, related to tag(0018,1020) Software Versions |  | 0..* | BackboneElement | Describes the Software Versions of the device, related to tag(0018,1020) Software Versions |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
type |  | 0..1 | CodeableConcept | The type of the device version |  | 0..1 | CodeableConcept | The type of the device version |
component |  | 0..1 | Identifier | A single component of the device version |  | 0..1 | Identifier | A single component of the device version |
value |  | 1..1 | string | The version text |  | 1..1 | string | The version text |
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible) |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible) |
valueQuantity |  | 0..* | Quantity | Property value as a quantity |  | 0..* | Quantity | Property value as a quantity |
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP) |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP) |
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed |
owner |  | 0..1 | Reference(Organization) | Organization responsible for device |  | 0..1 | Reference(Organization) | Organization responsible for device |
contact |  | 0..* | ContactPoint | Details for human/organization for support |  | 0..* | ContactPoint | Details for human/organization for support |
location |  | 0..1 | Reference(Location) | Where the device is found |  | 0..1 | Reference(Location) | Where the device is found |
url |  | 0..1 | uri | Network address to contact device |  | 0..1 | uri | Network address to contact device |
note |  | 0..* | Annotation | Device notes and comments |  | 0..* | Annotation | Device notes and comments |
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device | Σ | 0..* | CodeableConcept | Safety Characteristics of Device |
parent |  | 0..1 | Reference(Device) | The parent device |  | 0..1 | Reference(Device) | The parent device |
Documentation for this format