Radiation Dose Summary for Diagnostic Procedures on FHIR
1.0.0 - STU 1

Radiation Dose Summary for Diagnostic Procedures on FHIR, published by HL7 International / Imaging Integration. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/fhir-radiation-dose-summary-ig/ and changes regularly. See the Directory of published versions

## Resource Profile: ModalityDevice - Mappings

Page standards status: Trial-use | Maturity Level: 2

Mappings for the modality-device resource profile.

#### Mappings to Structures in this Implementation Guide

No Mappings Found

#### Mappings to other Structures

No Mappings Found

#### Other Mappings

Name | DICOM Equipement Module | RIM Mapping | FiveWs Pattern Mapping | UDI Mapping
--- | --- | --- | --- | ---
Device | General Equipment Module | Device |  |
id |  |  |  |
meta |  |  |  |
implicitRules |  |  |  |
language |  |  |  |
text |  | Act.text? |  |
contained |  | N/A |  |
extension |  | N/A |  |
modifierExtension |  | N/A |  |
Slices for identifier |  | .id | FiveWs.identifier | The serial number which is a component of the production identifier (PI) a conditional variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
identifier:deviceSerialNumber | tag(0018 1000) Device Serial Number | .id | FiveWs.identifier | The serial number which is a component of the production identifier (PI) a conditional variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
id |  | n/a |  |
extension |  | n/a |  |
use |  | Role.code or implied by context |  |
type |  | Role.code or implied by context |  |
system |  | II.root or Role.id.root |  |
value |  | II.extension or II.root if system indicates OID or GUID (Or Role.id.extension or root) |  |
period |  | Role.effectiveTime or implied by context |  |
assigner |  | II.assigningAuthorityName but note that this is an improper use by the definition of the field. Also Role.scoper |  |
identifier:aeTitle |  | .id | FiveWs.identifier | The serial number which is a component of the production identifier (PI) a conditional variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
id |  | n/a |  |
extension |  | n/a |  |
use |  | Role.code or implied by context |  |
type |  | Role.code or implied by context |  |
system |  | II.root or Role.id.root |  |
value |  | II.extension or II.root if system indicates OID or GUID (Or Role.id.extension or root) |  |
period |  | Role.effectiveTime or implied by context |  |
assigner |  | II.assigningAuthorityName but note that this is an improper use by the definition of the field. Also Role.scoper |  |
identifier:deviceUID | tag(0018 1002) Device UID | .id | FiveWs.identifier | The serial number which is a component of the production identifier (PI) a conditional variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
id |  | n/a |  |
extension |  | n/a |  |
use |  | Role.code or implied by context |  |
type |  | Role.code or implied by context |  |
system |  | II.root or Role.id.root |  |
value |  | II.extension or II.root if system indicates OID or GUID (Or Role.id.extension or root) |  |
period |  | Role.effectiveTime or implied by context |  |
assigner |  | II.assigningAuthorityName but note that this is an improper use by the definition of the field. Also Role.scoper |  |
identifier:deviceID |  | .id | FiveWs.identifier | The serial number which is a component of the production identifier (PI) a conditional variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
id |  | n/a |  |
extension |  | n/a |  |
use |  | Role.code or implied by context |  |
type |  | Role.code or implied by context |  |
system |  | II.root or Role.id.root |  |
value |  | II.extension or II.root if system indicates OID or GUID (Or Role.id.extension or root) |  |
period |  | Role.effectiveTime or implied by context |  |
assigner |  | II.assigningAuthorityName but note that this is an improper use by the definition of the field. Also Role.scoper |  |
definition |  |  |  |
udiCarrier |  | .id and .code | FiveWs.identifier |
id |  | n/a |  |
extension |  | n/a |  |
modifierExtension |  | N/A |  |
deviceIdentifier |  | Role.id.extension | FiveWs.what[x] | The device identifier (DI) a mandatory fixed portion of a UDI that identifies the labeler and the specific version or model of a device.
issuer |  | Role.id.root |  | http://hl7.org/fhir/NamingSystem/gs1 HIBCC DIs: http://hl7.org/fhir/NamingSystem/hibcc ICCBBA DIs for blood containers: http://hl7.org/fhir/NamingSystem/iccbba-blood ICCBA DIs for other devices: http://hl7.org/fhir/NamingSystem/iccbba-other
jurisdiction |  | Role.scoper |  |
carrierAIDC |  | Role.id.extension |  | A unique device identifier (UDI) on a device label a form that uses automatic identification and data capture (AIDC) technology.
carrierHRF |  | Role.id.extension |  | A unique device identifier (UDI) on a device label in plain text
entryType |  | NA |  |
status |  | .statusCode | FiveWs.status |
statusReason |  |  | FiveWs.status |
distinctIdentifier |  | .lotNumberText | FiveWs.what[x] | The lot or batch number within which a device was manufactured - which is a component of the production identifier (PI) a conditional variable portion of a UDI.
manufacturer | tag(0008 0070) manufacturer | .playedRole[typeCode=MANU].scoper.name | FiveWs.what[x] | N/A
manufactureDate |  | .existenceTime.low | FiveWs.what[x] | The date a specific device was manufactured - which is a component of the production identifier (PI) a conditional variable portion of a UDI. For FHIR MM:SS]. If hour is present the minutes and seconds should both be set to “00”.
expirationDate |  | .expirationTime | FiveWs.what[x] | the expiration date of a specific device - which is a component of the production identifier (PI) a conditional variable portion of a UDI. For FHIR MM:SS]. If hour is present the minutes and seconds should both be set to “00”.
lotNumber |  | .lotNumberText | FiveWs.what[x] | The lot or batch number within which a device was manufactured - which is a component of the production identifier (PI) a conditional variable portion of a UDI.
serialNumber | tag(0018 1000) Device Serial Number | .playedRole[typeCode=MANU].id | FiveWs.what[x] |
Slices for deviceName |  |  |  |
deviceName:All Slices |  |  |  |
id |  | n/a |  |
extension |  | n/a |  |
modifierExtension |  | N/A |  |
name |  |  |  |
type |  | .playedRole[typeCode=MANU].code | FiveWs.what[x] |
deviceName:manufacturer | tag(0008 0070) manufacturer |  |  |
id |  | n/a |  |
extension |  | n/a |  |
modifierExtension |  | N/A |  |
name |  |  |  |
type |  | .playedRole[typeCode=MANU].code | FiveWs.what[x] |
deviceName:manufacturerModelName | tag(0008 1090) Manufacturer's Model Name |  |  |
id |  | n/a |  |
extension |  | n/a |  |
modifierExtension |  | N/A |  |
name |  |  |  |
type |  | .playedRole[typeCode=MANU].code | FiveWs.what[x] |
modelNumber |  | .softwareName (included as part) | FiveWs.what[x] |
partNumber |  | .playedRole[typeCode=MANU].id | FiveWs.what[x] |
type |  |  |  |
specialization |  |  |  |
id |  | n/a |  |
extension |  | n/a |  |
modifierExtension |  | N/A |  |
systemType |  |  |  |
version |  |  | FiveWs.what[x] |
version |  |  |  |
id |  | n/a |  |
extension |  | n/a |  |
modifierExtension |  | N/A |  |
type |  |  |  |
component |  |  | FiveWs.what[x] |
value |  |  |  |
property |  |  |  |
id |  | n/a |  |
extension |  | n/a |  |
modifierExtension |  | N/A |  |
type |  |  |  |
valueQuantity |  |  |  |
valueCode |  |  |  |
patient |  | .playedRole[typeCode=USED].scoper.playedRole[typeCode=PAT] | FiveWs.subject |
owner |  | .playedRole[typeCode=OWN].scoper | FiveWs.source |
contact |  | .scopedRole[typeCode=CON].player | FiveWs.source |
location |  | .playedRole[typeCode=LOCE].scoper | FiveWs.where[x] |
url |  | .telecom | FiveWs.where[x] |
note |  | .text |  |
safety |  | NA |  |
parent |  |  |  |
Documentation for this format