Radiation Dose Summary for Diagnostic Procedures on FHIR
1.0.0 - STU 1

Radiation Dose Summary for Diagnostic Procedures on FHIR, published by HL7 International / Imaging Integration. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/fhir-radiation-dose-summary-ig/ and changes regularly. See the Directory of published versions

## ValueSet: Procedure Reported Type Value Set

Official URL: http://hl7.org/fhir/uv/radiation-dose-summary/ValueSet/procedure-reported-type-rds-vs | Version: 1.0.0
Standards status: Trial-use | Maturity Level: 2 | Computable Name: ProcedureReportedTypeVS
Copyright/Legal: This value set includes content from SNOMED CT, which is copyright © 2002+ International Health Terminology Standards Development Organisation (IHTSDO), and distributed by agreement between IHTSDO and HL7. Implementer use of SNOMED CT is not covered by this agreement.

What is the type of procedure reported in the Radiation Dose Summary

References

This value set is not used here; it may be used elsewhere (e.g. specifications and/or implementations that use this content)

### Logical Definition (CLD)

This value set includes codes based on the following rules:

- Include these codes as defined in `http://dicom.nema.org/resources/ontology/DCM` version `2025.2.20250411`

  Code | Display | Definition
  113502 | Radiopharmaceutical Administration | Information pertaining to the administration of a radiopharmaceutical
  113704 | Projection X-Ray | Imaging using a point X-Ray source with a diverging beam projected onto a 2 dimensional detector.

- Include these codes as defined in `http://snomed.info/sct`

  Code | Display
  77477000 | Computerized tomography
  71651007 | Mammography

### Expansion

Expansion from tx.fhir.org based on:

- codesystem DICOM Controlled Terminology Definitions v2025.2.20250411 (CodeSystem)
- SNOMED CT International edition 01-Feb 2025

This value set contains 4 concepts

Code | System | Display | Definition
113502 | http://dicom.nema.org/resources/ontology/DCM | Radiopharmaceutical Administration | Information pertaining to the administration of a radiopharmaceutical
113704 | http://dicom.nema.org/resources/ontology/DCM | Projection X-Ray | Imaging using a point X-Ray source with a diverging beam projected onto a 2 dimensional detector.
77477000 | http://snomed.info/sct | Computerized axial tomography |
71651007 | http://snomed.info/sct | Mammography |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code