Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Heart Rate Numeric metric example - TTL Representation

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:DeviceMetric ;
      fhir:nodeRole fhir:treeRoot ;
      fhir:id [ fhir:v "HeartRateNumericDeviceMetric"] ; #
      fhir:meta [
        ( fhir:profile [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericDeviceMetric"^^xsd:anyURI ;
    fhir:link <http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericDeviceMetric>     ] )
      ] ; #
      fhir:text [
    fhir:status [ fhir:v "extensions" ] ;
    fhir:div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p><b>Generated Narrative: DeviceMetric</b><a name=\"HeartRateNumericDeviceMetric\"> </a></p><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\">Resource DeviceMetric &quot;HeartRateNumericDeviceMetric&quot; </p><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-NumericDeviceMetric.html\">Numeric DeviceMetric profile</a></p></div><blockquote><p><b>Relation extension</b></p><blockquote><p><b>url</b></p><code>kind</code></blockquote><p><b>value</b>: DCE</p><blockquote><p><b>url</b></p><code>entries</code></blockquote><p><b>value</b>: <a href=\"DeviceMetric-ECGSampleArrayDeviceMetric.html\">DeviceMetric/ECGSampleArrayDeviceMetric</a></p></blockquote><blockquote><p><b>Technical range extension</b></p><blockquote><p><b>url</b></p><code>lowerLimit</code></blockquote><p><b>value</b>: 0</p><blockquote><p><b>url</b></p><code>upperLimit</code></blockquote><p><b>value</b>: 200</p><blockquote><p><b>url</b></p><code>stepWidth</code></blockquote><p><b>value</b>: 1</p><blockquote><p><b>url</b></p><code>relativeAccuracy</code></blockquote><p><b>value</b>: 0.01</p><blockquote><p><b>url</b></p><code>absoluteAccuracy</code></blockquote><p><b>value</b>: 0.01</p></blockquote><p><b>type</b>: HR <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#147842 &quot;MDC_ECG_HEART_RATE&quot;)</span></p><p><b>unit</b>: bpm <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#264864 &quot;MDC_DIM_BEAT_PER_MIN&quot;)</span></p><p><b>source</b>: <a href=\"Device-PhysioMonitorMdsDevice.html\">Device/PhysioMonitorMdsDevice</a></p><p><b>parent</b>: <a href=\"Device-HeartRateChannelDevice.html\">Device/HeartRateChannelDevice</a></p><p><b>operationalStatus</b>: on</p><p><b>color</b>: green</p><p><b>category</b>: measurement</p></div>"
      ] ; #
      fhir:extension ( [
    fhir:url [ fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/relation"^^xsd:anyURI ] ;
        ( fhir:extension [
    fhir:url [ fhir:v "kind"^^xsd:anyURI ] ;
    fhir:value [ fhir:v "DCE" ]     ] [
    fhir:url [ fhir:v "entries"^^xsd:anyURI ] ;
    fhir:value [
    a fhir:Reference ;
    fhir:reference [ fhir:v "DeviceMetric/ECGSampleArrayDeviceMetric" ]       ]     ] )
      ] [
    fhir:url [ fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/technical-range"^^xsd:anyURI ] ;
        ( fhir:extension [
    fhir:url [ fhir:v "lowerLimit"^^xsd:anyURI ] ;
    fhir:value [ fhir:v "0"^^xsd:decimal ]     ] [
    fhir:url [ fhir:v "upperLimit"^^xsd:anyURI ] ;
    fhir:value [ fhir:v "200"^^xsd:decimal ]     ] [
    fhir:url [ fhir:v "stepWidth"^^xsd:anyURI ] ;
    fhir:value [ fhir:v "1"^^xsd:decimal ]     ] [
    fhir:url [ fhir:v "relativeAccuracy"^^xsd:anyURI ] ;
    fhir:value [ fhir:v "0.01"^^xsd:decimal ]     ] [
    fhir:url [ fhir:v "absoluteAccuracy"^^xsd:anyURI ] ;
    fhir:value [ fhir:v "0.01"^^xsd:decimal ]     ] )
      ] ) ; #
      fhir:type [
        ( fhir:coding [
    fhir:system [ fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "147842" ] ;
    fhir:display [ fhir:v "MDC_ECG_HEART_RATE" ]     ] ) ;
    fhir:text [ fhir:v "HR" ]
      ] ; #
      fhir:unit [
        ( fhir:coding [
    fhir:system [ fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "264864" ] ;
    fhir:display [ fhir:v "MDC_DIM_BEAT_PER_MIN" ]     ] ) ;
    fhir:text [ fhir:v "bpm" ]
      ] ; #
      fhir:source [
    fhir:reference [ fhir:v "Device/PhysioMonitorMdsDevice" ]
      ] ; #
      fhir:parent [
    fhir:reference [ fhir:v "Device/HeartRateChannelDevice" ]
      ] ; #
      fhir:operationalStatus [ fhir:v "on"] ; #
      fhir:color [ fhir:v "green"] ; #
      fhir:category [ fhir:v "measurement"] . #