Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## CodeSystem: Operating mode code system

Official URL: http://hl7.org/fhir/uv/pocd/CodeSystem/operating-mode | Version: current
Draft as of 2020-05-12 | Computable Name: OperatingMode

CodeSystem for IEEE 11073-10207 MdsState/OperatingMode

This Code system is referenced in the content logical definition of the following value sets:

- OperatingMode

This code system `http://hl7.org/fhir/uv/pocd/CodeSystem/operating-mode` defines the following codes:

Code | Display | Definition
Nml | Normal | The POC MEDICAL DEVICE operates in a mode that supports the fulfillment of its clinical functions.
Dmo | Demo | The POC MEDICAL DEVICE operates in a mode that is intended for demonstration purposes only. Arbitrary values are generated.
Srv | Service | The POC MEDICAL DEVICE operates in a mode that is intended for services purposes only.
Mtn | Maintenance | Maintenance. The POC MEDICAL DEVICE operates in a mode that is intended for maintenance purposes only.