Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Measurement status codes - TTL Representation

Draft as of 2019-09-28

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:CodeSystem ;
      fhir:nodeRole fhir:treeRoot ;
      fhir:id [ fhir:v "measurement-status"] ; #
      fhir:meta [
        ( fhir:profile [
    fhir:v "http://hl7.org/fhir/StructureDefinition/shareablecodesystem"^^xsd:anyURI ;
    fhir:link <http://hl7.org/fhir/StructureDefinition/shareablecodesystem>     ] )
      ] ; #
      fhir:text [
    fhir:status [ fhir:v "generated" ] ;
    fhir:div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p>This code system <code>http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status</code> defines the following codes:</p><table class=\"codes\"><tr><td style=\"white-space:nowrap\"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style=\"white-space:nowrap\">questionable<a name=\"measurement-status-questionable\"> </a></td><td>Questionable</td><td>Data may not be reliable</td></tr><tr><td style=\"white-space:nowrap\">calibration-ongoing<a name=\"measurement-status-calibration-ongoing\"> </a></td><td>Calibration ongoing</td><td>Calibration is ongoing</td></tr><tr><td style=\"white-space:nowrap\">validated-data<a name=\"measurement-status-validated-data\"> </a></td><td>Validated data</td><td>Relevant, e.g., in an archive</td></tr><tr><td style=\"white-space:nowrap\">early-indication<a name=\"measurement-status-early-indication\"> </a></td><td>Early indication</td><td>Early estimate of value</td></tr><tr><td style=\"white-space:nowrap\">msmt-ongoing<a name=\"measurement-status-msmt-ongoing\"> </a></td><td>Measurement ongoing</td><td>Indicates that a new measurement is just being taken</td></tr><tr><td style=\"white-space:nowrap\">in-alarm<a name=\"measurement-status-in-alarm\"> </a></td><td>Measurement in alarm</td><td>Measurement has an active alarm condition</td></tr><tr><td style=\"white-space:nowrap\">alarm-inhibited<a name=\"measurement-status-alarm-inhibited\"> </a></td><td>Measurement alarms inhibited</td><td>Measurement supports alarming and alarms are turned off</td></tr></table></div>"
      ] ; #
      fhir:url [ fhir:v "http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status"^^xsd:anyURI] ; #
      fhir:version [ fhir:v "current"] ; #
      fhir:name [ fhir:v "MeasurementStatus"] ; #
      fhir:title [ fhir:v "Measurement status codes"] ; #
      fhir:status [ fhir:v "draft"] ; #
      fhir:experimental [ fhir:v "false"^^xsd:boolean] ; #
      fhir:date [ fhir:v "2019-09-28"^^xsd:date] ; #
      fhir:publisher [ fhir:v "HL7 International - Devices Work Group"] ; #
      fhir:contact ( [
        ( fhir:telecom [
    fhir:system [ fhir:v "url" ] ;
    fhir:value [ fhir:v "http://hl7.org/Special/committees/healthcaredevices" ]     ] )
      ] ) ; #
      fhir:description [ fhir:v "Measurement status definitions from the ISO/IEEE 11073-10201 DIM."] ; #
      fhir:jurisdiction ( [
        ( fhir:coding [
    fhir:system [ fhir:v "http://unstats.un.org/unsd/methods/m49/m49.htm"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "001" ]     ] )
      ] ) ; #
      fhir:caseSensitive [ fhir:v "false"^^xsd:boolean] ; #
      fhir:content [ fhir:v "complete"] ; #
      fhir:concept ( [
    fhir:code [ fhir:v "questionable" ] ;
    fhir:display [ fhir:v "Questionable" ] ;
    fhir:definition [ fhir:v "Data may not be reliable" ]
      ] [
    fhir:code [ fhir:v "calibration-ongoing" ] ;
    fhir:display [ fhir:v "Calibration ongoing" ] ;
    fhir:definition [ fhir:v "Calibration is ongoing" ]
      ] [
    fhir:code [ fhir:v "validated-data" ] ;
    fhir:display [ fhir:v "Validated data" ] ;
    fhir:definition [ fhir:v "Relevant, e.g., in an archive" ]
      ] [
    fhir:code [ fhir:v "early-indication" ] ;
    fhir:display [ fhir:v "Early indication" ] ;
    fhir:definition [ fhir:v "Early estimate of value" ]
      ] [
    fhir:code [ fhir:v "msmt-ongoing" ] ;
    fhir:display [ fhir:v "Measurement ongoing" ] ;
    fhir:definition [ fhir:v "Indicates that a new measurement is just being taken" ]
      ] [
    fhir:code [ fhir:v "in-alarm" ] ;
    fhir:display [ fhir:v "Measurement in alarm" ] ;
    fhir:definition [ fhir:v "Measurement has an active alarm condition" ]
      ] [
    fhir:code [ fhir:v "alarm-inhibited" ] ;
    fhir:display [ fhir:v "Measurement alarms inhibited" ] ;
    fhir:definition [ fhir:v "Measurement supports alarming and alarms are turned off" ]
      ] ) . #