Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Resource Profile: MdsDevice - Detailed Descriptions

Draft as of 2022-01-16

Definitions for the MdsDevice resource profile.

- Differential Elements Table
- Key Elements Table
- Snapshot Elements Table

Guidance on how to interpret the contents of this table can be found here.

1. Device
Invariants | Defined on this element pocd-dev-1: Must have at least identifier or udiCarrier (: identifier.exists() or udiCarrier.exists())
2. Device.extension
Slicing | This element introduces a set of slices on Device.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
3. Device.extension:approvedJurisdictions
SliceName | approvedJurisdictions
Definition | List of regions in which a device is approved to be operated.
Control | 0..?
Type | Extension(ApprovedJurisdictions) (Extension Type: CodeableConcept)
Must Support | true
4. Device.extension:approvedJurisdictions.valueCodeableConcept
Control | 0..?
5. Device.extension:approvedJurisdictions.valueCodeableConcept.coding
Control | 0..?
6. Device.extension:approvedJurisdictions.valueCodeableConcept.coding.system
Control | 0..?
7. Device.extension:approvedJurisdictions.valueCodeableConcept.coding.code
Control | 0..?
8. Device.extension:operator
SliceName | operator
Definition | Identifies an operator of the device.
Control | 0..1
Type | Extension(Operator) (Extension Type: Reference(Practitioner))
Must Support | true
9. Device.extension:operatingHours
SliceName | operatingHours
Definition | Optional amount of operating hours (e.g., an OR light).
Control | 0..1
Type | Extension(OperatingHours) (Extension Type: unsignedInt)
Must Support | true
10. Device.extension:operatingHours.valueUnsignedInt
Control | 0..?
11. Device.extension:operatingCycles
SliceName | operatingCycles
Definition | Optional amount of operating cycles, e.g., the number of measurements taken within the component.
Control | 0..1
Type | Extension(OperatingCycles) (Extension Type: unsignedInt)
Must Support | true
12. Device.extension:operatingCycles.valueUnsignedInt
Control | 0..?
13. Device.extension:operatingMode
SliceName | operatingMode
Definition | Operating mode that defines the interpretation constraints of the data that is provided.
Control | 0..1
Type | Extension(OperatingMode) (Extension Type: code)
Must Support | true
14. Device.extension:operatingMode.valueCode
Control | 0..?
15. Device.identifier
Note | This is a business identifier, not a resource identifier (see discussion)
Control | This element is affected by the following invariants: pocd-dev-1
Must Support | true
Slicing | This element introduces a set of slices on Device.identifier. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ system
16. Device.identifier:EUI-64
SliceName | EUI-64
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 0..1
17. Device.identifier:EUI-64.system
Control | 1..?
Fixed Value | urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680
18. Device.identifier:EUI-64.value
Control | 1..?
19. Device.udiCarrier
Control | This element is affected by the following invariants: pocd-dev-1
Must Support | true
20. Device.udiCarrier.deviceIdentifier
21. Device.udiCarrier.issuer
22. Device.udiCarrier.jurisdiction
23. Device.udiCarrier.carrierHRF
24. Device.status
Must Support | true
25. Device.statusReason
Must Support | true
26. Device.manufacturer
Must Support | true
27. Device.manufactureDate
28. Device.expirationDate
29. Device.lotNumber
30. Device.serialNumber
Must Support | true
31. Device.deviceName
Must Support | true
32. Device.deviceName.name
33. Device.modelNumber
Must Support | true
34. Device.partNumber
Must Support | true
35. Device.type
Control | 10..1
Binding | The codes SHALL be taken from MDC Object infrastructure and Device nomenclature; other codes may be used where these codes are not suitableFor example codes, see DeviceType
Must Support | true
36. Device.type.coding
Control | 0..?
37. Device.type.coding.system
Control | 0..?
38. Device.type.coding.version
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..?
39. Device.type.coding.code
Control | 0..?
40. Device.version
Note | This is a business versionId, not a resource version id (see discussion)
Must Support | true
41. Device.version.type
42. Device.version.type.coding
Control | 0..?
43. Device.version.type.coding.system
Control | 0..?
44. Device.version.type.coding.version
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..?
45. Device.version.type.coding.code
Control | 0..?
46. Device.version.component
47. Device.version.value
48. Device.property
49. Device.property.type
50. Device.property.type.coding
Control | 0..?
51. Device.property.type.coding.system
Control | 0..?
52. Device.property.type.coding.version
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..?
53. Device.property.type.coding.code
Control | 0..?
54. Device.property.valueCode
55. Device.property.valueCode.coding
Control | 0..?
56. Device.property.valueCode.coding.system
Control | 0..?
57. Device.property.valueCode.coding.version
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..?
58. Device.property.valueCode.coding.code
Control | 0..?
59. Device.patient
Must Support | true
60. Device.location
Must Support | true
61. Device.safety
Binding | The codes SHALL be taken from Safety; other codes may be used where these codes are not suitableFor codes, see (unbound) Safety classificatio
Must Support | true
62. Device.safety.coding
Control | 0..?
63. Device.safety.coding.system
Definition | http://hl7.org/fhir/uv/pocd/ValueSet/safety
Control | 0..?
64. Device.safety.coding.code
Control | 0..?
65. Device.parent
Type | Reference(MdsDevice|Device)
Must Support | true

Guidance on how to interpret the contents of this table can be found here.

1. Device
Definition | A type of a manufactured item that is used in the provision of healthcare without being substantially changed through that activity. The device may be a medical or non-medical device.
Control | 0..*
Summary | false
Invariants | Defined on this element dom-2: If the resource is contained in another resource, it SHALL NOT contain nested Resources (: contained.contained.empty()) dom-3: If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource (: contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()) dom-4: If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated (: contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()) dom-5: If a resource is contained in another resource, it SHALL NOT have a security label (: contained.meta.security.empty()) dom-6: A resource should have narrative for robust management (: text.`div`.exists()) pocd-dev-1: Must have at least identifier or udiCarrier (: identifier.exists() or udiCarrier.exists())
2. Device.implicitRules
Definition | A reference to a set of rules that were followed when the resource was constructed, and which must be understood when processing the content. Often, this is a reference to an implementation guide that defines the special rules along with other profiles etc.
Control | 0..1
Type | uri
Is Modifier | true
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Asserting this rule set restricts the content to be only understood by a limited set of trading partners. This inherently limits the usefulness of the data in the long term. However, the existing health eco-system is highly fractured, and not yet ready to define, collect, and exchange data in a generally computable sense. Wherever possible, implementers and/or specification writers should avoid using this element. Often, when used, the URL is a reference to an implementation guide that defines these special rules as part of it's narrative along with other profiles, value sets, etc.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
3. Device.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the resource. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
4. Device.extension:approvedJurisdictions
SliceName | approvedJurisdictions
Definition | List of regions in which a device is approved to be operated.
Control | 0..* This element is affected by the following invariants: ele-1
Type | Extension(ApprovedJurisdictions) (Extension Type: CodeableConcept)
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
5. Device.extension:approvedJurisdictions.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..0*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
6. Device.extension:approvedJurisdictions.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Control | 1..1
Type | uri
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Fixed Value | http://hl7.org/fhir/uv/pocd/StructureDefinition/approved-jurisdictions
7. Device.extension:approvedJurisdictions.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 10..1
Type | Choice of: CodeableConcept, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | See Choice of Data Types for further information about how to use [x]
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.extension.value[x]. The slices are unordered and Closed, and can be differentiated using the following discriminators: type @ $this
8. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept
SliceName | valueCodeableConcept
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 10..1
Binding | The codes SHALL be taken from Jurisdiction ValueSet; other codes may be used where these codes are not suitableFor codes, see (unbound) Codes for country, country subdivision and regio
Type | Choice of: CodeableConcept, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | See Choice of Data Types for further information about how to use [x]
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
9. Device.extension:operator
SliceName | operator
Definition | Identifies an operator of the device.
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Operator) (Extension Type: Reference(Practitioner))
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
10. Device.extension:operatingHours
SliceName | operatingHours
Definition | Optional amount of operating hours (e.g., an OR light).
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(OperatingHours) (Extension Type: unsignedInt)
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
11. Device.extension:operatingHours.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..0*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
12. Device.extension:operatingHours.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Control | 1..1
Type | uri
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Fixed Value | http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours
13. Device.extension:operatingHours.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 10..1
Type | Choice of: unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.extension.value[x]. The slices are unordered and Closed, and can be differentiated using the following discriminators: type @ $this
14. Device.extension:operatingHours.value[x]:valueUnsignedInt
SliceName | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 10..1
Type | Choice of: unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
15. Device.extension:operatingCycles
SliceName | operatingCycles
Definition | Optional amount of operating cycles, e.g., the number of measurements taken within the component.
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(OperatingCycles) (Extension Type: unsignedInt)
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
16. Device.extension:operatingCycles.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..0*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
17. Device.extension:operatingCycles.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Control | 1..1
Type | uri
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Fixed Value | http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles
18. Device.extension:operatingCycles.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 10..1
Type | Choice of: unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.extension.value[x]. The slices are unordered and Closed, and can be differentiated using the following discriminators: type @ $this
19. Device.extension:operatingCycles.value[x]:valueUnsignedInt
SliceName | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 10..1
Type | Choice of: unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
20. Device.extension:operatingMode
SliceName | operatingMode
Definition | Operating mode that defines the interpretation constraints of the data that is provided.
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(OperatingMode) (Extension Type: code)
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
21. Device.extension:operatingMode.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..0*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
22. Device.extension:operatingMode.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Control | 1..1
Type | uri
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Fixed Value | http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode
23. Device.extension:operatingMode.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 10..1
Binding | The codes SHALL be taken from Operating Mode; other codes may be used where these codes are not suitableFor codes, see (unbound) Codes that indicate the device operating mod
Type | Choice of: code, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.extension.value[x]. The slices are unordered and Closed, and can be differentiated using the following discriminators: type @ $this
24. Device.extension:operatingMode.value[x]:valueCode
SliceName | valueCode
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 10..1
Binding | The codes SHALL be taken from Operating Mode; other codes may be used where these codes are not suitableFor codes, see (unbound) Codes that indicate the device operating mod
Type | Choice of: code, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
25. Device.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the resource and that modifies the understanding of the element that contains it and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer is allowed to define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | false
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
26. Device.identifier
Definition | Unique instance identifiers assigned to a device by manufacturers other organizations or owners.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 0..* This element is affected by the following invariants: pocd-dev-1
Type | Identifier
Must Support | true
Summary | false
Comments | The barcode string from a barcode present on a device label or package may identify the instance, include names given to the device in local usage, or may identify the type of device. If the identifier identifies the type of device, Device.type element should be used.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.identifier. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ system
27. Device.identifier:EUI-64
SliceName | EUI-64
Definition | Unique instance identifiers assigned to a device by manufacturers other organizations or owners.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 0..1*
Type | Identifier
Summary | false
Comments | The barcode string from a barcode present on a device label or package may identify the instance, include names given to the device in local usage, or may identify the type of device. If the identifier identifies the type of device, Device.type element should be used.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
28. Device.identifier:EUI-64.use
Definition | The purpose of this identifier.
Control | 0..1
Binding | The codes SHALL be taken from IdentifierUse Identifies the purpose for this identifier, if known .
Type | code
Is Modifier | true
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Allows the appropriate identifier for a particular context of use to be selected from among a set of identifiers.
Comments | Applications can assume that an identifier is permanent unless it explicitly says that it is temporary.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
29. Device.identifier:EUI-64.system
Definition | Establishes the namespace for the value - that is, a URL that describes a set values that are unique.
Control | 10..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | There are many sets of identifiers. To perform matching of two identifiers, we need to know what set we're dealing with. The system identifies a particular set of unique identifiers.
Comments | Identifier.system is always case sensitive.
Fixed Value | urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680
Example | General:http://www.acme.com/identifiers/patient
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
30. Device.identifier:EUI-64.value
Definition | The portion of the identifier typically relevant to the user and which is unique within the context of the system.
Control | 10..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | If the value is a full URI, then the system SHALL be urn:ietf:rfc:3986. The value's primary purpose is computational mapping. As a result, it may be normalized for comparison purposes (e.g. removing non-significant whitespace, dashes, etc.) A value formatted for human display can be conveyed using the Rendered Value extension. Identifier.value is to be treated as case sensitive unless knowledge of the Identifier.system allows the processer to be confident that non-case-sensitive processing is safe.
Example | General:123456
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
31. Device.udiCarrier
Definition | Unique device identifier (UDI) assigned to device label or package. Note that the Device may include multiple udiCarriers as it either may include just the udiCarrier for the jurisdiction it is sold, or for multiple jurisdictions it could have been sold.
Control | 0..* This element is affected by the following invariants: pocd-dev-1
Type | BackboneElement
Must Support | true
Summary | true
Comments | UDI may identify an unique instance of a device, or it may only identify the type of the device. See UDI mappings for a complete mapping of UDI parts to Device.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
32. Device.udiCarrier.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
33. Device.udiCarrier.deviceIdentifier
Definition | The device identifier (DI) is a mandatory, fixed portion of a UDI that identifies the labeler and the specific version or model of a device.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | DI
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
34. Device.udiCarrier.issuer
Definition | Organization that is charged with issuing UDIs for devices. For example, the US FDA issuers include : GS1: http://hl7.org/fhir/NamingSystem/gs1-di, HIBCC: http://hl7.org/fhir/NamingSystem/hibcc-dI, ICCBBA for blood containers: http://hl7.org/fhir/NamingSystem/iccbba-blood-di, ICCBA for other devices: http://hl7.org/fhir/NamingSystem/iccbba-other-di.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Barcode System
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
35. Device.udiCarrier.jurisdiction
Definition | The identity of the authoritative source for UDI generation within a jurisdiction. All UDIs are globally unique within a single namespace with the appropriate repository uri as the system. For example, UDIs of devices managed in the U.S. by the FDA, the value is http://hl7.org/fhir/NamingSystem/fda-udi.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Requirements | Allows a recipient of a UDI to know which database will contain the UDI-associated metadata.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
36. Device.udiCarrier.carrierHRF
Definition | The full UDI carrier as the human readable form (HRF) representation of the barcode string as printed on the packaging of the device.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | Human Readable Form
Comments | If separate barcodes for DI and PI are present, concatenate the string with DI first and in order of human readable expression on label.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
37. Device.status
Definition | Status of the Device availability.
Control | 0..1
Binding | The codes SHALL be taken from FHIRDeviceStatus The availability status of the device.
Type | code
Is Modifier | true
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | true
Comments | This element is labeled as a modifier because the status contains the codes inactive and entered-in-error that mark the device (record)as not currently valid.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
38. Device.statusReason
Definition | Reason for the dtatus of the Device availability.
Control | 0..*
Binding | The codes SHALL be taken from FHIRDeviceStatusReason; other codes may be used where these codes are not suitable The availability status reason of the device.
Type | CodeableConcept
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
39. Device.manufacturer
Definition | A name of the manufacturer.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
40. Device.manufactureDate
Definition | The date and time when the device was manufactured.
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
41. Device.expirationDate
Definition | The date and time beyond which this device is no longer valid or should not be used (if applicable).
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
42. Device.lotNumber
Definition | Lot number assigned by the manufacturer.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
43. Device.serialNumber
Definition | The serial number assigned by the organization when the device was manufactured.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Comments | Alphanumeric Maximum 20.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
44. Device.deviceName
Definition | This represents the manufacturer's name of the device as provided by the device, from a UDI label, or by a person describing the Device. This typically would be used when a person provides the name(s) or when the device represents one of the names available from DeviceDefinition.
Control | 0..*
Type | BackboneElement
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
45. Device.deviceName.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
46. Device.deviceName.name
Definition | The name of the device.
Control | 1..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Σ
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
47. Device.deviceName.type
Definition | The type of deviceName. UDILabelName | UserFriendlyName | PatientReportedName | ManufactureDeviceName | ModelName.
Control | 1..1
Binding | The codes SHALL be taken from DeviceNameType The type of name the device is referred by.
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
48. Device.modelNumber
Definition | The model number for the device.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
49. Device.partNumber
Definition | The part number of the device.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Comments | Alphanumeric Maximum 20.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
50. Device.type
Definition | The kind or type of device.
Control | 10..1
Binding | The codes SHALL be taken from MDC Object infrastructure and Device nomenclature; other codes may be used where these codes are not suitableFor example codes, see DeviceType
Type | CodeableConcept
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
51. Device.type.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
52. Device.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
53. Device.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
54. Device.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
55. Device.version
Definition | The actual design of the device or software version running on the device.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..*
Type | BackboneElement
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
56. Device.version.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
57. Device.version.type
Definition | The type of the device version.
Control | 0..1
Type | CodeableConcept
Summary | false
Alternate Names | Σ
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
58. Device.version.type.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
59. Device.version.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
60. Device.version.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
61. Device.version.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
62. Device.version.component
Definition | A single component of the device version.
Control | 0..1
Type | Identifier
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
63. Device.version.value
Definition | The version text.
Control | 1..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
64. Device.property
Definition | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties.
Control | 0..*
Type | BackboneElement
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
65. Device.property.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
66. Device.property.type
Definition | Code that specifies the property DeviceDefinitionPropetyCode (Extensible).
Control | 1..1
Type | CodeableConcept
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
67. Device.property.type.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
68. Device.property.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
69. Device.property.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
70. Device.property.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
71. Device.property.valueCode
Definition | Property value as a code, e.g., NTP4 (synced to NTP).
Control | 0..*
Type | CodeableConcept
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
72. Device.property.valueCode.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
73. Device.property.valueCode.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
74. Device.property.valueCode.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
75. Device.property.valueCode.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
76. Device.patient
Definition | Patient information, If the device is affixed to a person.
Control | 0..1
Type | Reference(Patient)
Must Support | true
Summary | false
Requirements | If the device is implanted in a patient, then need to associate the device to the patient.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
77. Device.location
Definition | The place where the device can be found.
Control | 0..1
Type | Reference(Location)
Must Support | true
Summary | false
Requirements | Device.location can be used to track device location.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
78. Device.safety
Definition | Provides additional safety characteristics about a medical device. For example devices containing latex.
Control | 0..*
Binding | The codes SHALL be taken from Safety; other codes may be used where these codes are not suitableFor codes, see (unbound) Safety classificatio
Type | CodeableConcept
Must Support | true
Summary | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
79. Device.safety.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
80. Device.safety.coding.system
Definition | http://hl7.org/fhir/uv/pocd/ValueSet/safety The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
81. Device.safety.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
82. Device.parent
Definition | The parent device.
Control | 0..1
Type | Reference(MdsDevice|Device)
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))

Guidance on how to interpret the contents of this table can be found here.

1. Device
Definition | A type of a manufactured item that is used in the provision of healthcare without being substantially changed through that activity. The device may be a medical or non-medical device.
Control | 0..*
Summary | false
2. Device.id
Definition | The logical id of the resource, as used in the URL for the resource. Once assigned, this value never changes.
Control | 0..1
Type | id
Summary | true
Comments | The only time that a resource does not have an id is when it is being submitted to the server using a create operation.
3. Device.meta
Definition | The metadata about the resource. This is content that is maintained by the infrastructure. Changes to the content might not always be associated with version changes to the resource.
Control | 0..1
Type | Meta
Summary | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
4. Device.implicitRules
Definition | A reference to a set of rules that were followed when the resource was constructed, and which must be understood when processing the content. Often, this is a reference to an implementation guide that defines the special rules along with other profiles etc.
Control | 0..1
Type | uri
Is Modifier | true
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Asserting this rule set restricts the content to be only understood by a limited set of trading partners. This inherently limits the usefulness of the data in the long term. However, the existing health eco-system is highly fractured, and not yet ready to define, collect, and exchange data in a generally computable sense. Wherever possible, implementers and/or specification writers should avoid using this element. Often, when used, the URL is a reference to an implementation guide that defines these special rules as part of it's narrative along with other profiles, value sets, etc.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
5. Device.language
Definition | The base language in which the resource is written.
Control | 0..1
Binding | The codes SHOULD be taken from CommonLanguages A human language
Additional Bindings | Purpose
AllLanguages | Max Binding
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Comments | Language is provided to support indexing and accessibility (typically, services such as text to speech use the language tag). The html language tag in the narrative applies to the narrative. The language tag on the resource may be used to specify the language of other presentations generated from the data in the resource. Not all the content has to be in the base language. The Resource.language should not be assumed to apply to the narrative automatically. If a language is specified, it should it also be specified on the div element in the html (see rules in HTML5 for information about the relationship between xml:lang and the html lang attribute).
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
6. Device.text
Definition | A human-readable narrative that contains a summary of the resource and can be used to represent the content of the resource to a human. The narrative need not encode all the structured data, but is required to contain sufficient detail to make it "clinically safe" for a human to just read the narrative. Resource definitions may define what content should be represented in the narrative to ensure clinical safety.
Control | 0..1
Type | Narrative
Summary | false
Alternate Names | narrative, html, xhtml, display
Comments | Contained resources do not have narrative. Resources that are not contained SHOULD have a narrative. In some cases, a resource may only have text with little or no additional discrete data (as long as all minOccurs=1 elements are satisfied). This may be necessary for data from legacy systems where information is captured as a "text blob" or where text is additionally entered raw or narrated and encoded information is added later.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
7. Device.contained
Definition | These resources do not have an independent existence apart from the resource that contains them - they cannot be identified independently, and nor can they have their own independent transaction scope.
Control | 0..*
Type | Resource
Summary | false
Alternate Names | inline resources, anonymous resources, contained resources
Comments | This should never be done when the content can be identified properly, as once identification is lost, it is extremely difficult (and context dependent) to restore it again. Contained resources may have profiles and tags In their meta elements, but SHALL NOT have security labels.
8. Device.extension
Definition | An Extension
Control | 0..*
Type | Extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
9. Device.extension:approvedJurisdictions
SliceName | approvedJurisdictions
Definition | List of regions in which a device is approved to be operated.
Control | 0..* This element is affected by the following invariants: ele-1
Type | Extension(ApprovedJurisdictions) (Extension Type: CodeableConcept)
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
10. Device.extension:approvedJurisdictions.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
11. Device.extension:approvedJurisdictions.extension
Definition | An Extension
Control | 0..0
Type | Extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
12. Device.extension:approvedJurisdictions.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Control | 1..1
Type | uri
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Fixed Value | http://hl7.org/fhir/uv/pocd/StructureDefinition/approved-jurisdictions
13. Device.extension:approvedJurisdictions.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 1..1
Type | CodeableConcept
[x] Note | See Choice of Data Types for further information about how to use [x]
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.extension.value[x]. The slices are unordered and Closed, and can be differentiated using the following discriminators: type @ $this
14. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept
SliceName | valueCodeableConcept
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 1..1
Binding | The codes SHALL be taken from Jurisdiction ValueSet; other codes may be used where these codes are not suitable Codes for country, country subdivision and regio
Type | CodeableConcept
[x] Note | See Choice of Data Types for further information about how to use [x]
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
15. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
16. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.value[x].extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
17. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
18. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
19. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.value[x].coding.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
20. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
21. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
22. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
23. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
24. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Control | 0..1
Type | boolean
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
25. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Comments | Very often the text is the same as a displayName of one of the codings.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
26. Device.extension:operator
SliceName | operator
Definition | Identifies an operator of the device.
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Operator) (Extension Type: Reference(Practitioner))
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
27. Device.extension:operatingHours
SliceName | operatingHours
Definition | Optional amount of operating hours (e.g., an OR light).
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(OperatingHours) (Extension Type: unsignedInt)
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
28. Device.extension:operatingHours.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
29. Device.extension:operatingHours.extension
Definition | An Extension
Control | 0..0
Type | Extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
30. Device.extension:operatingHours.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Control | 1..1
Type | uri
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Fixed Value | http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours
31. Device.extension:operatingHours.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 1..1
Type | unsignedInt
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.extension.value[x]. The slices are unordered and Closed, and can be differentiated using the following discriminators: type @ $this
32. Device.extension:operatingHours.value[x]:valueUnsignedInt
SliceName | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 1..1
Type | unsignedInt
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
33. Device.extension:operatingCycles
SliceName | operatingCycles
Definition | Optional amount of operating cycles, e.g., the number of measurements taken within the component.
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(OperatingCycles) (Extension Type: unsignedInt)
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
34. Device.extension:operatingCycles.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
35. Device.extension:operatingCycles.extension
Definition | An Extension
Control | 0..0
Type | Extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
36. Device.extension:operatingCycles.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Control | 1..1
Type | uri
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Fixed Value | http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles
37. Device.extension:operatingCycles.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 1..1
Type | unsignedInt
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.extension.value[x]. The slices are unordered and Closed, and can be differentiated using the following discriminators: type @ $this
38. Device.extension:operatingCycles.value[x]:valueUnsignedInt
SliceName | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 1..1
Type | unsignedInt
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
39. Device.extension:operatingMode
SliceName | operatingMode
Definition | Operating mode that defines the interpretation constraints of the data that is provided.
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(OperatingMode) (Extension Type: code)
Must Support | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
40. Device.extension:operatingMode.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
41. Device.extension:operatingMode.extension
Definition | An Extension
Control | 0..0
Type | Extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.extension.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
42. Device.extension:operatingMode.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Control | 1..1
Type | uri
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Fixed Value | http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode
43. Device.extension:operatingMode.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 1..1
Binding | The codes SHALL be taken from Operating Mode; other codes may be used where these codes are not suitable Codes that indicate the device operating mod
Type | code
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.extension.value[x]. The slices are unordered and Closed, and can be differentiated using the following discriminators: type @ $this
44. Device.extension:operatingMode.value[x]:valueCode
SliceName | valueCode
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Control | 1..1
Binding | The codes SHALL be taken from Operating Mode; other codes may be used where these codes are not suitable Codes that indicate the device operating mod
Type | code
[x] Note | See Choice of Data Types for further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
45. Device.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the resource and that modifies the understanding of the element that contains it and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer is allowed to define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | false
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
46. Device.identifier
Definition | Unique instance identifiers assigned to a device by manufacturers other organizations or owners.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 0..* This element is affected by the following invariants: pocd-dev-1
Type | Identifier
Must Support | true
Summary | false
Comments | The barcode string from a barcode present on a device label or package may identify the instance, include names given to the device in local usage, or may identify the type of device. If the identifier identifies the type of device, Device.type element should be used.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on Device.identifier. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ system
47. Device.identifier:EUI-64
SliceName | EUI-64
Definition | Unique instance identifiers assigned to a device by manufacturers other organizations or owners.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 0..1
Type | Identifier
Summary | false
Comments | The barcode string from a barcode present on a device label or package may identify the instance, include names given to the device in local usage, or may identify the type of device. If the identifier identifies the type of device, Device.type element should be used.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
48. Device.identifier:EUI-64.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
49. Device.identifier:EUI-64.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.identifier.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
50. Device.identifier:EUI-64.use
Definition | The purpose of this identifier.
Control | 0..1
Binding | The codes SHALL be taken from IdentifierUse Identifies the purpose for this identifier, if known
Type | code
Is Modifier | true
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Allows the appropriate identifier for a particular context of use to be selected from among a set of identifiers.
Comments | Applications can assume that an identifier is permanent unless it explicitly says that it is temporary.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
51. Device.identifier:EUI-64.type
Definition | A coded type for the identifier that can be used to determine which identifier to use for a specific purpose.
Control | 0..1
Binding | The codes SHALL be taken from Identifier Type Codes; other codes may be used where these codes are not suitable A coded type for an identifier that can be used to determine which identifier to use for a specific purpose
Type | CodeableConcept
Summary | true
Requirements | Allows users to make use of identifiers when the identifier system is not known.
Comments | This element deals only with general categories of identifiers. It SHOULD not be used for codes that correspond 1..1 with the Identifier.system. Some identifiers may fall into multiple categories due to common usage. Where the system is known, a type is unnecessary because the type is always part of the system definition. However systems often need to handle identifiers where the system is not known. There is not a 1:1 relationship between type and system, since many different systems have the same type.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
52. Device.identifier:EUI-64.system
Definition | Establishes the namespace for the value - that is, a URL that describes a set values that are unique.
Control | 1..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | There are many sets of identifiers. To perform matching of two identifiers, we need to know what set we're dealing with. The system identifies a particular set of unique identifiers.
Comments | Identifier.system is always case sensitive.
Fixed Value | urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680
Example | General:http://www.acme.com/identifiers/patient
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
53. Device.identifier:EUI-64.value
Definition | The portion of the identifier typically relevant to the user and which is unique within the context of the system.
Control | 1..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | If the value is a full URI, then the system SHALL be urn:ietf:rfc:3986. The value's primary purpose is computational mapping. As a result, it may be normalized for comparison purposes (e.g. removing non-significant whitespace, dashes, etc.) A value formatted for human display can be conveyed using the Rendered Value extension. Identifier.value is to be treated as case sensitive unless knowledge of the Identifier.system allows the processer to be confident that non-case-sensitive processing is safe.
Example | General:123456
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
54. Device.identifier:EUI-64.period
Definition | Time period during which identifier is/was valid for use.
Control | 0..1
Type | Period
Summary | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
55. Device.identifier:EUI-64.assigner
Definition | Organization that issued/manages the identifier.
Control | 0..1
Type | Reference(Organization)
Summary | true
Comments | The Identifier.assigner may omit the .reference element and only contain a .display element reflecting the name or other textual information about the assigning organization.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
56. Device.definition
Definition | The reference to the definition for the device.
Control | 0..1
Type | Reference(DeviceDefinition)
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
57. Device.udiCarrier
Definition | Unique device identifier (UDI) assigned to device label or package. Note that the Device may include multiple udiCarriers as it either may include just the udiCarrier for the jurisdiction it is sold, or for multiple jurisdictions it could have been sold.
Control | 0..* This element is affected by the following invariants: pocd-dev-1
Type | BackboneElement
Must Support | true
Summary | true
Comments | UDI may identify an unique instance of a device, or it may only identify the type of the device. See UDI mappings for a complete mapping of UDI parts to Device.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
58. Device.udiCarrier.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
59. Device.udiCarrier.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
60. Device.udiCarrier.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
61. Device.udiCarrier.deviceIdentifier
Definition | The device identifier (DI) is a mandatory, fixed portion of a UDI that identifies the labeler and the specific version or model of a device.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | DI
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
62. Device.udiCarrier.issuer
Definition | Organization that is charged with issuing UDIs for devices. For example, the US FDA issuers include : GS1: http://hl7.org/fhir/NamingSystem/gs1-di, HIBCC: http://hl7.org/fhir/NamingSystem/hibcc-dI, ICCBBA for blood containers: http://hl7.org/fhir/NamingSystem/iccbba-blood-di, ICCBA for other devices: http://hl7.org/fhir/NamingSystem/iccbba-other-di.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Barcode System
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
63. Device.udiCarrier.jurisdiction
Definition | The identity of the authoritative source for UDI generation within a jurisdiction. All UDIs are globally unique within a single namespace with the appropriate repository uri as the system. For example, UDIs of devices managed in the U.S. by the FDA, the value is http://hl7.org/fhir/NamingSystem/fda-udi.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Requirements | Allows a recipient of a UDI to know which database will contain the UDI-associated metadata.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
64. Device.udiCarrier.carrierAIDC
Definition | The full UDI carrier of the Automatic Identification and Data Capture (AIDC) technology representation of the barcode string as printed on the packaging of the device - e.g., a barcode or RFID. Because of limitations on character sets in XML and the need to round-trip JSON data through XML, AIDC Formats SHALL be base64 encoded.
Control | 0..1
Type | base64Binary
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | Automatic Identification and Data Capture
Comments | The AIDC form of UDIs should be scanned or otherwise used for the identification of the device whenever possible to minimize errors in records resulting from manual transcriptions. If separate barcodes for DI and PI are present, concatenate the string with DI first and in order of human readable expression on label.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
65. Device.udiCarrier.carrierHRF
Definition | The full UDI carrier as the human readable form (HRF) representation of the barcode string as printed on the packaging of the device.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | Human Readable Form
Comments | If separate barcodes for DI and PI are present, concatenate the string with DI first and in order of human readable expression on label.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
66. Device.udiCarrier.entryType
Definition | A coded entry to indicate how the data was entered.
Control | 0..1
Binding | The codes SHALL be taken from UDIEntryType Codes to identify how UDI data was entered
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Requirements | Supports a way to distinguish hand entered from machine read data.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
67. Device.status
Definition | Status of the Device availability.
Control | 0..1
Binding | The codes SHALL be taken from FHIRDeviceStatus The availability status of the device
Type | code
Is Modifier | true
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | true
Comments | This element is labeled as a modifier because the status contains the codes inactive and entered-in-error that mark the device (record)as not currently valid.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
68. Device.statusReason
Definition | Reason for the dtatus of the Device availability.
Control | 0..*
Binding | The codes SHALL be taken from FHIRDeviceStatusReason; other codes may be used where these codes are not suitable The availability status reason of the device
Type | CodeableConcept
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
69. Device.distinctIdentifier
Definition | The distinct identification string as required by regulation for a human cell, tissue, or cellular and tissue-based product.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Distinct Identification Code (DIC)
Comments | For example, this applies to devices in the United States regulated under Code of Federal Regulation 21CFR§1271.290(c).
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
70. Device.manufacturer
Definition | A name of the manufacturer.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
71. Device.manufactureDate
Definition | The date and time when the device was manufactured.
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
72. Device.expirationDate
Definition | The date and time beyond which this device is no longer valid or should not be used (if applicable).
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
73. Device.lotNumber
Definition | Lot number assigned by the manufacturer.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
74. Device.serialNumber
Definition | The serial number assigned by the organization when the device was manufactured.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Comments | Alphanumeric Maximum 20.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
75. Device.deviceName
Definition | This represents the manufacturer's name of the device as provided by the device, from a UDI label, or by a person describing the Device. This typically would be used when a person provides the name(s) or when the device represents one of the names available from DeviceDefinition.
Control | 0..*
Type | BackboneElement
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
76. Device.deviceName.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
77. Device.deviceName.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
78. Device.deviceName.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
79. Device.deviceName.name
Definition | The name of the device.
Control | 1..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Σ
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
80. Device.deviceName.type
Definition | The type of deviceName. UDILabelName | UserFriendlyName | PatientReportedName | ManufactureDeviceName | ModelName.
Control | 1..1
Binding | The codes SHALL be taken from DeviceNameType The type of name the device is referred by
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
81. Device.modelNumber
Definition | The model number for the device.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
82. Device.partNumber
Definition | The part number of the device.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Comments | Alphanumeric Maximum 20.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
83. Device.type
Definition | The kind or type of device.
Control | 1..1
Binding | The codes SHALL be taken from MDC Object infrastructure and Device nomenclature; other codes may be used where these codes are not suitable
Type | CodeableConcept
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
84. Device.type.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
85. Device.type.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.type.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
86. Device.type.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
87. Device.type.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
88. Device.type.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.type.coding.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
89. Device.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
90. Device.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
91. Device.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
92. Device.type.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
93. Device.type.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Control | 0..1
Type | boolean
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
94. Device.type.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Comments | Very often the text is the same as a displayName of one of the codings.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
95. Device.specialization
Definition | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication.
Control | 0..*
Type | BackboneElement
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
96. Device.specialization.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
97. Device.specialization.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
98. Device.specialization.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
99. Device.specialization.systemType
Definition | The standard that is used to operate and communicate.
Control | 1..1
Type | CodeableConcept
Summary | false
Alternate Names | Σ
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
100. Device.specialization.version
Definition | The version of the standard that is used to operate and communicate.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
101. Device.version
Definition | The actual design of the device or software version running on the device.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..*
Type | BackboneElement
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
102. Device.version.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
103. Device.version.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
104. Device.version.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
105. Device.version.type
Definition | The type of the device version.
Control | 0..1
Type | CodeableConcept
Summary | false
Alternate Names | Σ
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
106. Device.version.type.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
107. Device.version.type.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.version.type.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
108. Device.version.type.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
109. Device.version.type.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
110. Device.version.type.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.version.type.coding.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
111. Device.version.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
112. Device.version.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
113. Device.version.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
114. Device.version.type.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
115. Device.version.type.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Control | 0..1
Type | boolean
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
116. Device.version.type.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Comments | Very often the text is the same as a displayName of one of the codings.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
117. Device.version.component
Definition | A single component of the device version.
Control | 0..1
Type | Identifier
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
118. Device.version.value
Definition | The version text.
Control | 1..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
119. Device.property
Definition | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties.
Control | 0..*
Type | BackboneElement
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
120. Device.property.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
121. Device.property.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
122. Device.property.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Control | 0..*
Type | Extension
Is Modifier | true
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
123. Device.property.type
Definition | Code that specifies the property DeviceDefinitionPropetyCode (Extensible).
Control | 1..1
Type | CodeableConcept
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
124. Device.property.type.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
125. Device.property.type.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.property.type.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
126. Device.property.type.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
127. Device.property.type.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
128. Device.property.type.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.property.type.coding.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
129. Device.property.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
130. Device.property.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
131. Device.property.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
132. Device.property.type.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
133. Device.property.type.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Control | 0..1
Type | boolean
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
134. Device.property.type.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Comments | Very often the text is the same as a displayName of one of the codings.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
135. Device.property.valueQuantity
Definition | Property value as a quantity.
Control | 0..*
Type | Quantity
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
136. Device.property.valueCode
Definition | Property value as a code, e.g., NTP4 (synced to NTP).
Control | 0..*
Type | CodeableConcept
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
137. Device.property.valueCode.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
138. Device.property.valueCode.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.property.valueCode.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
139. Device.property.valueCode.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
140. Device.property.valueCode.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
141. Device.property.valueCode.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.property.valueCode.coding.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
142. Device.property.valueCode.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
143. Device.property.valueCode.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
144. Device.property.valueCode.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
145. Device.property.valueCode.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
146. Device.property.valueCode.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Control | 0..1
Type | boolean
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
147. Device.property.valueCode.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Comments | Very often the text is the same as a displayName of one of the codings.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
148. Device.patient
Definition | Patient information, If the device is affixed to a person.
Control | 0..1
Type | Reference(Patient)
Must Support | true
Summary | false
Requirements | If the device is implanted in a patient, then need to associate the device to the patient.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
149. Device.owner
Definition | An organization that is responsible for the provision and ongoing maintenance of the device.
Control | 0..1
Type | Reference(Organization)
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
150. Device.contact
Definition | Contact details for an organization or a particular human that is responsible for the device.
Control | 0..*
Type | ContactPoint
Summary | false
Comments | used for troubleshooting etc.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
151. Device.location
Definition | The place where the device can be found.
Control | 0..1
Type | Reference(Location)
Must Support | true
Summary | false
Requirements | Device.location can be used to track device location.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
152. Device.url
Definition | A network address on which the device may be contacted directly.
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Comments | If the device is running a FHIR server, the network address should be the Base URL from which a conformance statement may be retrieved.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
153. Device.note
Definition | Descriptive information, usage information or implantation information that is not captured in an existing element.
Control | 0..*
Type | Annotation
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
154. Device.safety
Definition | Provides additional safety characteristics about a medical device. For example devices containing latex.
Control | 0..*
Binding | The codes SHALL be taken from Safety; other codes may be used where these codes are not suitable Safety classificatio
Type | CodeableConcept
Must Support | true
Summary | true
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
155. Device.safety.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
156. Device.safety.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.safety.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
157. Device.safety.coding
Definition | A reference to a code defined by a terminology system.
Control | 0..*
Type | Coding
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
158. Device.safety.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Control | 0..1
Type | string
XML Representation | In the XML format, this property is represented as an attribute.
Summary | false
159. Device.safety.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Control | 0..*
Type | Extension
Summary | false
Alternate Names | extensions, user content
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (: extension.exists() != value.exists())
Slicing | This element introduces a set of slices on Device.safety.coding.extension. The slices are unordered and Open, and can be differentiated using the following discriminators: value @ url
160. Device.safety.coding.system
Definition | http://hl7.org/fhir/uv/pocd/ValueSet/safety
Control | 0..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
161. Device.safety.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Note | This is a business versionId, not a resource version id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
162. Device.safety.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Control | 0..1
Type | code
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
163. Device.safety.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
164. Device.safety.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Control | 0..1
Type | boolean
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
165. Device.safety.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Comments | Very often the text is the same as a displayName of one of the codings.
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))
166. Device.parent
Definition | The parent device.
Control | 0..1
Type | Reference(MdsDevice)
Must Support | true
Summary | false
Invariants | Defined on this element ele-1: All FHIR elements must have a @value or children (: hasValue() or (children().count() > id.count()))