Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example DeviceMetric: NBP Numeric metric example

Generated Narrative: DeviceMetric

Resource DeviceMetric "NBPNumericDeviceMetric"

Profile: Numeric DeviceMetric profile

Metric availability extension: Intr

type: NBP (ISO 11073-10101 Health informatics - Point-of-care#150020 "MDC_PRESS_BLD_NONINV")

unit: mmHg (ISO 11073-10101 Health informatics - Point-of-care#266016 "MDC_DIM_MMHG")

source: Device/PhysioMonitorMdsDevice

parent: Device/NBPChannelDevice

operationalStatus: on

color: red

category: measurement

measurementPeriod: Once per 15 minutes