Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Operating mode code system - JSON Representation

Draft as of 2020-05-12

Raw json | Download

    {
      "resourceType" : "CodeSystem",
      "id" : "operating-mode",
      "meta" : {
        "profile" : [
          "http://hl7.org/fhir/StructureDefinition/shareablecodesystem"
        ]
      },
      "text" : {
        "status" : "generated",
        "div" : "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p>This code system <code>http://hl7.org/fhir/uv/pocd/CodeSystem/operating-mode</code> defines the following codes:</p><table class=\"codes\"><tr><td style=\"white-space:nowrap\"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style=\"white-space:nowrap\">Nml<a name=\"operating-mode-Nml\"> </a></td><td>Normal</td><td>The POC MEDICAL DEVICE operates in a mode that supports the fulfillment of its clinical functions.</td></tr><tr><td style=\"white-space:nowrap\">Dmo<a name=\"operating-mode-Dmo\"> </a></td><td>Demo</td><td>The POC MEDICAL DEVICE operates in a mode that is intended for demonstration purposes only. Arbitrary values are generated.</td></tr><tr><td style=\"white-space:nowrap\">Srv<a name=\"operating-mode-Srv\"> </a></td><td>Service</td><td>The POC MEDICAL DEVICE operates in a mode that is intended for services purposes only.</td></tr><tr><td style=\"white-space:nowrap\">Mtn<a name=\"operating-mode-Mtn\"> </a></td><td>Maintenance</td><td>Maintenance. The POC MEDICAL DEVICE operates in a mode that is intended for maintenance purposes only.</td></tr></table></div>"
      },
      "url" : "http://hl7.org/fhir/uv/pocd/CodeSystem/operating-mode",
      "version" : "current",
      "name" : "OperatingMode",
      "title" : "Operating mode",
      "status" : "draft",
      "experimental" : false,
      "date" : "2020-05-12",
      "publisher" : "HL7 International - Devices Work Group",
      "contact" : [
        {
          "telecom" : [
            {
              "system" : "url",
              "value" : "http://hl7.org/Special/committees/healthcaredevices"
            }
          ]
        }
      ],
      "description" : "CodeSystem for IEEE 11073-10207 MdsState/OperatingMode",
      "jurisdiction" : [
        {
          "coding" : [
            {
              "system" : "http://unstats.un.org/unsd/methods/m49/m49.htm",
              "code" : "001"
            }
          ]
        }
      ],
      "caseSensitive" : false,
      "content" : "complete",
      "concept" : [
        {
          "code" : "Nml",
          "display" : "Normal",
          "definition" : "The POC MEDICAL DEVICE operates in a mode that supports the fulfillment of its clinical functions."
        },
        {
          "code" : "Dmo",
          "display" : "Demo",
          "definition" : "The POC MEDICAL DEVICE operates in a mode that is intended for demonstration purposes only. Arbitrary values are generated."
        },
        {
          "code" : "Srv",
          "display" : "Service",
          "definition" : "The POC MEDICAL DEVICE operates in a mode that is intended for services purposes only."
        },
        {
          "code" : "Mtn",
          "display" : "Maintenance",
          "definition" : "Maintenance. The POC MEDICAL DEVICE operates in a mode that is intended for maintenance purposes only."
        }
      ]
    }