Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Resource Profile: VmdDevice - Mappings

Draft as of 2022-01-16

Mappings for the VmdDevice resource profile.

### Mappings for IEEE 11073-10201 DIM (urn:iso:std:iso:11073:10201)

VmdDevice
Device |
extension |
extension (instance) |
extension |
extension (number) |
value[x] (valueUnsignedInt) | VMD::Instance-Number
extension (approvedJurisdictions) |
extension (operatingHours) |
value[x] (valueUnsignedInt) | VMD::Operating-Hours
extension (operatingCycles) |
value[x] (valueUnsignedInt) | VMD::Operation-Cycles
udiCarrier |
deviceIdentifier | VMD::Production-Specification[spec-type=device-identifier]::prod-spec
issuer | VMD::Udi::udi-issuer
jurisdiction | VMD::Udi::udi-authority
carrierHRF | VMD::Udi::udi-label
statusReason | VMD::Vmd-Status
manufacturer | VMD::Vmd-Model::manufacturer
manufactureDate | VMD::Production-Specification[spec-type=manufacture-date]::prod-spec
expirationDate | VMD::Production-Specification[spec-type=expiry-date]::prod-spec
lotNumber | VMD::Production-Specification[spec-type=lot-number]::prod-spec
serialNumber | VMD::Production-Specification[spec-type=serial-number]::prod-spec
modelNumber | VMD::Vmd-Model::model-number
partNumber | VMD::Production-Specification[spec-type=part-number]::prod-spec
type |
coding |
code | VMO::Type
text | VMO::Label-String
version |
type | VMD::Production-Specification[spec-type=hw-revision|sw-revision|fw-revision]::spec-type
component | VMD::Production-Specification[spec-type=hw-revision|sw-revision|fw-revision]::component-id
value | VMD::Production-Specification[spec-type=hw-revision|sw-revision|fw-revision]::prod-spec

### Mappings for IEEE 11073-10207 SDC (urn:iso:std:iso:11073:10207)

VmdDevice
Device |
extension |
extension (instance) |
extension |
extension (number) |
value[x] (valueUnsignedInt) | VmdState/PhysicalConnector/Number
extension (label) |
value[x] (valueString) | VmdState/PhysicalConnector/Label
extension (approvedJurisdictions) |
value[x] |
value[x] (valueCodeableConcept) |
coding |
system | ApprovedJurisdictions/ApprovedJurisdiction/Root
code | ApprovedJurisdictions/ApprovedJurisdiction/Extension
extension (operatingHours) |
value[x] (valueUnsignedInt) | VmdState/OperatingHours
extension (operatingCycles) |
value[x] (valueUnsignedInt) | VmdState/OperatingCycles
identifier |
system | MdsDescriptor/Vmd/ProductionSpecification/ComponentId/Root
value | MdsDescriptor/Vmd/ProductionSpecification/ComponentId/Extension
statusReason | VmdState/ActivationState note the mapping of the value set
type |
coding |
system | MdsDescriptor/Vmd/Type/CodingSystem
version | MdsDescriptor/Vmd/Type/CodingSystemVersion
code | MdsDescriptor/Vmd/Type/Code
version |
type |
coding |
system | MdsDescriptor/Vmd/ProductionSpecification/SpecType/CodingSystem
version | MdsDescriptor/Vmd/ProductionSpecification/SpecType/CodingSystemVersion
code | MdsDescriptor/Vmd/ProductionSpecification/SpecType/Code
value | MdsDescriptor/Vmd/ProductionSpecification/ProductionSpec
safety |
coding |
code | MdsDescriptor/Vmd/SafetyClassification

### Mappings for RIM Mapping (http://hl7.org/v3)

VmdDevice
Device | Entity. Role, or Act, Device
text | Act.text?
contained | N/A
extension |
extension (instance) |
id | n/a
extension |
extension (number) |
id | n/a
extension | n/a
url | N/A
value[x] | N/A
value[x] (valueUnsignedInt) | N/A
extension (label) |
id | n/a
extension | n/a
url | N/A
value[x] | N/A
value[x] (valueString) | N/A
url | N/A
extension (approvedJurisdictions) |
id | n/a
url | N/A
value[x] | N/A
value[x] (valueCodeableConcept) | N/A
id | n/a
extension | n/a
coding | union(., ./translation)
id | n/a
extension | n/a
system | ./codeSystem
version | ./codeSystemVersion
code | ./code
display | CV.displayName
userSelected | CD.codingRationale
text | ./originalText[mediaType/code="text/plain"]/data
extension (operatingHours) |
id | n/a
url | N/A
value[x] | N/A
value[x] (valueUnsignedInt) | N/A
extension (operatingCycles) |
id | n/a
url | N/A
value[x] | N/A
value[x] (valueUnsignedInt) | N/A
modifierExtension | N/A
identifier | .id
id | n/a
extension | n/a
use | Role.code or implied by context
type | Role.code or implied by context
system | II.root or Role.id.root
value | II.extension or II.root if system indicates OID or GUID (Or Role.id.extension or root)
period | Role.effectiveTime or implied by context
assigner | II.assigningAuthorityName but note that this is an improper use by the definition of the field. Also Role.scoper
udiCarrier | .id and .code
id | n/a
extension | n/a
modifierExtension | N/A
deviceIdentifier | Role.id.extension
issuer | Role.id.root
jurisdiction | Role.scoper
carrierAIDC | Role.id.extension
carrierHRF | Role.id.extension
entryType | NA
status | .statusCode
distinctIdentifier | .lotNumberText
manufacturer | .playedRole[typeCode=MANU].scoper.name
manufactureDate | .existenceTime.low
expirationDate | .expirationTime
lotNumber | .lotNumberText
serialNumber | .playedRole[typeCode=MANU].id
deviceName |
id | n/a
extension | n/a
modifierExtension | N/A
type | .playedRole[typeCode=MANU].code
modelNumber | .softwareName (included as part)
partNumber | .playedRole[typeCode=MANU].id
type |
id | n/a
extension | n/a
coding | union(., ./translation)
id | n/a
extension | n/a
system | ./codeSystem
version | ./codeSystemVersion
code | ./code
display | CV.displayName
userSelected | CD.codingRationale
text | ./originalText[mediaType/code="text/plain"]/data
specialization |
id | n/a
extension | n/a
modifierExtension | N/A
version |
id | n/a
extension | n/a
modifierExtension | N/A
type |
id | n/a
extension | n/a
coding | union(., ./translation)
id | n/a
extension | n/a
system | ./codeSystem
version | ./codeSystemVersion
code | ./code
display | CV.displayName
userSelected | CD.codingRationale
text | ./originalText[mediaType/code="text/plain"]/data
property |
id | n/a
extension | n/a
modifierExtension | N/A
owner | .playedRole[typeCode=OWN].scoper
contact | .scopedRole[typeCode=CON].player
url | .telecom
note | .text
safety | NA
id | n/a
extension | n/a
coding | union(., ./translation)
id | n/a
extension | n/a
system | ./codeSystem
version | ./codeSystemVersion
code | ./code
display | CV.displayName
userSelected | CD.codingRationale
text | ./originalText[mediaType/code="text/plain"]/data

### Mappings for FiveWs Pattern Mapping (http://hl7.org/fhir/fivews)

VmdDevice
Device |
identifier | FiveWs.identifier
udiCarrier | FiveWs.identifier
deviceIdentifier | FiveWs.what[x]
status | FiveWs.status
statusReason | FiveWs.status
distinctIdentifier | FiveWs.what[x]
manufacturer | FiveWs.what[x]
manufactureDate | FiveWs.what[x]
expirationDate | FiveWs.what[x]
lotNumber | FiveWs.what[x]
serialNumber | FiveWs.what[x]
deviceName |
type | FiveWs.what[x]
modelNumber | FiveWs.what[x]
partNumber | FiveWs.what[x]
specialization |
version | FiveWs.what[x]
version |
component | FiveWs.what[x]
owner | FiveWs.source
contact | FiveWs.source
url | FiveWs.where[x]

### Mappings for UDI Mapping (http://fda.gov/UDI)

VmdDevice
Device |
identifier | The serial number which is a component of the production identifier (PI), a conditional, variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
udiCarrier |
deviceIdentifier | The device identifier (DI), a mandatory, fixed portion of a UDI that identifies the labeler and the specific version or model of a device.
issuer | All UDIs are to be issued under a system operated by an Jurisdiction-accredited issuing agency. GS1 DIs: http://hl7.org/fhir/NamingSystem/gs1 HIBCC DIs: http://hl7.org/fhir/NamingSystem/hibcc ICCBBA DIs for blood containers: http://hl7.org/fhir/NamingSystem/iccbba-blood ICCBA DIs for other devices: http://hl7.org/fhir/NamingSystem/iccbba-other
carrierAIDC | A unique device identifier (UDI) on a device label a form that uses automatic identification and data capture (AIDC) technology.
carrierHRF | A unique device identifier (UDI) on a device label in plain text
distinctIdentifier | The lot or batch number within which a device was manufactured - which is a component of the production identifier (PI), a conditional, variable portion of a UDI.
manufacturer | N/A
manufactureDate | The date a specific device was manufactured - which is a component of the production identifier (PI), a conditional, variable portion of a UDI. For FHIR, The datetime syntax must converted to YYYY-MM-DD[THH:MM:SS]. If hour is present, the minutes and seconds should both be set to “00”.
expirationDate | the expiration date of a specific device - which is a component of the production identifier (PI), a conditional, variable portion of a UDI. For FHIR, The datetime syntax must converted to YYYY-MM-DD[THH:MM:SS]. If hour is present, the minutes and seconds should both be set to “00”.
lotNumber | The lot or batch number within which a device was manufactured - which is a component of the production identifier (PI), a conditional, variable portion of a UDI.