Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example DeviceMetric: ECG Sample Array metric example

Generated Narrative: DeviceMetric

Resource DeviceMetric "ECGSampleArrayDeviceMetric"

Profile: Sample Array DeviceMetric profile

Resolution extension: 0.001

Sweep Speed extension: 25 mm/s (Details: UCUM code mm/s = 'mm/s')

type: ECG (ISO 11073-10101 Health informatics - Point-of-care#131328 "MDC_ECG_ELEC_POTL")

unit: mV (ISO 11073-10101 Health informatics - Point-of-care#266418 "MDC_DIM_MILLI_VOLT")

source: Device/PhysioMonitorMdsDevice

parent: Device/ECGChannelDevice

operationalStatus: on

color: green

category: measurement