Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## CodeSystem: Measurement status codes

Official URL: http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status | Version: current
Draft as of 2019-09-28 | Computable Name: MeasurementStatus

Measurement status definitions from the ISO/IEEE 11073-10201 DIM.

This Code system is referenced in the content logical definition of the following value sets:

- ObservationInterpretation

This code system `http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status` defines the following codes:

Code | Display | Definition
questionable | Questionable | Data may not be reliable
calibration-ongoing | Calibration ongoing | Calibration is ongoing
validated-data | Validated data | Relevant, e.g., in an archive
early-indication | Early indication | Early estimate of value
msmt-ongoing | Measurement ongoing | Indicates that a new measurement is just being taken
in-alarm | Measurement in alarm | Measurement has an active alarm condition
alarm-inhibited | Measurement alarms inhibited | Measurement supports alarming and alarms are turned off