Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example DeviceMetric: CVP Sample Array metric example

Generated Narrative: DeviceMetric

Resource DeviceMetric "CVPSampleArrayDeviceMetric"

Profile: Sample Array DeviceMetric profile

Sweep Speed extension: 25 mm/s (Details: UCUM code mm/s = 'mm/s')

> Visual Grid extension

> > url

> > `position`

> value: 0 mmHg (Details: UCUM code mm[Hg] = 'mm[Hg]')

> > url

> > `position`

> value: 10 mmHg (Details: UCUM code mm[Hg] = 'mm[Hg]')

> > url

> > `level`

> value: 0

> Visual Grid extension

> > url

> > `position`

> value: 5 mmHg (Details: UCUM code mm[Hg] = 'mm[Hg]')

> > url

> > `level`

> value: 1

type: CVP (ISO 11073-10101 Health informatics - Point-of-care#150084 "MDC_PRESS_BLD_VEN_CENT")

unit: mmHg (ISO 11073-10101 Health informatics - Point-of-care#266016 "MDC_DIM_MMHG")

source: Device/PhysioMonitorMdsDevice

parent: Device/BloodPressureChannelDevice

operationalStatus: on

color: cyan

category: measurement

### Calibrations

- | Type | State | Time
* | offset | calibrated | Jul 9, 2021, 8:20:30 AM