Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Measurement status codes - XML Representation

Draft as of 2019-09-28

Raw xml | Download

    <CodeSystem xmlns="http://hl7.org/fhir">
      <id value="measurement-status"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/StructureDefinition/shareablecodesystem"/>
      </meta>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p>This code system <code>http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status</code> defines the following codes:</p><table class="codes"><tr><td style="white-space:nowrap"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style="white-space:nowrap">questionable<a name="measurement-status-questionable"> </a></td><td>Questionable</td><td>Data may not be reliable</td></tr><tr><td style="white-space:nowrap">calibration-ongoing<a name="measurement-status-calibration-ongoing"> </a></td><td>Calibration ongoing</td><td>Calibration is ongoing</td></tr><tr><td style="white-space:nowrap">validated-data<a name="measurement-status-validated-data"> </a></td><td>Validated data</td><td>Relevant, e.g., in an archive</td></tr><tr><td style="white-space:nowrap">early-indication<a name="measurement-status-early-indication"> </a></td><td>Early indication</td><td>Early estimate of value</td></tr><tr><td style="white-space:nowrap">msmt-ongoing<a name="measurement-status-msmt-ongoing"> </a></td><td>Measurement ongoing</td><td>Indicates that a new measurement is just being taken</td></tr><tr><td style="white-space:nowrap">in-alarm<a name="measurement-status-in-alarm"> </a></td><td>Measurement in alarm</td><td>Measurement has an active alarm condition</td></tr><tr><td style="white-space:nowrap">alarm-inhibited<a name="measurement-status-alarm-inhibited"> </a></td><td>Measurement alarms inhibited</td><td>Measurement supports alarming and alarms are turned off</td></tr></table></div>
      </text>
      <url value="http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status"/>
      <version value="current"/>
      <name value="MeasurementStatus"/>
      <title value="Measurement status codes"/>
      <status value="draft"/>
      <experimental value="false"/>
      <date value="2019-09-28"/>
      <publisher value="HL7 International - Devices Work Group"/>
      <contact>
        <telecom>
          <system value="url"/>
          <value value="http://hl7.org/Special/committees/healthcaredevices"/>
        </telecom>
      </contact>
      <description
                   value="Measurement status definitions from the ISO/IEEE 11073-10201 DIM."/>
      <jurisdiction>
        <coding>
          <system value="http://unstats.un.org/unsd/methods/m49/m49.htm"/>
          <code value="001"/>
        </coding>
      </jurisdiction>
      <caseSensitive value="false"/>
      <content value="complete"/>
      <concept>
        <code value="questionable"/>
        <display value="Questionable"/>
        <definition value="Data may not be reliable"/>
      </concept>
      <concept>
        <code value="calibration-ongoing"/>
        <display value="Calibration ongoing"/>
        <definition value="Calibration is ongoing"/>
      </concept>
      <concept>
        <code value="validated-data"/>
        <display value="Validated data"/>
        <definition value="Relevant, e.g., in an archive"/>
      </concept>
      <concept>
        <code value="early-indication"/>
        <display value="Early indication"/>
        <definition value="Early estimate of value"/>
      </concept>
      <concept>
        <code value="msmt-ongoing"/>
        <display value="Measurement ongoing"/>
        <definition value="Indicates that a new measurement is just being taken"/>
      </concept>
      <concept>
        <code value="in-alarm"/>
        <display value="Measurement in alarm"/>
        <definition value="Measurement has an active alarm condition"/>
      </concept>
      <concept>
        <code value="alarm-inhibited"/>
        <display value="Measurement alarms inhibited"/>
        <definition
                    value="Measurement supports alarming and alarms are turned off"/>
      </concept>
    </CodeSystem>