Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : ECG Channel example - TTL Representation

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:Device ;
      fhir:nodeRole fhir:treeRoot ;
      fhir:id [ fhir:v "ECGChannelDevice"] ; #
      fhir:meta [
        ( fhir:profile [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/ChannelDevice"^^xsd:anyURI ;
    fhir:link <http://hl7.org/fhir/uv/pocd/StructureDefinition/ChannelDevice>     ] )
      ] ; #
      fhir:text [
    fhir:status [ fhir:v "generated" ] ;
    fhir:div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p><b>Generated Narrative: Device</b><a name=\"ECGChannelDevice\"> </a></p><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\">Resource Device &quot;ECGChannelDevice&quot; </p><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-ChannelDevice.html\">Channel Device profile</a></p></div><p><b>status</b>: active</p><p><b>type</b>: MDC_DEV_ECG_CHAN <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#69799)</span></p><p><b>parent</b>: <a href=\"Device-ECGVmdDevice.html\">Device/ECGVmdDevice</a></p></div>"
      ] ; #
      fhir:status [ fhir:v "active"] ; #
      fhir:type [
        ( fhir:coding [
    fhir:system [ fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "69799" ] ;
    fhir:display [ fhir:v "MDC_DEV_ECG_CHAN" ]     ] )
      ] ; #
      fhir:parent [
    fhir:reference [ fhir:v "Device/ECGVmdDevice" ]
      ] . #