Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : NBP Numeric observation example - TTL Representation

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix loinc: <https://loinc.org/rdf/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:Observation ;
      fhir:nodeRole fhir:treeRoot ;
      fhir:id [ fhir:v "NBPCompoundNumericObservation"] ; #
      fhir:meta [
        ( fhir:profile [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/CompoundNumericObservation"^^xsd:anyURI ;
    fhir:link <http://hl7.org/fhir/uv/pocd/StructureDefinition/CompoundNumericObservation>     ] )
      ] ; #
      fhir:text [
    fhir:status [ fhir:v "generated" ] ;
    fhir:div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p><b>Generated Narrative: Observation</b><a name=\"NBPCompoundNumericObservation\"> </a></p><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\">Resource Observation &quot;NBPCompoundNumericObservation&quot; </p><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-CompoundNumericObservation.html\">Compound Numeric Observation profile</a></p></div><p><b>status</b>: final</p><p><b>category</b>: Vital Signs <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-observation-category.html\">Observation Category Codes</a>#vital-signs)</span></p><p><b>code</b>: Blood pressure panel with all children optional <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"https://loinc.org/\">LOINC</a>#85354-9; <a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#150020 &quot;MDC_PRESS_BLD_NONINV&quot;)</span></p><p><b>subject</b>: <a href=\"Patient-SomePatient.html\">Patient/SomePatient</a> &quot; DOE&quot;</p><p><b>effective</b>: 2021-07-09 11:30:12+0200</p><p><b>device</b>: <a href=\"DeviceMetric-NBPNumericDeviceMetric.html\">DeviceMetric/NBPNumericDeviceMetric</a></p><blockquote><p><b>component</b></p><p><b>code</b>: Systolic blood pressure <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"https://loinc.org/\">LOINC</a>#8480-6; <a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#150021 &quot;MDC_PRESS_BLD_NONINV_SYS&quot;)</span></p><p><b>value</b>: 120 mmHg<span style=\"background: LightGoldenRodYellow\"> (Details: UCUM code mm[Hg] = 'mm[Hg]')</span></p></blockquote><blockquote><p><b>component</b></p><p><b>code</b>: Diastolic blood pressure <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"https://loinc.org/\">LOINC</a>#8462-4; <a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#150022 &quot;MDC_PRESS_BLD_NONINV_DIA&quot;)</span></p><p><b>value</b>: 80 mmHg<span style=\"background: LightGoldenRodYellow\"> (Details: UCUM code mm[Hg] = 'mm[Hg]')</span></p></blockquote><blockquote><p><b>component</b></p><p><b>code</b>: Mean blood pressure <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"https://loinc.org/\">LOINC</a>#8478-0; <a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#150023 &quot;MDC_PRESS_BLD_NONINV_MEAN&quot;)</span></p><p><b>value</b>: 90 mmHg<span style=\"background: LightGoldenRodYellow\"> (Details: UCUM code mm[Hg] = 'mm[Hg]')</span></p></blockquote></div>"
      ] ; #
      fhir:status [ fhir:v "final"] ; #
      fhir:category ( [
        ( fhir:coding [
    fhir:system [ fhir:v "http://terminology.hl7.org/CodeSystem/observation-category"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "vital-signs" ] ;
    fhir:display [ fhir:v "Vital Signs" ]     ] )
      ] ) ; #
      fhir:code [
        ( fhir:coding [
    a loinc:85354-9 ;
    fhir:system [ fhir:v "http://loinc.org"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "85354-9" ] ;
    fhir:display [ fhir:v "Blood pressure panel with all children optional" ]     ] [
    fhir:system [ fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "150020" ] ;
    fhir:display [ fhir:v "MDC_PRESS_BLD_NONINV" ]     ] )
      ] ; #
      fhir:subject [
    fhir:reference [ fhir:v "Patient/SomePatient" ]
      ] ; #
      fhir:effective [ fhir:v "2021-07-09T11:30:12+02:00"^^xsd:dateTime] ; #
      fhir:device [
    fhir:reference [ fhir:v "DeviceMetric/NBPNumericDeviceMetric" ]
      ] ; #
      fhir:component ( [
    fhir:code [
          ( fhir:coding [
    a loinc:8480-6 ;
    fhir:system [ fhir:v "http://loinc.org"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "8480-6" ] ;
    fhir:display [ fhir:v "Systolic blood pressure" ]       ] [
    fhir:system [ fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "150021" ] ;
    fhir:display [ fhir:v "MDC_PRESS_BLD_NONINV_SYS" ]       ] )     ] ;
    fhir:value [
    a fhir:Quantity ;
    fhir:value [ fhir:v "120"^^xsd:decimal ] ;
    fhir:unit [ fhir:v "mmHg" ] ;
    fhir:system [ fhir:v "http://unitsofmeasure.org"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "mm[Hg]" ]     ]
      ] [
    fhir:code [
          ( fhir:coding [
    a loinc:8462-4 ;
    fhir:system [ fhir:v "http://loinc.org"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "8462-4" ] ;
    fhir:display [ fhir:v "Diastolic blood pressure" ]       ] [
    fhir:system [ fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "150022" ] ;
    fhir:display [ fhir:v "MDC_PRESS_BLD_NONINV_DIA" ]       ] )     ] ;
    fhir:value [
    a fhir:Quantity ;
    fhir:value [ fhir:v "80"^^xsd:decimal ] ;
    fhir:unit [ fhir:v "mmHg" ] ;
    fhir:system [ fhir:v "http://unitsofmeasure.org"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "mm[Hg]" ]     ]
      ] [
    fhir:code [
          ( fhir:coding [
    a loinc:8478-0 ;
    fhir:system [ fhir:v "http://loinc.org"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "8478-0" ] ;
    fhir:display [ fhir:v "Mean blood pressure" ]       ] [
    fhir:system [ fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "150023" ] ;
    fhir:display [ fhir:v "MDC_PRESS_BLD_NONINV_MEAN" ]       ] )     ] ;
    fhir:value [
    a fhir:Quantity ;
    fhir:value [ fhir:v "90"^^xsd:decimal ] ;
    fhir:unit [ fhir:v "mmHg" ] ;
    fhir:system [ fhir:v "http://unitsofmeasure.org"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "mm[Hg]" ]     ]
      ] ) . #