Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : CVP Sample Array metric example - XML Representation

Raw xml | Download

    <DeviceMetric xmlns="http://hl7.org/fhir">
      <id value="CVPSampleArrayDeviceMetric"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayDeviceMetric"/>
      </meta>
      <text>
        <status value="extensions"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p><b>Generated Narrative: DeviceMetric</b><a name="CVPSampleArrayDeviceMetric"> </a></p><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px">Resource DeviceMetric &quot;CVPSampleArrayDeviceMetric&quot; </p><p style="margin-bottom: 0px">Profile: <a href="StructureDefinition-SampleArrayDeviceMetric.html">Sample Array DeviceMetric profile</a></p></div><p><b>Sweep Speed extension</b>: 25 mm/s<span style="background: LightGoldenRodYellow"> (Details: UCUM code mm/s = 'mm/s')</span></p><blockquote><p><b>Visual Grid extension</b></p><blockquote><p><b>url</b></p><code>position</code></blockquote><p><b>value</b>: 0 mmHg<span style="background: LightGoldenRodYellow"> (Details: UCUM code mm[Hg] = 'mm[Hg]')</span></p><blockquote><p><b>url</b></p><code>position</code></blockquote><p><b>value</b>: 10 mmHg<span style="background: LightGoldenRodYellow"> (Details: UCUM code mm[Hg] = 'mm[Hg]')</span></p><blockquote><p><b>url</b></p><code>level</code></blockquote><p><b>value</b>: 0</p></blockquote><blockquote><p><b>Visual Grid extension</b></p><blockquote><p><b>url</b></p><code>position</code></blockquote><p><b>value</b>: 5 mmHg<span style="background: LightGoldenRodYellow"> (Details: UCUM code mm[Hg] = 'mm[Hg]')</span></p><blockquote><p><b>url</b></p><code>level</code></blockquote><p><b>value</b>: 1</p></blockquote><p><b>type</b>: CVP <span style="background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki"> (<a href="http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html">ISO 11073-10101 Health informatics - Point-of-care</a>#150084 &quot;MDC_PRESS_BLD_VEN_CENT&quot;)</span></p><p><b>unit</b>: mmHg <span style="background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki"> (<a href="http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html">ISO 11073-10101 Health informatics - Point-of-care</a>#266016 &quot;MDC_DIM_MMHG&quot;)</span></p><p><b>source</b>: <a href="Device-PhysioMonitorMdsDevice.html">Device/PhysioMonitorMdsDevice</a></p><p><b>parent</b>: <a href="Device-BloodPressureChannelDevice.html">Device/BloodPressureChannelDevice</a></p><p><b>operationalStatus</b>: on</p><p><b>color</b>: cyan</p><p><b>category</b>: measurement</p><h3>Calibrations</h3><table class="grid"><tr><td style="display: none">-</td><td><b>Type</b></td><td><b>State</b></td><td><b>Time</b></td></tr><tr><td style="display: none">*</td><td>offset</td><td>calibrated</td><td>Jul 9, 2021, 8:20:30 AM</td></tr></table></div>
      </text>
      <extension
                 url="http://hl7.org/fhir/uv/pocd/StructureDefinition/sweep-speed">
        <valueQuantity>
          <value value="25"/>
          <unit value="mm/s"/>
          <system value="http://unitsofmeasure.org"/>
          <code value="mm/s"/>
        </valueQuantity>
      </extension>
      <extension
                 url="http://hl7.org/fhir/uv/pocd/StructureDefinition/visual-grid">
        <extension url="position">
          <valueQuantity>
            <value value="0"/>
            <unit value="mmHg"/>
            <system value="http://unitsofmeasure.org"/>
            <code value="mm[Hg]"/>
          </valueQuantity>
        </extension>
        <extension url="position">
          <valueQuantity>
            <value value="10"/>
            <unit value="mmHg"/>
            <system value="http://unitsofmeasure.org"/>
            <code value="mm[Hg]"/>
          </valueQuantity>
        </extension>
        <extension url="level">
          <valueUnsignedInt value="0"/>
        </extension>
      </extension>
      <extension
                 url="http://hl7.org/fhir/uv/pocd/StructureDefinition/visual-grid">
        <extension url="position">
          <valueQuantity>
            <value value="5"/>
            <unit value="mmHg"/>
            <system value="http://unitsofmeasure.org"/>
            <code value="mm[Hg]"/>
          </valueQuantity>
        </extension>
        <extension url="level">
          <valueUnsignedInt value="1"/>
        </extension>
      </extension>
      <type>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="150084"/>
          <display value="MDC_PRESS_BLD_VEN_CENT"/>
        </coding>
        <text value="CVP"/>
      </type>
      <unit>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="266016"/>
          <display value="MDC_DIM_MMHG"/>
        </coding>
        <text value="mmHg"/>
      </unit>
      <source>
        <reference value="Device/PhysioMonitorMdsDevice"/>
      </source>
      <parent>
        <reference value="Device/BloodPressureChannelDevice"/>
      </parent>
      <operationalStatus value="on"/>
      <color value="cyan"/>
      <category value="measurement"/>
      <calibration>
        <type value="offset"/>
        <state value="calibrated"/>
        <time value="2021-07-09T10:20:30+02:00"/>
      </calibration>
    </DeviceMetric>