Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example DeviceMetric: Heart Rate Numeric metric example

Generated Narrative: DeviceMetric

Resource DeviceMetric "HeartRateNumericDeviceMetric"

Profile: Numeric DeviceMetric profile

> Relation extension

> > url

> > `kind`

> value: DCE

> > url

> > `entries`

> value: DeviceMetric/ECGSampleArrayDeviceMetric

> Technical range extension

> > url

> > `lowerLimit`

> value: 0

> > url

> > `upperLimit`

> value: 200

> > url

> > `stepWidth`

> value: 1

> > url

> > `relativeAccuracy`

> value: 0.01

> > url

> > `absoluteAccuracy`

> value: 0.01

type: HR (ISO 11073-10101 Health informatics - Point-of-care#147842 "MDC_ECG_HEART_RATE")

unit: bpm (ISO 11073-10101 Health informatics - Point-of-care#264864 "MDC_DIM_BEAT_PER_MIN")

source: Device/PhysioMonitorMdsDevice

parent: Device/HeartRateChannelDevice

operationalStatus: on

color: green

category: measurement