Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Change Log

### Version 0.3.0

- Add "Getting Started" section.
- Add "Technical Implementation Guidance" section with mappings from HL7 V2 and ISO/IEEE 11073.
- Update all artifacts to FHIR Release #4 (version 4.0.1).
- Add Sample Array DeviceMetric and Observation profiles and extensions for waveforms.
- Add Device and DeviceMetric extensions and value sets for SDC mappings.
- Add mustSupport flags to profile definitions.
- Add Server CapabilityStatement.
- Update and add examples.

### Version 0.2.0

- Move content from Simplifier to GitHub for use by the IG Publisher, including restructuring and formatting changes.
- Replace PoC Device and DeviceComponent profiles with MDS, VMD, and Channel Device profiles reflecting the Device-DeviceComponent resource merge.
- Change Device.type, DeviceMetric.type, DeviceMetric.unit, Observation.code, and Observation.component.code to an extensible binding to the 11073 MDC terminology.
- Replace measurement status extension by an extended value set for Observation.interpretation and Observation.component.interpretation.
- Create ValueSets for the 11073 MDC nomenclature filtered by partition.
- Create CodeSystem and extend ValueSet for Observation interpretation codes including measurement status.
- Update examples for new profile definitions.

### Version 0.1.0

- First draft for comment.