Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example Observation: NBP Numeric observation example

Generated Narrative: Observation

Resource Observation "NBPCompoundNumericObservation"

Profile: Compound Numeric Observation profile

status: final

category: Vital Signs (Observation Category Codes#vital-signs)

code: Blood pressure panel with all children optional (LOINC#85354-9; ISO 11073-10101 Health informatics - Point-of-care#150020 "MDC_PRESS_BLD_NONINV")

subject: Patient/SomePatient " DOE"

effective: 2021-07-09 11:30:12+0200

device: DeviceMetric/NBPNumericDeviceMetric

> component

> code: Systolic blood pressure (LOINC#8480-6; ISO 11073-10101 Health informatics - Point-of-care#150021 "MDC_PRESS_BLD_NONINV_SYS")

> value: 120 mmHg (Details: UCUM code mm[Hg] = 'mm[Hg]')

> component

> code: Diastolic blood pressure (LOINC#8462-4; ISO 11073-10101 Health informatics - Point-of-care#150022 "MDC_PRESS_BLD_NONINV_DIA")

> value: 80 mmHg (Details: UCUM code mm[Hg] = 'mm[Hg]')

> component

> code: Mean blood pressure (LOINC#8478-0; ISO 11073-10101 Health informatics - Point-of-care#150023 "MDC_PRESS_BLD_NONINV_MEAN")

> value: 90 mmHg (Details: UCUM code mm[Hg] = 'mm[Hg]')