## Profile Comparison between http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode vs http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode

Left: | Operating mode extension (http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode)
Right: | Operating mode extension (http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode)

### Messages

Error | StructureDefinition.version | Values for version differ: '0.3.0' vs 'current'
Information | StructureDefinition.date | Values for date differ: '2021-07-07' vs '2022-01-16'
Warning | Extension | Elements differ in short: 'Extension' vs 'Operating mode'
Warning | Extension | Elements differ in definition: 'An Extension' vs 'Operating mode that defines the interpretation constraints of the data that is provided.'
Information | Extension | Element maximum cardinalities differ: '1' vs '2147483647'
Warning | Extension.value[x] | Elements differ in short: 'Operating mode' vs 'Value of extension'
Warning | Extension.value[x] | Elements differ in description: 'Operating Mode of the MDS' vs 'Codes that indicate the device operating mode'
Warning | Extension.value[x] | Elements differ in description: 'Operating Mode of the MDS' vs 'Codes that indicate the device operating mode'

### Metadata

Name | Value | Comments
--- | --- | ---
abstract | false |
baseDefinition | http://hl7.org/fhir/StructureDefinition/Extension |
copyright |  |
date | 2021-07-07 | 2022-01-16 | Values Differ
description | Operating mode that defines if the operation is accessible. | StructureDefinition that adds an operating mode to a Device. | Values Differ
experimental |  |
fhirVersion | 4.0.1 |
jurisdiction |  |
jurisdiction[0] | http://unstats.un.org/unsd/methods/m49/m49.htm#001 |
kind | complex-type |
name | OperatingMode |
publisher | HL7 International - Devices Work Group |
purpose |  |
status | draft |
title | Operating mode extension |
type | Extension |
url | http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode |
version | 0.3.0 | current | Values Differ

### Structure

Name | L Flags | L Card. | L Type | L Description & Constraints | R Flags | R Card. | L Type | L Description & Constraints | Comments
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Extension |  | 0..1 | Extension | Extension |  | 0..* | Extension | Operating mode | Elements differ in short: 'Extension' vs 'Operating mode' Elements differ in definition: 'An Extension' vs 'Operating mode that defines the interpretation constraints of the data that is provided.' Element maximum cardinalities differ: '1' vs '2147483647'
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
Slices for extension |  | 0..0 |  |  |  | 0..0 |  |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode" |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-mode" |
value[x] |  | 1..1 | code | Operating mode Binding: ?? (extensible): Operating Mode of the MDS |  | 1..1 | code | Value of extension Binding: ?? (extensible): Codes that indicate the device operating mode | Elements differ in short: 'Operating mode' vs 'Value of extension' Elements differ in description: 'Operating Mode of the MDS' vs 'Codes that indicate the device operating mode' Elements differ in description: 'Operating Mode of the MDS' vs 'Codes that indicate the device operating mode'
Documentation for this format