Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : CVP Sample Array observation example - TTL Representation

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:Observation ;
      fhir:nodeRole fhir:treeRoot ;
      fhir:id [ fhir:v "CVPSampleArrayObservation"] ; #
      fhir:meta [
        ( fhir:profile [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayObservation"^^xsd:anyURI ;
    fhir:link <http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayObservation>     ] )
      ] ; #
      fhir:text [
    fhir:status [ fhir:v "generated" ] ;
    fhir:div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p><b>Generated Narrative: Observation</b><a name=\"CVPSampleArrayObservation\"> </a></p><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\">Resource Observation &quot;CVPSampleArrayObservation&quot; </p><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-SampleArrayObservation.html\">Sample Array Observation profile</a></p></div><p><b>status</b>: final</p><p><b>code</b>: MDC_PRESS_BLD_VEN_CENT <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#150084)</span></p><p><b>subject</b>: <a href=\"Patient-SomePatient.html\">Patient/SomePatient</a> &quot; DOE&quot;</p><p><b>effective</b>: 2021-07-09 11:33:23+0200 --&gt; 2021-07-09 11:33:24+0200</p><p><b>value</b>: Origin: 0 mmHg, Interval: 8, Dimensions: 1, Data: 2.00 2.00 2.00 2.01 2.02 2.03 2.06 2.09 2.13 2.19 2.25 2.33 2.42 2.53 2.65 2.78 2.93 3.09 3.27 3.47 3.68 3.90 4.14 4.40 4.67 4.96 5.34 5.82 6.37 6.90 7.35 7.68 7.89 7.98 8.00 7.94 7.82 7.64 7.41 7.14 6.84 6.48 6.11 5.85 5.73 5.79 5.95 6.22 6.45 6.54 6.56 6.44 6.20 5.88 5.48 5.01 4.71 4.44 4.18 3.95 3.73 3.53 3.36 3.20 3.06 2.94 2.85 2.77 2.70 2.67 2.64 2.64 2.65 2.70 2.75 2.82 2.91 3.02 3.15 3.29 3.46 3.64 3.84 4.06 4.27 4.48 4.68 4.88 5.06 5.23 5.38 5.52 5.63 5.71 5.76 5.75 5.72 5.62 5.47 5.26 5.01 4.74 4.45 4.16 3.90 3.66 3.45 3.25 3.08 2.92 2.78 2.66 2.55 2.46 2.37 2.31 2.24 2.19 2.15 2.11 2.08 2.05 2.03 2.02 2.01</p><p><b>device</b>: <a href=\"DeviceMetric-CVPSampleArrayDeviceMetric.html\">DeviceMetric/CVPSampleArrayDeviceMetric</a></p></div>"
      ] ; #
      fhir:status [ fhir:v "final"] ; #
      fhir:code [
        ( fhir:coding [
    fhir:system [ fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "150084" ] ;
    fhir:display [ fhir:v "MDC_PRESS_BLD_VEN_CENT" ]     ] )
      ] ; #
      fhir:subject [
    fhir:reference [ fhir:v "Patient/SomePatient" ]
      ] ; #
      fhir:effective [
    a fhir:Period ;
    fhir:start [ fhir:v "2021-07-09T11:33:23+02:00"^^xsd:dateTime ] ;
    fhir:end [ fhir:v "2021-07-09T11:33:24+02:00"^^xsd:dateTime ]
      ] ; #
      fhir:value [
    a fhir:SampledData ;
    fhir:origin [
    fhir:value [ fhir:v "0"^^xsd:decimal ] ;
    fhir:unit [ fhir:v "mmHg" ] ;
    fhir:system [ fhir:v "http://unitsofmeasure.org"^^xsd:anyURI ] ;
    fhir:code [ fhir:v "mm[Hg]" ]     ] ;
    fhir:period [ fhir:v "8"^^xsd:decimal ] ;
    fhir:dimensions [ fhir:v "1"^^xsd:positiveInteger ] ;
    fhir:data [ fhir:v "2.00 2.00 2.00 2.01 2.02 2.03 2.06 2.09 2.13 2.19 2.25 2.33 2.42 2.53 2.65 2.78 2.93 3.09 3.27 3.47 3.68 3.90 4.14 4.40 4.67 4.96 5.34 5.82 6.37 6.90 7.35 7.68 7.89 7.98 8.00 7.94 7.82 7.64 7.41 7.14 6.84 6.48 6.11 5.85 5.73 5.79 5.95 6.22 6.45 6.54 6.56 6.44 6.20 5.88 5.48 5.01 4.71 4.44 4.18 3.95 3.73 3.53 3.36 3.20 3.06 2.94 2.85 2.77 2.70 2.67 2.64 2.64 2.65 2.70 2.75 2.82 2.91 3.02 3.15 3.29 3.46 3.64 3.84 4.06 4.27 4.48 4.68 4.88 5.06 5.23 5.38 5.52 5.63 5.71 5.76 5.75 5.72 5.62 5.47 5.26 5.01 4.74 4.45 4.16 3.90 3.66 3.45 3.25 3.08 2.92 2.78 2.66 2.55 2.46 2.37 2.31 2.24 2.19 2.15 2.11 2.08 2.05 2.03 2.02 2.01" ]
      ] ; #
      fhir:device [
    fhir:reference [ fhir:v "DeviceMetric/CVPSampleArrayDeviceMetric" ]
      ] . #