Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## CapabilityStatement: Server CapabilityStatement

Official URL: http://hl7.org/fhir/uv/pocd/CapabilityStatement/ServerCapabilityStatement | Version: current
Draft as of 2021-07-17 | Computable Name: ServerCapabilityStatement

CapabilityStatement that describes the expected capabilities of a server processing data from Point-of-Care devices.

Raw OpenAPI-Swagger Definition file | Download

## ServerCapabilityStatement

CapabilityStatement that describes the expected capabilities of a server processing data from Point-of-Care devices.

Mode | SERVER
Description | A FHIR server conforming to the Point-of-Care Device Implementation Guide shall: Implement the "RESTful FHIR" exchange framework according to the FHIR specification. Accept both XML and JSON resource format for interactions. Support all profiles, extensions, and terminologies as defined in this implementation guide. Support transactions.
Transaction | y
System History |
System Search |

Resource Type | Profile | Read | V-Read | Search | Update | Create | Delete
--- | --- | --- | --- | --- | --- | --- | ---
Device | Supported profiles: MDS Device profile VMD Device profile Channel Device profile | y | y | y | y | y | y
DeviceMetric | Supported profiles: Numeric DeviceMetric profile Enumeration DeviceMetric profile Sample Array DeviceMetric profile | y | y | y | y | y | y
Observation | Supported profiles: Numeric Observation profile Compound Numeric Observation profile Enumeration Observation profile Sample Array Observation profile | y | y | y | y | y | y
Patient |  | y |  | y |  | y |
Practitioner |  | y |  | y |  | y |
Location |  | y |  | y |  | y |