Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : ECG Sample Array metric example - XML Representation

Raw xml | Download

    <DeviceMetric xmlns="http://hl7.org/fhir">
      <id value="ECGSampleArrayDeviceMetric"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayDeviceMetric"/>
      </meta>
      <text>
        <status value="extensions"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p><b>Generated Narrative: DeviceMetric</b><a name="ECGSampleArrayDeviceMetric"> </a></p><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px">Resource DeviceMetric &quot;ECGSampleArrayDeviceMetric&quot; </p><p style="margin-bottom: 0px">Profile: <a href="StructureDefinition-SampleArrayDeviceMetric.html">Sample Array DeviceMetric profile</a></p></div><p><b>Resolution extension</b>: 0.001</p><p><b>Sweep Speed extension</b>: 25 mm/s<span style="background: LightGoldenRodYellow"> (Details: UCUM code mm/s = 'mm/s')</span></p><p><b>type</b>: ECG <span style="background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki"> (<a href="http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html">ISO 11073-10101 Health informatics - Point-of-care</a>#131328 &quot;MDC_ECG_ELEC_POTL&quot;)</span></p><p><b>unit</b>: mV <span style="background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki"> (<a href="http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html">ISO 11073-10101 Health informatics - Point-of-care</a>#266418 &quot;MDC_DIM_MILLI_VOLT&quot;)</span></p><p><b>source</b>: <a href="Device-PhysioMonitorMdsDevice.html">Device/PhysioMonitorMdsDevice</a></p><p><b>parent</b>: <a href="Device-ECGChannelDevice.html">Device/ECGChannelDevice</a></p><p><b>operationalStatus</b>: on</p><p><b>color</b>: green</p><p><b>category</b>: measurement</p></div>
      </text>
      <extension
                 url="http://hl7.org/fhir/uv/pocd/StructureDefinition/resolution">
        <valueDecimal value="0.001"/>
      </extension>
      <extension
                 url="http://hl7.org/fhir/uv/pocd/StructureDefinition/sweep-speed">
        <valueQuantity>
          <value value="25"/>
          <unit value="mm/s"/>
          <system value="http://unitsofmeasure.org"/>
          <code value="mm/s"/>
        </valueQuantity>
      </extension>
      <type>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="131328"/>
          <display value="MDC_ECG_ELEC_POTL"/>
        </coding>
        <text value="ECG"/>
      </type>
      <unit>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="266418"/>
          <display value="MDC_DIM_MILLI_VOLT"/>
        </coding>
        <text value="mV"/>
      </unit>
      <source>
        <reference value="Device/PhysioMonitorMdsDevice"/>
      </source>
      <parent>
        <reference value="Device/ECGChannelDevice"/>
      </parent>
      <operationalStatus value="on"/>
      <color value="green"/>
      <category value="measurement"/>
    </DeviceMetric>