Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example Observation: CVP Sample Array observation example

Generated Narrative: Observation

Resource Observation "CVPSampleArrayObservation"

Profile: Sample Array Observation profile

status: final

code: MDC_PRESS_BLD_VEN_CENT (ISO 11073-10101 Health informatics - Point-of-care#150084)

subject: Patient/SomePatient " DOE"

effective: 2021-07-09 11:33:23+0200 --> 2021-07-09 11:33:24+0200

value: Origin: 0 mmHg, Interval: 8, Dimensions: 1, Data: 2.00 2.00 2.00 2.01 2.02 2.03 2.06 2.09 2.13 2.19 2.25 2.33 2.42 2.53 2.65 2.78 2.93 3.09 3.27 3.47 3.68 3.90 4.14 4.40 4.67 4.96 5.34 5.82 6.37 6.90 7.35 7.68 7.89 7.98 8.00 7.94 7.82 7.64 7.41 7.14 6.84 6.48 6.11 5.85 5.73 5.79 5.95 6.22 6.45 6.54 6.56 6.44 6.20 5.88 5.48 5.01 4.71 4.44 4.18 3.95 3.73 3.53 3.36 3.20 3.06 2.94 2.85 2.77 2.70 2.67 2.64 2.64 2.65 2.70 2.75 2.82 2.91 3.02 3.15 3.29 3.46 3.64 3.84 4.06 4.27 4.48 4.68 4.88 5.06 5.23 5.38 5.52 5.63 5.71 5.76 5.75 5.72 5.62 5.47 5.26 5.01 4.74 4.45 4.16 3.90 3.66 3.45 3.25 3.08 2.92 2.78 2.66 2.55 2.46 2.37 2.31 2.24 2.19 2.15 2.11 2.08 2.05 2.03 2.02 2.01

device: DeviceMetric/CVPSampleArrayDeviceMetric