Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Resource Profile: Channel Device profile

Official URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/ChannelDevice | Version: current
Draft as of 2022-01-16 | Computable Name: ChannelDevice

StructureDefinition for Device resources that represent Channels, which are used for grouping metrics together.

### Scope and Usage

This profile sets minimum expectations for the Device resource that represents a Channel, which is used for grouping metrics together.

Usage:

- Refer to this Resource Profile: Enumeration DeviceMetric profile, Numeric DeviceMetric profile and Sample Array DeviceMetric profile
- Examples for this Resource Profile: Device/BloodPressureChannelDevice, Device/ECGChannelDevice, Device/HeartRateChannelDevice and Device/NBPChannelDevice

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Differential Table
- Key Elements Table
- Snapshot Table
- Statistics/References
- All

This structure is derived from Device

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
instance | S | 0..1 | (Complex) | Instance number or label URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance
extension:number |  | 0..1 | Extension | Instance number
valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
extension:label |  | 0..1 | Extension | Instance label
valueString |  | 1..1 | string | Value of extension
operatingHours | S | 0..1 | unsignedInt | Operating hours URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours
valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
operatingCycles | S | 0..1 | unsignedInt | Operating cycles URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles
valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
identifier | S | 0..* | Identifier | Instance identifier
system |  | 0..1 | uri | The namespace for the identifier value
value |  | 0..1 | string | The value that is unique
status | S | 0..1 | code | active | inactive | entered-in-error | unknown
statusReason | S | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: MDC Object infrastructure and Device nomenclature (extensible)
coding |  | 0..* | Coding | Code defined by a terminology system
system |  | 0..1 | uri | Identity of the terminology system
version |  | 0..1 | string | Version of the system - if relevant
code |  | 0..1 | code | Symbol in syntax defined by the system
text |  | 0..1 | string | Plain text representation of the concept
version | S | 0..* | BackboneElement | The actual design of the device or software version running on the device
type |  | 0..1 | CodeableConcept | The type of the device version
coding |  | 0..* | Coding | Code defined by a terminology system
system |  | 0..1 | uri | Identity of the terminology system
version |  | 0..1 | string | Version of the system - if relevant
code |  | 0..1 | code | Symbol in syntax defined by the system
value |  | 1..1 | string | The version text
patient |  | 0..0 |  |
location |  | 0..0 |  |
safety | S | 0..* | CodeableConcept | Safety Characteristics of Device Binding: Safety (extensible): Safety classification
coding |  | 0..* | Coding | Code defined by a terminology system
system |  | 0..1 | uri | Identity of the terminology system
code |  | 0..1 | code | Symbol in syntax defined by the system
parent | S | 1..1 | Reference(VMD Device profile) | The parent device
Documentation for this format

#### Terminology Bindings (Differential)

Path | Conformance | ValueSet
Device.type | extensible | MdcObject
Device.safety | extensible | Safety

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
instance | S | 0..1 | (Complex) | Instance number or label URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance
extension:number |  | 0..1 | Extension | Instance number
url |  | 1..1 | uri | "number"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
extension:label |  | 0..1 | Extension | Instance label
url |  | 1..1 | uri | "label"
Slices for value[x] |  | 1..1 | string | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueString |  | 1..1 | string | Value of extension
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance"
operatingHours | S | 0..1 | unsignedInt | Operating hours URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours
extension |  | 0..0 |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
operatingCycles | S | 0..1 | unsignedInt | Operating cycles URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles
extension |  | 0..0 |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | S | 0..* | Identifier | Instance identifier
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
system | Σ | 0..1 | uri | The namespace for the identifier value Example General: http://www.acme.com/identifiers/patient
value | Σ | 0..1 | string | The value that is unique Example General: 123456
status | ?!S Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason | S | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: MDC Object infrastructure and Device nomenclature (extensible)
coding | Σ | 0..* | Coding | Code defined by a terminology system
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
text | Σ | 0..1 | string | Plain text representation of the concept
version | S | 0..* | BackboneElement | The actual design of the device or software version running on the device
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
coding | Σ | 0..* | Coding | Code defined by a terminology system
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
value |  | 1..1 | string | The version text
safety | S Σ | 0..* | CodeableConcept | Safety Characteristics of Device Binding: Safety (extensible): Safety classification
coding | Σ | 0..* | Coding | Code defined by a terminology system
system | Σ | 0..1 | uri | Identity of the terminology system
code | Σ | 0..1 | code | Symbol in syntax defined by the system
parent | S | 1..1 | Reference(VMD Device profile) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet
Device.identifier.use | required | IdentifierUse
Device.status | required | FHIRDeviceStatus
Device.statusReason | extensible | FHIRDeviceStatusReason
Device.type | extensible | MdcObject
Device.safety | extensible | Safety

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation
contained |  | 0..* | Resource | Contained, inline Resources
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
instance | S | 0..1 | (Complex) | Instance number or label URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance
id |  | 0..1 | string | Unique id for inter-element referencing
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
extension:number |  | 0..1 | Extension | Instance number
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
url |  | 1..1 | uri | "number"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
extension:label |  | 0..1 | Extension | Instance label
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
url |  | 1..1 | uri | "label"
Slices for value[x] |  | 1..1 | string | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueString |  | 1..1 | string | Value of extension
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance"
operatingHours | S | 0..1 | unsignedInt | Operating hours URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
operatingCycles | S | 0..1 | unsignedInt | Operating cycles URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | S | 0..* | Identifier | Instance identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 0..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
system | Σ | 0..1 | uri | The namespace for the identifier value Example General: http://www.acme.com/identifiers/patient
value | Σ | 0..1 | string | The value that is unique Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!S Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason | S | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: MDC Object infrastructure and Device nomenclature (extensible)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 0..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version | S | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 0..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | S Σ | 0..* | CodeableConcept | Safety Characteristics of Device Binding: Safety (extensible): Safety classification
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 0..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
parent | S | 1..1 | Reference(VMD Device profile) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet
Device.language | preferred | CommonLanguages
Additional Bindings | Purpose
AllLanguages | Max Binding
Device.identifier.use | required | IdentifierUse
Device.identifier.type | extensible | Identifier Type Codes
Device.udiCarrier.entryType | required | UDIEntryType
Device.status | required | FHIRDeviceStatus
Device.statusReason | extensible | FHIRDeviceStatusReason
Device.deviceName.type | required | DeviceNameType
Device.type | extensible | MdcObject
Device.safety | extensible | Safety

This structure is derived from Device

The profile defines the following rules:

- `Device.type` shall be present and have a coding from the ISO/IEEE 11073 MDC Device nomenclature if there is an appropriate code available.
- `Device.patient` and `Device.location` references must not be present.
- `Device.parent` shall be pesent and refer to the VMD Device resource which this channel belongs to.
- If multiple instances of the same Channel type exist, the Instance extension allows a sequence to be defined.
- Extensions allow operating hours and operating cycles to be added.

Differential View

This structure is derived from Device

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
instance | S | 0..1 | (Complex) | Instance number or label URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance
extension:number |  | 0..1 | Extension | Instance number
valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
extension:label |  | 0..1 | Extension | Instance label
valueString |  | 1..1 | string | Value of extension
operatingHours | S | 0..1 | unsignedInt | Operating hours URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours
valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
operatingCycles | S | 0..1 | unsignedInt | Operating cycles URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles
valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
identifier | S | 0..* | Identifier | Instance identifier
system |  | 0..1 | uri | The namespace for the identifier value
value |  | 0..1 | string | The value that is unique
status | S | 0..1 | code | active | inactive | entered-in-error | unknown
statusReason | S | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: MDC Object infrastructure and Device nomenclature (extensible)
coding |  | 0..* | Coding | Code defined by a terminology system
system |  | 0..1 | uri | Identity of the terminology system
version |  | 0..1 | string | Version of the system - if relevant
code |  | 0..1 | code | Symbol in syntax defined by the system
text |  | 0..1 | string | Plain text representation of the concept
version | S | 0..* | BackboneElement | The actual design of the device or software version running on the device
type |  | 0..1 | CodeableConcept | The type of the device version
coding |  | 0..* | Coding | Code defined by a terminology system
system |  | 0..1 | uri | Identity of the terminology system
version |  | 0..1 | string | Version of the system - if relevant
code |  | 0..1 | code | Symbol in syntax defined by the system
value |  | 1..1 | string | The version text
patient |  | 0..0 |  |
location |  | 0..0 |  |
safety | S | 0..* | CodeableConcept | Safety Characteristics of Device Binding: Safety (extensible): Safety classification
coding |  | 0..* | Coding | Code defined by a terminology system
system |  | 0..1 | uri | Identity of the terminology system
code |  | 0..1 | code | Symbol in syntax defined by the system
parent | S | 1..1 | Reference(VMD Device profile) | The parent device
Documentation for this format

#### Terminology Bindings (Differential)

Path | Conformance | ValueSet
Device.type | extensible | MdcObject
Device.safety | extensible | Safety

Key Elements View

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
instance | S | 0..1 | (Complex) | Instance number or label URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance
extension:number |  | 0..1 | Extension | Instance number
url |  | 1..1 | uri | "number"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
extension:label |  | 0..1 | Extension | Instance label
url |  | 1..1 | uri | "label"
Slices for value[x] |  | 1..1 | string | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueString |  | 1..1 | string | Value of extension
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance"
operatingHours | S | 0..1 | unsignedInt | Operating hours URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours
extension |  | 0..0 |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
operatingCycles | S | 0..1 | unsignedInt | Operating cycles URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles
extension |  | 0..0 |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | S | 0..* | Identifier | Instance identifier
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
system | Σ | 0..1 | uri | The namespace for the identifier value Example General: http://www.acme.com/identifiers/patient
value | Σ | 0..1 | string | The value that is unique Example General: 123456
status | ?!S Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason | S | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: MDC Object infrastructure and Device nomenclature (extensible)
coding | Σ | 0..* | Coding | Code defined by a terminology system
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
text | Σ | 0..1 | string | Plain text representation of the concept
version | S | 0..* | BackboneElement | The actual design of the device or software version running on the device
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
coding | Σ | 0..* | Coding | Code defined by a terminology system
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
value |  | 1..1 | string | The version text
safety | S Σ | 0..* | CodeableConcept | Safety Characteristics of Device Binding: Safety (extensible): Safety classification
coding | Σ | 0..* | Coding | Code defined by a terminology system
system | Σ | 0..1 | uri | Identity of the terminology system
code | Σ | 0..1 | code | Symbol in syntax defined by the system
parent | S | 1..1 | Reference(VMD Device profile) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet
Device.identifier.use | required | IdentifierUse
Device.status | required | FHIRDeviceStatus
Device.statusReason | extensible | FHIRDeviceStatusReason
Device.type | extensible | MdcObject
Device.safety | extensible | Safety

Snapshot View

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation
contained |  | 0..* | Resource | Contained, inline Resources
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
instance | S | 0..1 | (Complex) | Instance number or label URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance
id |  | 0..1 | string | Unique id for inter-element referencing
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
extension:number |  | 0..1 | Extension | Instance number
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
url |  | 1..1 | uri | "number"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
extension:label |  | 0..1 | Extension | Instance label
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
url |  | 1..1 | uri | "label"
Slices for value[x] |  | 1..1 | string | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueString |  | 1..1 | string | Value of extension
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance"
operatingHours | S | 0..1 | unsignedInt | Operating hours URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
operatingCycles | S | 0..1 | unsignedInt | Operating cycles URL: http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles"
Slices for value[x] |  | 1..1 | unsignedInt | Value of extension Slice: Unordered, Closed by type:$this
value[x]:valueUnsignedInt |  | 1..1 | unsignedInt | Value of extension
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | S | 0..* | Identifier | Instance identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 0..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
system | Σ | 0..1 | uri | The namespace for the identifier value Example General: http://www.acme.com/identifiers/patient
value | Σ | 0..1 | string | The value that is unique Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!S Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason | S | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: MDC Object infrastructure and Device nomenclature (extensible)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 0..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version | S | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 0..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | S Σ | 0..* | CodeableConcept | Safety Characteristics of Device Binding: Safety (extensible): Safety classification
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 0..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
parent | S | 1..1 | Reference(VMD Device profile) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet
Device.language | preferred | CommonLanguages
Additional Bindings | Purpose
AllLanguages | Max Binding
Device.identifier.use | required | IdentifierUse
Device.identifier.type | extensible | Identifier Type Codes
Device.udiCarrier.entryType | required | UDIEntryType
Device.status | required | FHIRDeviceStatus
Device.statusReason | extensible | FHIRDeviceStatusReason
Device.deviceName.type | required | DeviceNameType
Device.type | extensible | MdcObject
Device.safety | extensible | Safety

This structure is derived from Device

The profile defines the following rules:

- `Device.type` shall be present and have a coding from the ISO/IEEE 11073 MDC Device nomenclature if there is an appropriate code available.
- `Device.patient` and `Device.location` references must not be present.
- `Device.parent` shall be pesent and refer to the VMD Device resource which this channel belongs to.
- If multiple instances of the same Channel type exist, the Instance extension allows a sequence to be defined.
- Extensions allow operating hours and operating cycles to be added.

Other representations of profile: CSV, Excel, Schematron