Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example Device: Patient Monitor MDS example

Generated Narrative: Device

Resource Device "PhysioMonitorMdsDevice"

Profile: MDS Device profile

Approved Jurisdictions extension: United States of America (ISO 3166-1 Codes for the representation of names of countries and their subdivisions — Part 1: Country code#840)

Operator extension: Practitioner/SomePractitioner " CAREFUL"

Operating hours extension: 8760

Operating cycles extension: 156

Operating mode extension: Dmo

identifier: id: 01-23-45-67-89-AB-CD-EF

### UdiCarriers

- | DeviceIdentifier | CarrierHRF
* | 00012345678905 | (01)00012345678905(21)123456

status: active

manufacturer: MyCompany

serialNumber: 123456

### DeviceNames

- | Name | Type
* | MyPhysioMonitor | model-name

modelNumber: PM1

type: Patient Monitor (ISO 11073-10101 Health informatics - Point-of-care#69965 "MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS")

patient: Patient/SomePatient " DOE"

location: Location/SomeLocation "Bed 42"