Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## CodeSystem: Measurement status codes

Official URL: http://terminology.hl7.org/CodeSystem/measurement-status | Version: 1.0.0
Standards status: Trial-use | Maturity Level: 2 | Computable Name: MeasurementStatus

Measurement status definitions from the ISO/IEEE 11073-10201 DIM. This CodeSystem is intended to be part of THO (terminology.hl7.org) and the URL already assumes that.

This Code system is referenced in the content logical definition of the following value sets:

- ObservationInterpretation

Profile: Shareable CodeSystem

This case-insensitive code system `http://terminology.hl7.org/CodeSystem/measurement-status` defines the following codes:

Code | Display | Definition
questionable | Questionable | Data may not be reliable
calibration-ongoing | Calibration ongoing | Calibration is ongoing
validated-data | Validated data | Relevant, e.g., in an archive
early-indication | Early indication | Early estimate of value
msmt-ongoing | Measurement ongoing | Indicates that a new measurement is just being taken
in-alarm | Measurement in alarm | Measurement has an active alarm condition
alarm-inhibited | Measurement alarms inhibited | Measurement supports alarming and alarms are turned off