Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## ValueSet: Safety

Official URL: http://hl7.org/fhir/uv/pocd/ValueSet/safety | Version: 1.0.0
Standards status: Trial-use | Maturity Level: 2 | Computable Name: Safety

CodeSystem for IEEE 11073-10207 SafetyClassification

References

This value set is not used here; it may be used elsewhere (e.g. specifications and/or implementations that use this content)

### Logical Definition (CLD)

Profile: Shareable ValueSet

- Include all codes defined in `http://hl7.org/fhir/uv/pocd/CodeSystem/safety` version Not Stated (use latest from terminology server)

### Expansion

No Expansion for this valueset (Unknown Code System)

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code