Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Heart Rate Numeric observation example - JSON Representation

Page standards status: Informative

Raw json | Download

    {
      "resourceType" : "Observation",
      "id" : "HeartRateNumericObservation",
      "meta" : {
        "profile" : [
          🔗 "http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericObservation"
        ]
      },
      "text" : {
        "status" : "generated",
        "div" : "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p class=\"res-header-id\"><b>Generated Narrative: Observation HeartRateNumericObservation</b></p><a name=\"HeartRateNumericObservation\"> </a><a name=\"hcHeartRateNumericObservation\"> </a><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\"/><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-NumericObservation.html\">Numeric Observation profile</a></p></div><p><b>status</b>: Final</p><p><b>category</b>: <span title=\"Codes:{http://terminology.hl7.org/CodeSystem/observation-category vital-signs}\">Vital Signs</span></p><p><b>code</b>: <span title=\"Codes:{http://loinc.org 8867-4}, {urn:iso:std:iso:11073:10101 147842}\">Heart rate</span></p><p><b>subject</b>: <a href=\"Patient-SomePatient.html\">John Doe  Male, DoB: 1967-05-04 ( Medical record number)</a></p><p><b>effective</b>: 2021-07-09 11:33:24+0200</p><p><b>value</b>: 60 bpm<span style=\"background: LightGoldenRodYellow\"> (Details: UCUM  code/min = '/min')</span></p><p><b>device</b>: <a href=\"DeviceMetric-HeartRateNumericDeviceMetric.html\">DeviceMetric: extension = ,,; type = MDC_ECG_HEART_RATE; unit = MDC_DIM_BEAT_PER_MIN; operationalStatus = on; color = green; category = measurement</a></p></div>"
      },
      "status" : "final",
      "category" : [
        {
          "coding" : [
            {
              "system" : "http://terminology.hl7.org/CodeSystem/observation-category",
              "code" : "vital-signs",
              "display" : "Vital Signs"
            }
          ]
        }
      ],
      "code" : {
        "coding" : [
          {
            "system" : "http://loinc.org",
            "code" : "8867-4",
            "display" : "Heart rate"
          },
          {
            "system" : "urn:iso:std:iso:11073:10101",
            "code" : "147842",
            "display" : "MDC_ECG_HEART_RATE"
          }
        ]
      },
      "subject" : {
        🔗 "reference" : "Patient/SomePatient"
      },
      "effectiveDateTime" : "2021-07-09T11:33:24+02:00",
      "valueQuantity" : {
        "value" : 60,
        "unit" : "bpm",
        "system" : "http://unitsofmeasure.org",
        "code" : "/min"
      },
      "device" : {
        🔗 "reference" : "DeviceMetric/HeartRateNumericDeviceMetric"
      }
    }