# Reference range type value set - Point-of-Care Device Implementation Guide v1.0.0

* [**Table of Contents**](toc.md)
* [**Artifact List**](artifacts.md)
* **Reference range type value set**

## ValueSet: Reference range type value set 

| | | |
| :--- | :--- | :--- |
| *Official URL*:http://hl7.org/fhir/uv/pocd/ValueSet/reference-range-type | *Version*:1.0.0 | |
| * Standards status: *[Trial-use](http://hl7.org/fhir/R4/versions.html#std-process) | [Maturity Level](http://hl7.org/fhir/versions.html#maturity): 2 | *Computable Name*:ReferenceRangeType |

 
ValueSet for classifying the type of reference range applied to a DeviceMetric. 

 **References** 

* [Reference range extension](StructureDefinition-reference-range.md)

### Logical Definition (CLD)

 

### Expansion

-------

 Explanation of the columns that may appear on this page: 

| | |
| :--- | :--- |
| Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies |
| System | The source of the definition of the code (when the value set draws in codes defined elsewhere) |
| Code | The code (used as the code in the resource instance) |
| Display | The display (used in the*display*element of a[Coding](http://hl7.org/fhir/R4/datatypes.html#Coding)). If there is no display, implementers should not simply display the code, but map the concept into their application |
| Definition | An explanation of the meaning of the concept |
| Comments | Additional notes about how to use the code |



## Resource Content

```json
{
  "resourceType" : "ValueSet",
  "id" : "reference-range-type",
  "meta" : {
    "profile" : ["http://hl7.org/fhir/StructureDefinition/shareablevalueset"]
  },
  "extension" : [{
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-wg",
    "valueCode" : "dev"
  },
  {
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-fmm",
    "valueInteger" : 2,
    "_valueInteger" : {
      "extension" : [{
        "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
        "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
      }]
    }
  },
  {
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-standards-status",
    "valueCode" : "trial-use",
    "_valueCode" : {
      "extension" : [{
        "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
        "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
      }]
    }
  }],
  "url" : "http://hl7.org/fhir/uv/pocd/ValueSet/reference-range-type",
  "version" : "1.0.0",
  "name" : "ReferenceRangeType",
  "title" : "Reference Range Type",
  "status" : "draft",
  "experimental" : false,
  "date" : "2026-03-26",
  "publisher" : "HL7 International / Devices",
  "contact" : [{
    "telecom" : [{
      "system" : "url",
      "value" : "http://www.hl7.org/Special/committees/healthcaredevices"
    }]
  }],
  "description" : "ValueSet for classifying the type of reference range applied to a DeviceMetric.",
  "jurisdiction" : [{
    "coding" : [{
      "system" : "http://unstats.un.org/unsd/methods/m49/m49.htm",
      "code" : "001"
    }]
  }],
  "compose" : {
    "include" : [{
      "system" : "http://hl7.org/fhir/uv/pocd/CodeSystem/reference-range-type"
    },
    {
      "system" : "http://terminology.hl7.org/CodeSystem/referencerange-meaning"
    }]
  }
}

```
