Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## ValueSet: MDC Object infrastructure and Device nomenclature

Official URL: http://terminology.hl7.org/ValueSet/11073MDC-object | Version: 1.0.0
Standards status: Trial-use | Maturity Level: 2 | Computable Name: MdcObject

ValueSet for the ISO/IEEE 11073-10101 Nomenclature filtered by Object partition. This ValueSet is intended to be part of THO (terminology.hl7.org) and the URL already assumes that.

References

- Channel Device profile
- MDS Device profile
- VMD Device profile

### Logical Definition (CLD)

Profile: Shareable ValueSet

- Include codes from`urn:iso:std:iso:11073:10101` version ⏿2024-12-05 where partition = 1

### Expansion

Expansion performed internally based on codesystem MDC Nomenclature v2024-12-05 (CodeSystem)

This value set has 1,466 codes in it. In order to keep the publication size manageable, only a selection (1,000 codes) of the whole set of codes is shown.

System | Code | Display (en) | Definition | JSON | XML
`urn:iso:std:iso:11073:10101` | 65537 | MDC_MOC_VMO | VMO |  |
`urn:iso:std:iso:11073:10101` | 65538 | MDC_MOC_VMO_VMD | VMD |  |
`urn:iso:std:iso:11073:10101` | 65539 | MDC_MOC_VMO_CHAN | Channel |  |
`urn:iso:std:iso:11073:10101` | 65540 | MDC_MOC_VMO_METRIC | Metric |  |
`urn:iso:std:iso:11073:10101` | 65541 | MDC_MOC_VMO_METRIC_ENUM | Enumeration |  |
`urn:iso:std:iso:11073:10101` | 65542 | MDC_MOC_VMO_METRIC_NU | Numeric |  |
`urn:iso:std:iso:11073:10101` | 65543 | MDC_MOC_VMO_METRIC_SA | Sample Array |  |
`urn:iso:std:iso:11073:10101` | 65544 | MDC_MOC_VMO_METRIC_SA_D | Distribution Sample Array |  |
`urn:iso:std:iso:11073:10101` | 65545 | MDC_MOC_VMO_METRIC_SA_RT | Real Time Sample Array |  |
`urn:iso:std:iso:11073:10101` | 65546 | MDC_MOC_VMO_METRIC_SA_T | Time Sample Array |  |
`urn:iso:std:iso:11073:10101` | 65552 | MDC_MOC_SCAN | Scanner |  |
`urn:iso:std:iso:11073:10101` | 65553 | MDC_MOC_SCAN_CFG | Configurable Scanner |  |
`urn:iso:std:iso:11073:10101` | 65554 | MDC_MOC_SCAN_CFG_EPI | Episodic Configurable Scanner |  |
`urn:iso:std:iso:11073:10101` | 65555 | MDC_MOC_SCAN_CFG_PERI | Periodic Configurable Scanner |  |
`urn:iso:std:iso:11073:10101` | 65556 | MDC_MOC_SCAN_CFG_PERI_FAST | Fast Periodic Configurable Scanner |  |
`urn:iso:std:iso:11073:10101` | 65557 | MDC_MOC_SCAN_UCFG | Unconfigurable Scanner |  |
`urn:iso:std:iso:11073:10101` | 65558 | MDC_MOC_SCAN_UCFG_ALSTAT | Alert Scanner |  |
`urn:iso:std:iso:11073:10101` | 65559 | MDC_MOC_SCAN_UCFG_CTXT | Context Scanner |  |
`urn:iso:std:iso:11073:10101` | 65560 | MDC_MOC_SCAN_UCFG_OP | Operating Scanner |  |
`urn:iso:std:iso:11073:10101` | 65564 | MDC_MOC_CC | Communication Controller |  |
`urn:iso:std:iso:11073:10101` | 65568 | MDC_MOC_VMS | VMS |  |
`urn:iso:std:iso:11073:10101` | 65569 | MDC_MOC_VMS_MDS | MDS |  |
`urn:iso:std:iso:11073:10101` | 65570 | MDC_MOC_VMS_MDS_COMPOS_MULTI_BED | Composite Multiple Bed MDS |  |
`urn:iso:std:iso:11073:10101` | 65571 | MDC_MOC_VMS_MDS_COMPOS_SINGLE_BED | Composite Single Bed MDS |  |
`urn:iso:std:iso:11073:10101` | 65572 | MDC_MOC_VMS_MDS_HYD | Hydra MDS |  |
`urn:iso:std:iso:11073:10101` | 65573 | MDC_MOC_VMS_MDS_SIMP | Simple MDS |  |
`urn:iso:std:iso:11073:10101` | 65574 | MDC_MOC_LOG | Log |  |
`urn:iso:std:iso:11073:10101` | 65575 | MDC_MOC_LOG_ERR | Log error |  |
`urn:iso:std:iso:11073:10101` | 65576 | MDC_MOC_LOG_SERV | Log server |  |
`urn:iso:std:iso:11073:10101` | 65577 | MDC_MOC_BATT | Battery |  |
`urn:iso:std:iso:11073:10101` | 65578 | MDC_MOC_PT_DEMOG | Patient Demographics |  |
`urn:iso:std:iso:11073:10101` | 65579 | MDC_MOC_CNTRL_SCO | SCO |  |
`urn:iso:std:iso:11073:10101` | 65580 | MDC_MOC_CNTRL_OP | Operation |  |
`urn:iso:std:iso:11073:10101` | 65581 | MDC_MOC_CNTRL_OP_SEL_IT | Select Item Operation |  |
`urn:iso:std:iso:11073:10101` | 65582 | MDC_MOC_CNTRL_OP_SEL_IT_A | Select Item Operation |  |
`urn:iso:std:iso:11073:10101` | 65583 | MDC_MOC_CNTRL_OP_SEL_VAL | Set Value Operation |  |
`urn:iso:std:iso:11073:10101` | 65584 | MDC_MOC_CNTRL_OP_SEL_VAL_A | Set Value Operation |  |
`urn:iso:std:iso:11073:10101` | 65585 | MDC_MOC_CNTRL_OP_TOG | Toggle Flag Operation |  |
`urn:iso:std:iso:11073:10101` | 65586 | MDC_MOC_CNTRL_OP_ACTIV | Activate Operation |  |
`urn:iso:std:iso:11073:10101` | 65587 | MDC_MOC_CNTRL_OP_LIM | Limit Alert Operation |  |
`urn:iso:std:iso:11073:10101` | 65588 | MDC_MOC_VMO_AL | Alert |  |
`urn:iso:std:iso:11073:10101` | 65589 | MDC_MOC_VMO_AL_STAT | Alert Status |  |
`urn:iso:std:iso:11073:10101` | 65590 | MDC_MOC_VMO_AL_MON | Alert Monitor |  |
`urn:iso:std:iso:11073:10101` | 65597 | MDC_MOC_VMO_PMSTORE | PM-Store |  |
`urn:iso:std:iso:11073:10101` | 65598 | MDC_MOC_PM_SEGMENT | PM-Segment |  |
`urn:iso:std:iso:11073:10101` | 65599 | MDC_MOC_ARCHIVE_MULTI_PT | Multipatient Archive |  |
`urn:iso:std:iso:11073:10101` | 65600 | MDC_MOC_ARCHIVE_PT | Patient Archive |  |
`urn:iso:std:iso:11073:10101` | 65601 | MDC_MOC_ARCHIVE_SESSION | Session Archive |  |
`urn:iso:std:iso:11073:10101` | 65602 | MDC_MOC_DISCRIM | Discriminator |  |
`urn:iso:std:iso:11073:10101` | 65603 | MDC_MOC_PHYSICIAN | Physician |  |
`urn:iso:std:iso:11073:10101` | 65604 | MDC_MOC_SESSION_NOTES | Session Notes |  |
`urn:iso:std:iso:11073:10101` | 65605 | MDC_MOC_SESSION_TEST | Session Test |  |
`urn:iso:std:iso:11073:10101` | 65606 | MDC_MOC_TOP | Top |  |
`urn:iso:std:iso:11073:10101` | 65608 | MDC_MOC_LOG_EVENT | Event Log |  |
`urn:iso:std:iso:11073:10101` | 65609 | MDC_MOC_CNTRL_OP_SET_STRING | Set String Operation |  |
`urn:iso:std:iso:11073:10101` | 65610 | MDC_MOC_PRINTER | Printer |  |
`urn:iso:std:iso:11073:10101` | 65611 | MDC_MOC_PT_DEMOG_MGR | Patient demographics manager |  |
`urn:iso:std:iso:11073:10101` | 65612 | MDC_MOC_DCC | DCC [device communication controller] |  |
`urn:iso:std:iso:11073:10101` | 65613 | MDC_MOC_BCC | BCC [bedside communication controller] |  |
`urn:iso:std:iso:11073:10101` | 65614 | MDC_MOC_CLOCK | Clock |  |
`urn:iso:std:iso:11073:10101` | 65615 | MDC_MOC_VMO_METRIC_CMPLX | Complex Metric |  |
`urn:iso:std:iso:11073:10101` | 65616 | MDC_MOC_CNTRL_OP_SET_RANGE | Set Range Operation |  |
`urn:iso:std:iso:11073:10101` | 66817 | MDC_ALSTAT_MDS | Device to monitor system status. |  |
`urn:iso:std:iso:11073:10101` | 66818 | MDC_ALSTAT_VMD | Device to monitor system status. |  |
`urn:iso:std:iso:11073:10101` | 67073 | MDC_PMSTORE_PERI_SIMP |  |  |
`urn:iso:std:iso:11073:10101` | 67074 | MDC_PMSTORE_PERI_CMPD |  |  |
`urn:iso:std:iso:11073:10101` | 67075 | MDC_PMSTORE_PERI_CMPLX |  |  |
`urn:iso:std:iso:11073:10101` | 67076 | MDC_PMSTORE_EPI_SIMP |  |  |
`urn:iso:std:iso:11073:10101` | 67077 | MDC_PMSTORE_EPI_CMPD |  |  |
`urn:iso:std:iso:11073:10101` | 67078 | MDC_PMSTORE_EPI_CMPLX |  |  |
`urn:iso:std:iso:11073:10101` | 67585 | MDC_ATTR_GRP_AL_MON | Alert Monitor Group |  |
`urn:iso:std:iso:11073:10101` | 67586 | MDC_ATTR_GRP_AL_STAT | Alert Status Group |  |
`urn:iso:std:iso:11073:10101` | 67587 | MDC_ATTR_GRP_METRIC_VAL_OBS | Metric Observed Value Group |  |
`urn:iso:std:iso:11073:10101` | 67588 | MDC_ATTR_GRP_OP_DYN_CTXT | Operation Dynamic Context Group |  |
`urn:iso:std:iso:11073:10101` | 67589 | MDC_ATTR_GRP_OP_STATIC_CTXT | Operation Static Context Group |  |
`urn:iso:std:iso:11073:10101` | 67590 | MDC_ATTR_GRP_PMSTORE | PM-Store Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67591 | MDC_ATTR_GRP_PT_DEMOG | Patient Demographics Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67592 | MDC_ATTR_GRP_SCAN | Scanner Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67593 | MDC_ATTR_GRP_SCO_TRANSACTION | SCO Transaction Group |  |
`urn:iso:std:iso:11073:10101` | 67594 | MDC_ATTR_GRP_SYS_APPL | System Application Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67595 | MDC_ATTR_GRP_SYS_ID | System Identification Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67596 | MDC_ATTR_GRP_SYS_PROD | System Production Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67598 | MDC_ATTR_GRP_VMD_APPL | VMD Application Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67599 | MDC_ATTR_GRP_VMD_PROD | VMD Production Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67600 | MDC_ATTR_GRP_VMO_DYN | VMO Dynamic Context Group * |  |
`urn:iso:std:iso:11073:10101` | 67601 | MDC_ATTR_GRP_VMO_STATIC | VMO Static Context Group * |  |
`urn:iso:std:iso:11073:10101` | 67603 | MDC_ATTR_GRP_AL | Alert Group |  |
`urn:iso:std:iso:11073:10101` | 67604 | MDC_ATTR_GRP_ARCHIVE | Archival Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67605 | MDC_ATTR_GRP_BATT | Battery Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67606 | MDC_ATTR_GRP_DISCRIM | Discriminator Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67607 | MDC_ATTR_GRP_PHYSICIAN | Physician Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67608 | MDC_ATTR_GRP_RELATION | Relationship Attribute Group * |  |
`urn:iso:std:iso:11073:10101` | 67609 | MDC_ATTR_GRP_T_PROFILE_MGMT |  |  |
`urn:iso:std:iso:11073:10101` | 67610 | MDC_ATTR_GRP_PRINTER |  |  |
`urn:iso:std:iso:11073:10101` | 67611 | MDC_ATTR_GRP_PDMO_STATIC | Patient Demographics Management Static Group |  |
`urn:iso:std:iso:11073:10101` | 67612 | MDC_ATTR_GRP_PDMO_DYN | Patient Demographics Management Dynamic Group |  |
`urn:iso:std:iso:11073:10101` | 67613 | MDC_ATTR_GRP_CC | Communication Controller Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 67614 | MDC_ATTR_GRP_CLOCK | Clock Attribute Group |  |
`urn:iso:std:iso:11073:10101` | 68162 | MDC_ATTR_FILTER_LABEL_STRING | Filter-Label-String |  |
`urn:iso:std:iso:11073:10101` | 68163 | MDC_ATTR_ENUM_RANGE_MSMT_LABELS | Enum-Measure-Range-Labels |  |
`urn:iso:std:iso:11073:10101` | 67841 | MDC_ATTR_AL_LIMIT_SPEC_LIST | Limit-Spec-List |  |
`urn:iso:std:iso:11073:10101` | 67842 | MDC_ATTR_AL_MON_P_AL_LIST | Device-P-Alarm-List |  |
`urn:iso:std:iso:11073:10101` | 67843 | MDC_ATTR_AL_MON_S_AL_LIST | Device-Sup-Alarm-List |  |
`urn:iso:std:iso:11073:10101` | 67844 | MDC_ATTR_AL_MON_T_AL_LIST | Device-T-Alarm-List |  |
`urn:iso:std:iso:11073:10101` | 67845 | MDC_ATTR_AL_OP_CAPAB | Alert-Op-Capability |  |
`urn:iso:std:iso:11073:10101` | 67846 | MDC_ATTR_AL_OP_STAT | Alert-Op-State |  |
`urn:iso:std:iso:11073:10101` | 67847 | MDC_ATTR_AL_OP_TEXT | Alert-Op-Text-String |  |
`urn:iso:std:iso:11073:10101` | 67848 | MDC_ATTR_AL_STAT_AL_C_LIST | Alert-Capab-List |  |
`urn:iso:std:iso:11073:10101` | 67850 | MDC_ATTR_AL_STAT_P_AL_LIST | Physio-Alert-List |  |
`urn:iso:std:iso:11073:10101` | 67851 | MDC_ATTR_AL_STAT_T_AL_LIST | Tech-Alert-List |  |
`urn:iso:std:iso:11073:10101` | 67852 | MDC_ATTR_ALTITUDE | Altitude |  |
`urn:iso:std:iso:11073:10101` | 67853 | MDC_ATTR_AREA_APPL | Application-Area |  |
`urn:iso:std:iso:11073:10101` | 67854 | MDC_ATTR_CHAN_ID | Channel-Id |  |
`urn:iso:std:iso:11073:10101` | 67855 | MDC_ATTR_CHAN_NUM_PHYS | Physical-Channel-Number |  |
`urn:iso:std:iso:11073:10101` | 67856 | MDC_ATTR_CHAN_STAT | Channel-Status |  |
`urn:iso:std:iso:11073:10101` | 67857 | MDC_ATTR_COLOR | Color |  |
`urn:iso:std:iso:11073:10101` | 67858 | MDC_ATTR_COMPRES | Compression |  |
`urn:iso:std:iso:11073:10101` | 67859 | MDC_ATTR_CONFIRM_MODE | Confirm-Mode |  |
`urn:iso:std:iso:11073:10101` | 67860 | MDC_ATTR_CONFIRM_TIMEOUT | Confirm-Timeout |  |
`urn:iso:std:iso:11073:10101` | 67861 | MDC_ATTR_CYC_OP | Operation-Cycles |  |
`urn:iso:std:iso:11073:10101` | 67862 | MDC_ATTR_DEV_AL_COND | Device-Alert-Condition |  |
`urn:iso:std:iso:11073:10101` | 67863 | MDC_ATTR_DISP_RES | Display-Resolution |  |
`urn:iso:std:iso:11073:10101` | 67864 | MDC_ATTR_ERR_LOG_ENTRY_LIST | Error-Log-Entry-List |  |
`urn:iso:std:iso:11073:10101` | 67865 | MDC_ATTR_FILTER_SPECN | Filter-Specification |  |
`urn:iso:std:iso:11073:10101` | 67866 | MDC_ATTR_GRID_VIS_I16 | Visual-Grid |  |
`urn:iso:std:iso:11073:10101` | 67867 | MDC_ATTR_GRID_VIS_I32 | Visual-Grid |  |
`urn:iso:std:iso:11073:10101` | 67868 | MDC_ATTR_GRID_VIS_I8 | Visual-Grid |  |
`urn:iso:std:iso:11073:10101` | 67869 | MDC_ATTR_ID_ASSOC_NO | Association-Invoke-Id |  |
`urn:iso:std:iso:11073:10101` | 67870 | MDC_ATTR_ID_BED_LABEL | Bed-Label |  |
`urn:iso:std:iso:11073:10101` | 67871 | MDC_ATTR_ID_CHAN_NUM_PHYS | Physical-Channel-Label |  |
`urn:iso:std:iso:11073:10101` | 67872 | MDC_ATTR_ID_COMPAT | Compatibility-Id * |  |
`urn:iso:std:iso:11073:10101` | 67873 | MDC_ATTR_ID_HANDLE | Handle * |  |
`urn:iso:std:iso:11073:10101` | 67874 | MDC_ATTR_ID_INSTNO | Instance-Number * |  |
`urn:iso:std:iso:11073:10101` | 67875 | MDC_ATTR_ID_INVOK_COOKIE | Invoke-Cookie |  |
`urn:iso:std:iso:11073:10101` | 67876 | MDC_ATTR_ID_LABEL |  |  |
`urn:iso:std:iso:11073:10101` | 67877 | MDC_ATTR_ID_LABEL_ACT |  |  |
`urn:iso:std:iso:11073:10101` | 67878 | MDC_ATTR_ID_LABEL_HELP |  |  |
`urn:iso:std:iso:11073:10101` | 67879 | MDC_ATTR_ID_LABEL_STRING | Label |  |
`urn:iso:std:iso:11073:10101` | 67880 | MDC_ATTR_ID_MODEL | Vmd-Model * |  |
`urn:iso:std:iso:11073:10101` | 67881 | MDC_ATTR_ID_NOM_PARTITION | Nom-Partition |  |
`urn:iso:std:iso:11073:10101` | 67882 | MDC_ATTR_ID_PARAM_GRP | Parameter-Group |  |
`urn:iso:std:iso:11073:10101` | 67883 | MDC_ATTR_ID_PHYSIO | Metric-Id (”Physio ID”) |  |
`urn:iso:std:iso:11073:10101` | 67884 | MDC_ATTR_ID_POSN | Position |  |
`urn:iso:std:iso:11073:10101` | 67885 | MDC_ATTR_ID_PROD_SPECN | Production-Specification * |  |
`urn:iso:std:iso:11073:10101` | 67886 | MDC_ATTR_ID_SOFT | Soft-Id |  |
`urn:iso:std:iso:11073:10101` | 67887 | MDC_ATTR_ID_TYPE | Type |  |
`urn:iso:std:iso:11073:10101` | 67888 | MDC_ATTR_ID_TYPE_ACT |  |  |
`urn:iso:std:iso:11073:10101` | 67889 | MDC_ATTR_ID_TYPE_METRIC_STAT | Metric-Id |  |
`urn:iso:std:iso:11073:10101` | 67890 | MDC_ATTR_INDEX_SEL | Selected-Item-Index |  |
`urn:iso:std:iso:11073:10101` | 67891 | MDC_ATTR_INDIC_ACTIV | Activity-Indicator |  |
`urn:iso:std:iso:11073:10101` | 67892 | MDC_ATTR_LIMIT_CURR | Limit Alert Operation |  |
`urn:iso:std:iso:11073:10101` | 67893 | MDC_ATTR_LINE_FREQ | Line-Frequency |  |
`urn:iso:std:iso:11073:10101` | 67894 | MDC_ATTR_LIST_SEL | Select-List |  |
`urn:iso:std:iso:11073:10101` | 67895 | MDC_ATTR_LOCALIZN | Localization |  |
`urn:iso:std:iso:11073:10101` | 67896 | MDC_ATTR_LOG_ENTRIES_CURR | Current-Log-Entries |  |
`urn:iso:std:iso:11073:10101` | 67897 | MDC_ATTR_LOG_ENTRIES_MAX | Max-Log-Entries |  |
`urn:iso:std:iso:11073:10101` | 67898 | MDC_ATTR_METRIC_CALIB | Metric-Calibration |  |
`urn:iso:std:iso:11073:10101` | 67899 | MDC_ATTR_METRIC_CLASS | Metric-Class |  |
`urn:iso:std:iso:11073:10101` | 67900 | MDC_ATTR_METRIC_INFO_LABEL | Metric-Info-Label |  |
`urn:iso:std:iso:11073:10101` | 67901 | MDC_ATTR_METRIC_INFO_LABEL_STR | Metric-Info-Label-String |  |
`urn:iso:std:iso:11073:10101` | 67902 | MDC_ATTR_METRIC_LIST_SRC | Metric-Source-List |  |
`urn:iso:std:iso:11073:10101` | 67903 | MDC_ATTR_METRIC_SPECN | Metric-Specification |  |
`urn:iso:std:iso:11073:10101` | 67904 | MDC_ATTR_METRIC_STAT | Metric-Status |  |
`urn:iso:std:iso:11073:10101` | 67905 | MDC_ATTR_METRIC_STORE_CAPAC_CNT | Store-Capacity-Count |  |
`urn:iso:std:iso:11073:10101` | 67906 | MDC_ATTR_METRIC_STORE_FORMAT | Storage-Format |  |
`urn:iso:std:iso:11073:10101` | 67907 | MDC_ATTR_METRIC_STORE_SAMPLE_ALG | Store-Sample-Algorithm |  |
`urn:iso:std:iso:11073:10101` | 67908 | MDC_ATTR_METRIC_STORE_USAGE_CNT | Store-Usage-Count |  |
`urn:iso:std:iso:11073:10101` | 67909 | MDC_ATTR_MODE_MSMT | Measure-Mode |  |
`urn:iso:std:iso:11073:10101` | 67910 | MDC_ATTR_MODE_OP | Operating-Mode |  |
`urn:iso:std:iso:11073:10101` | 67911 | MDC_ATTR_MSMT_STAT | Measurement-Status |  |
`urn:iso:std:iso:11073:10101` | 67912 | MDC_ATTR_NOM_VERS | Nomenclature-Version |  |
`urn:iso:std:iso:11073:10101` | 67914 | MDC_ATTR_NU_ACCUR_MSMT | Accuracy |  |
`urn:iso:std:iso:11073:10101` | 67915 | MDC_ATTR_NU_CMPD_VAL_OBS | Compound-Nu-Observed-Value |  |
`urn:iso:std:iso:11073:10101` | 67917 | MDC_ATTR_NU_MSMT_RES | Nu-Measure-Resolution |  |
`urn:iso:std:iso:11073:10101` | 67918 | MDC_ATTR_NU_RANGE_MSMT | Nu-Measure-Range |  |
`urn:iso:std:iso:11073:10101` | 67919 | MDC_ATTR_NU_RANGE_PHYSIO | Nu-Physiological-Range |  |
`urn:iso:std:iso:11073:10101` | 67920 | MDC_ATTR_NU_VAL_OBS | Nu-Observed-Value |  |
`urn:iso:std:iso:11073:10101` | 67921 | MDC_ATTR_NUM_SEG | Number-of-Segments |  |
`urn:iso:std:iso:11073:10101` | 67922 | MDC_ATTR_OP_SPEC | Operation-Spec |  |
`urn:iso:std:iso:11073:10101` | 67923 | MDC_ATTR_OP_STAT | Operational-State * |  |
`urn:iso:std:iso:11073:10101` | 67924 | MDC_ATTR_OP_TEXT | Operation-Text |  |
`urn:iso:std:iso:11073:10101` | 67925 | MDC_ATTR_POWER_STAT | Power-Status |  |
`urn:iso:std:iso:11073:10101` | 67926 | MDC_ATTR_PT_BSA | Patient-Bsa |  |
`urn:iso:std:iso:11073:10101` | 67927 | MDC_ATTR_PT_DEMOG_ST | Pat-Demo-State |  |
`urn:iso:std:iso:11073:10101` | 67928 | MDC_ATTR_PT_DOB | Date-Of-Birth |  |
`urn:iso:std:iso:11073:10101` | 67929 | MDC_ATTR_PT_GEN_INFO | Patient-General-Info |  |
`urn:iso:std:iso:11073:10101` | 67930 | MDC_ATTR_PT_ID | Patient-Id |  |
`urn:iso:std:iso:11073:10101` | 67931 | MDC_ATTR_PT_NAME | Name |  |
`urn:iso:std:iso:11073:10101` | 67932 | MDC_ATTR_PT_NAME_FAMILY | Family-Name |  |
`urn:iso:std:iso:11073:10101` | 67933 | MDC_ATTR_PT_NAME_GIVEN | Given-Name |  |
`urn:iso:std:iso:11073:10101` | 67934 | MDC_ATTR_PT_NAME_BIRTH | Birth-Name |  |
`urn:iso:std:iso:11073:10101` | 67935 | MDC_ATTR_PT_NAME_MIDDLE | Middle-Name |  |
`urn:iso:std:iso:11073:10101` | 67936 | MDC_ATTR_PT_NAME_TITLE | Title-Name |  |
`urn:iso:std:iso:11073:10101` | 67937 | MDC_ATTR_PT_SEX | Sex |  |
`urn:iso:std:iso:11073:10101` | 67938 | MDC_ATTR_PT_TYPE | Patient-Type * |  |
`urn:iso:std:iso:11073:10101` | 67939 | MDC_ATTR_RANGE_DISTRIB | Distribution-Range-Specification |  |
`urn:iso:std:iso:11073:10101` | 67940 | MDC_ATTR_SA_CALIB_I16 | Sa-Calibration-Data |  |
`urn:iso:std:iso:11073:10101` | 67941 | MDC_ATTR_SA_CALIB_I32 | Sa-Calibration-Data |  |
`urn:iso:std:iso:11073:10101` | 67942 | MDC_ATTR_SA_CALIB_I8 | Sa-Calibration-Data |  |
`urn:iso:std:iso:11073:10101` | 67943 | MDC_ATTR_SA_CMPD_VAL_OBS | Compound-Sa-Observed-Value |  |
`urn:iso:std:iso:11073:10101` | 67944 | MDC_ATTR_SA_FREQ_SIG | Sa-Signal-Frequency |  |
`urn:iso:std:iso:11073:10101` | 67945 | MDC_ATTR_SA_MSMT_RES | Sa-Measure-Resolution |  |
`urn:iso:std:iso:11073:10101` | 67946 | MDC_ATTR_SA_RANGE_PHYS_I16 | Sa-Physiological-Range |  |
`urn:iso:std:iso:11073:10101` | 67947 | MDC_ATTR_SA_RANGE_PHYS_I32 | Sa-Physiological-Range |  |
`urn:iso:std:iso:11073:10101` | 67948 | MDC_ATTR_SA_RANGE_PHYS_I8 | Sa-Physiological-Range |  |
`urn:iso:std:iso:11073:10101` | 67949 | MDC_ATTR_SA_SPECN | Sa-Specification |  |
`urn:iso:std:iso:11073:10101` | 67950 | MDC_ATTR_SA_VAL_OBS | Sa-Observed-Value |  |
`urn:iso:std:iso:11073:10101` | 67951 | MDC_ATTR_SCALE_SPECN_I16 | Scale-and-Range-Specification |  |
`urn:iso:std:iso:11073:10101` | 67952 | MDC_ATTR_SCALE_SPECN_I32 | Scale-and-Range-Specification |  |
`urn:iso:std:iso:11073:10101` | 67953 | MDC_ATTR_SCALE_SPECN_I8 | Scale-and-Range-Specification |  |
`urn:iso:std:iso:11073:10101` | 67954 | MDC_ATTR_SCAN_CTXT_MODE | Context-Mode |  |
`urn:iso:std:iso:11073:10101` | 67955 | MDC_ATTR_SCAN_EXTEND | Scan-Extensibility |  |
`urn:iso:std:iso:11073:10101` | 67956 | MDC_ATTR_SCAN_LIST | Scan-List |  |
`urn:iso:std:iso:11073:10101` | 67957 | MDC_ATTR_SCAN_REP_PD | Reporting-Interval |  |
`urn:iso:std:iso:11073:10101` | 67958 | MDC_ATTR_SCO_CAPAB | Sco-Capability |  |
`urn:iso:std:iso:11073:10101` | 67960 | MDC_ATTR_SEG_DATA_GEN | Segment-Data |  |
`urn:iso:std:iso:11073:10101` | 67961 | MDC_ATTR_SEG_DATA_NU_OPT | Segment-Data |  |
`urn:iso:std:iso:11073:10101` | 67962 | MDC_ATTR_SEG_DATA_RTSA_OPT | Segment-Data |  |
`urn:iso:std:iso:11073:10101` | 67963 | MDC_ATTR_SEG_USAGE_CNT | Segment-Usage-Count |  |
`urn:iso:std:iso:11073:10101` | 67964 | MDC_ATTR_SETTINGS_SYST |  |  |
`urn:iso:std:iso:11073:10101` | 67965 | MDC_ATTR_SITE_LIST_BODY | Body-Site-List |  |
`urn:iso:std:iso:11073:10101` | 67966 | MDC_ATTR_SITE_LIST_MSMT | Msmt-Site-List |  |
`urn:iso:std:iso:11073:10101` | 67967 | MDC_ATTR_SPD_SWEEP_DEFAULT | Sweep-Speed |  |
`urn:iso:std:iso:11073:10101` | 67968 | MDC_ATTR_STAT_LOCK | Lock-State |  |
`urn:iso:std:iso:11073:10101` | 67969 | MDC_ATTR_STAT_OP_TOG | Toggle-State |  |
`urn:iso:std:iso:11073:10101` | 67970 | MDC_ATTR_STD_SAFETY |  |  |
`urn:iso:std:iso:11073:10101` | 67971 | MDC_ATTR_SYS_CAPAB | System-Capability |  |
`urn:iso:std:iso:11073:10101` | 67972 | MDC_ATTR_SYS_ID | System-Id * |  |
`urn:iso:std:iso:11073:10101` | 67973 | MDC_ATTR_SYS_SPECN | System-Specification |  |
`urn:iso:std:iso:11073:10101` | 67974 | MDC_ATTR_SYS_TYPE | System-Type |  |
`urn:iso:std:iso:11073:10101` | 67975 | MDC_ATTR_TIME_ABS | Specifies the absolute date and time for system or device clock and derived objects (resolution of up to 1/100 of a second, encoded as eight pairs of 4-bit BCD nibbles denoting the { century, year, month, day, hour, minute, second, sec-fractions }). |  |
`urn:iso:std:iso:11073:10101` | 67976 | MDC_ATTR_TIME_BATT_REMAIN | Remaining-Battery-Time * |  |
`urn:iso:std:iso:11073:10101` | 67978 | MDC_ATTR_TIME_END_SEG | Segment-End-Abs-Time |  |
`urn:iso:std:iso:11073:10101` | 67979 | MDC_ATTR_TIME_PD_MSMT | Measure-Period |  |
`urn:iso:std:iso:11073:10101` | 67980 | MDC_ATTR_TIME_PD_OP_HRS | Operating-Hours |  |
`urn:iso:std:iso:11073:10101` | 67981 | MDC_ATTR_TIME_PD_SAMP | Sample-Period |  |
`urn:iso:std:iso:11073:10101` | 67982 | MDC_ATTR_TIME_PD_AL_SUSP | Suspension-Period |  |
`urn:iso:std:iso:11073:10101` | 67983 | MDC_ATTR_TIME_REL | Specifies the relative time value for system or device clock and derived objects (default 125 μs resolution counter having an arbitrary start time and value). |  |
`urn:iso:std:iso:11073:10101` | 67984 | MDC_ATTR_TIME_STAMP_ABS | Absolute time stamp value for observations and derived objects. |  |
`urn:iso:std:iso:11073:10101` | 67985 | MDC_ATTR_TIME_STAMP_REL | Relative time stamp value for observations and derived objects. |  |
`urn:iso:std:iso:11073:10101` | 67986 | MDC_ATTR_TIME_START_SEG | Segment-Start-Abs-Time |  |
`urn:iso:std:iso:11073:10101` | 67987 | MDC_ATTR_TOG_LABELS |  |  |
`urn:iso:std:iso:11073:10101` | 67988 | MDC_ATTR_TSA_MARKER_LIST | Tsa-Marker-List |  |
`urn:iso:std:iso:11073:10101` | 67989 | MDC_ATTR_TX_WIND | Transmit-Window |  |
`urn:iso:std:iso:11073:10101` | 67990 | MDC_ATTR_UNIT_CODE | Unit-Code * |  |
`urn:iso:std:iso:11073:10101` | 67991 | MDC_ATTR_UNIT_CODE_X | x-Unit-Code |  |
`urn:iso:std:iso:11073:10101` | 67992 | MDC_ATTR_UNIT_LABEL |  |  |
`urn:iso:std:iso:11073:10101` | 67993 | MDC_ATTR_UNIT_LABEL_STRING | Unit-Label-String |  |
`urn:iso:std:iso:11073:10101` | 67994 | MDC_ATTR_UNIT_LABEL_STRING_X | x-Unit-Label-String |  |
`urn:iso:std:iso:11073:10101` | 67995 | MDC_ATTR_UNIT_LABEL_X |  |  |
`urn:iso:std:iso:11073:10101` | 67996 | MDC_ATTR_VAL_BATT_CHARGE | Battery-Level (”charge”) |  |
`urn:iso:std:iso:11073:10101` | 67997 | MDC_ATTR_VAL_CURR | Current-Value |  |
`urn:iso:std:iso:11073:10101` | 67998 | MDC_ATTR_VAL_ENUM_OBS | Enum-Observed-Value |  |
`urn:iso:std:iso:11073:10101` | 67999 | MDC_ATTR_VAL_ENUM_OBS_CMPD | Compound-Enum-Observed-Value |  |
`urn:iso:std:iso:11073:10101` | 68000 | MDC_ATTR_VAL_RANGE | Set-Value-Range |  |
`urn:iso:std:iso:11073:10101` | 68001 | MDC_ATTR_VAL_STEP_WIDTH | Step-Width |  |
`urn:iso:std:iso:11073:10101` | 68002 | MDC_ATTR_VMD_STAT | Vmd-Status |  |
`urn:iso:std:iso:11073:10101` | 68003 | MDC_ATTR_VMO_LIST_SRC | Vmo-Source-List |  |
`urn:iso:std:iso:11073:10101` | 68004 | MDC_ATTR_VMO_REF | Vmo-Reference * |  |
`urn:iso:std:iso:11073:10101` | 68005 | MDC_ATTR_VMO_REF_GLB | Vmo-Global-Reference |  |
`urn:iso:std:iso:11073:10101` | 68006 | MDC_ATTR_VMS_MDS_LOCALIZN | Mds_localization |  |
`urn:iso:std:iso:11073:10101` | 68007 | MDC_ATTR_VMS_MDS_STAT | Mds-Status |  |
`urn:iso:std:iso:11073:10101` | 68008 | MDC_ATTR_VMS_MDS_TEXT_CAT | Mds-Text-Cat |  |
`urn:iso:std:iso:11073:10101` | 68012 | MDC_ATTR_AL_COND | Alert-Condition |  |
`urn:iso:std:iso:11073:10101` | 68013 | MDC_ATTR_AL_LIMIT | Limit-Specification |  |
`urn:iso:std:iso:11073:10101` | 68014 | MDC_ATTR_AL_OP_TEXT_STRING | Alert-Op-Text-String |  |
`urn:iso:std:iso:11073:10101` | 68015 | MDC_ATTR_ANAESTHETIST | Anesthetist |  |
`urn:iso:std:iso:11073:10101` | 68016 | MDC_ATTR_ARCHIVE_VERS | Version |  |
`urn:iso:std:iso:11073:10101` | 68017 | MDC_ATTR_AUTH_LEVEL | Authorization-Level |  |
`urn:iso:std:iso:11073:10101` | 68018 | MDC_ATTR_BATT_CHARGE_CYCLES | Charge-Cycles |  |
`urn:iso:std:iso:11073:10101` | 68019 | MDC_ATTR_BATT_CURR | Current |  |
`urn:iso:std:iso:11073:10101` | 68020 | MDC_ATTR_BATT_STAT | Battery-Status |  |
`urn:iso:std:iso:11073:10101` | 68021 | MDC_ATTR_BATT_VOLTAGE | Voltage |  |
`urn:iso:std:iso:11073:10101` | 68022 | MDC_ATTR_BATT_VOLTAGE_SPECN | Voltage-Specified |  |
`urn:iso:std:iso:11073:10101` | 68023 | MDC_ATTR_CAPAC_BATT_FULL | Capacity-Full-Charge |  |
`urn:iso:std:iso:11073:10101` | 68024 | MDC_ATTR_CAPAC_BATT_REMAIN | Capacity-Remaining |  |
`urn:iso:std:iso:11073:10101` | 68025 | MDC_ATTR_CAPAC_BATT_SPECN | Capacity-Specified |  |
`urn:iso:std:iso:11073:10101` | 68026 | MDC_ATTR_CIRCUM_HEAD | Patient-Head-Circumference |  |
`urn:iso:std:iso:11073:10101` | 68027 | MDC_ATTR_CLASS | Class |  |
`urn:iso:std:iso:11073:10101` | 68028 | MDC_ATTR_CODE_DIAGNOSTIC | Diagnostic-Codes |  |
`urn:iso:std:iso:11073:10101` | 68029 | MDC_ATTR_CODE_PROCEDURE | Procedure-Codes * |  |
`urn:iso:std:iso:11073:10101` | 68030 | MDC_ATTR_DESC_DIAGNOSTIC | Diagnosis-Description |  |
`urn:iso:std:iso:11073:10101` | 68031 | MDC_ATTR_DESC_PROCEDURE | Procedure-Description * |  |
`urn:iso:std:iso:11073:10101` | 68032 | MDC_ATTR_DIAGNOSTIC_INFO | Diagnostic-Info |  |
`urn:iso:std:iso:11073:10101` | 68033 | MDC_ATTR_DISCRIM_CONSTRUCT | Discriminator-Construct |  |
`urn:iso:std:iso:11073:10101` | 68034 | MDC_ATTR_ENUM_ADD_DATA | Enum-Additional-Data |  |
`urn:iso:std:iso:11073:10101` | 68035 | MDC_ATTR_EXT_OBJ_RELATION | Ext-Obj-Relations * |  |
`urn:iso:std:iso:11073:10101` | 68036 | MDC_ATTR_FINDINGS | Findings |  |
`urn:iso:std:iso:11073:10101` | 68037 | MDC_ATTR_ID_BED | Bed-Id |  |
`urn:iso:std:iso:11073:10101` | 68038 | MDC_ATTR_ID_MSMT_EXT | Metric-Id-Ext |  |
`urn:iso:std:iso:11073:10101` | 68039 | MDC_ATTR_ID_PHYSICIAN | Physician-Id |  |
`urn:iso:std:iso:11073:10101` | 68040 | MDC_ATTR_ID_PT_MOTHER | Mother-Patient-Id |  |
`urn:iso:std:iso:11073:10101` | 68041 | MDC_ATTR_ID_SESS_NOTES_ARCHIVE | Sn-Id |  |
`urn:iso:std:iso:11073:10101` | 68042 | MDC_ATTR_ID_SESS_TEST_ARCHIVE | St-Archive-Id |  |
`urn:iso:std:iso:11073:10101` | 68043 | MDC_ATTR_ID_SESS_ARCHIVE | S-Archive-Id |  |
`urn:iso:std:iso:11073:10101` | 68044 | MDC_ATTR_ID_SUBSTANCE_LABEL_STRING | Substance-Label-String |  |
`urn:iso:std:iso:11073:10101` | 68045 | MDC_ATTR_LOCATION | Location |  |
`urn:iso:std:iso:11073:10101` | 68046 | MDC_ATTR_NAME_BINDING | Name-Binding |  |
`urn:iso:std:iso:11073:10101` | 68047 | MDC_ATTR_NAME_SESS_NOTES_ARCHIVE | Sn-Name |  |
`urn:iso:std:iso:11073:10101` | 68048 | MDC_ATTR_NAME_SESS_TEST_ARCHIVE | St-Archive-Name |  |
`urn:iso:std:iso:11073:10101` | 68049 | MDC_ATTR_NAME_SESS_ARCHIVE | S-Archive-Name |  |
`urn:iso:std:iso:11073:10101` | 68050 | MDC_ATTR_OP_TEXT_STRING | Operation-Text-String |  |
`urn:iso:std:iso:11073:10101` | 68051 | MDC_ATTR_PHYSICIAN_ADMIT | Admitting-Physician |  |
`urn:iso:std:iso:11073:10101` | 68052 | MDC_ATTR_PHYSICIAN_ATTEND | Attending-Physician |  |
`urn:iso:std:iso:11073:10101` | 68053 | MDC_ATTR_PROC_HIST | Processing-History |  |
`urn:iso:std:iso:11073:10101` | 68054 | MDC_ATTR_PROCEDURE_DATE | Date-Of-Procedure |  |
`urn:iso:std:iso:11073:10101` | 68055 | MDC_ATTR_PROTECTION | Protection |  |
`urn:iso:std:iso:11073:10101` | 68056 | MDC_ATTR_PT_AGE | Patient-Age |  |
`urn:iso:std:iso:11073:10101` | 68057 | MDC_ATTR_PT_AGE_GEST | Gestational-Age |  |
`urn:iso:std:iso:11073:10101` | 68058 | MDC_ATTR_PT_BIRTH_LENGTH | Patient-Birth-Length |  |
`urn:iso:std:iso:11073:10101` | 68059 | MDC_ATTR_PT_BIRTH_WEIGHT | Patient-Birth-Weight |  |
`urn:iso:std:iso:11073:10101` | 68060 | MDC_ATTR_PT_HEIGHT | Patient-Height |  |
`urn:iso:std:iso:11073:10101` | 68061 | MDC_ATTR_PT_NAME_MOTHER | Mother-Name |  |
`urn:iso:std:iso:11073:10101` | 68062 | MDC_ATTR_PT_RACE | Race |  |
`urn:iso:std:iso:11073:10101` | 68063 | MDC_ATTR_PT_WEIGHT | Patient-Weight |  |
`urn:iso:std:iso:11073:10101` | 68064 | MDC_ATTR_SESS_NOTES_ARCHIVE_COMMENTS | Sn-Comments |  |
`urn:iso:std:iso:11073:10101` | 68065 | MDC_ATTR_SESS_TEST_ARCHIVE_COMMENTS | St-Archive-Comments |  |
`urn:iso:std:iso:11073:10101` | 68066 | MDC_ATTR_SESS_ARCHIVE_COMMENTS | S-Archive-Comments |  |
`urn:iso:std:iso:11073:10101` | 68067 | MDC_ATTR_NAME_STUDY | Study-Name |  |
`urn:iso:std:iso:11073:10101` | 68068 | MDC_ATTR_SURGEON | Surgeon |  |
`urn:iso:std:iso:11073:10101` | 68070 | MDC_ATTR_TEMP_BATT | Battery-Temperature |  |
`urn:iso:std:iso:11073:10101` | 68071 | MDC_ATTR_TIME_PD_AVG | Averaging-Period |  |
`urn:iso:std:iso:11073:10101` | 68072 | MDC_ATTR_TIME_REL_HI_RES | Specifies the high-res relative time value for system or device clock and derived objects (default 1 μs resolution counter having an arbitrary start time and value). |  |
`urn:iso:std:iso:11073:10101` | 68073 | MDC_ATTR_TIME_STAMP_REL_HI_RES | Hi-Res relative time stamp value for observations and derived objects. |  |
`urn:iso:std:iso:11073:10101` | 68074 | MDC_ATTR_TIME_START | Start-Time * |  |
`urn:iso:std:iso:11073:10101` | 68075 | MDC_ATTR_TIME_STOP | Stop-Time * |  |
`urn:iso:std:iso:11073:10101` | 68076 | MDC_ATTR_TOG_LABELS_STRING | Toggle-Label-Strings |  |
`urn:iso:std:iso:11073:10101` | 68078 | MDC_ATTR_ID_SUBSTANCE | Substance |  |
`urn:iso:std:iso:11073:10101` | 68079 | MDC_ATTR_NAME_SYS | System-Name |  |
`urn:iso:std:iso:11073:10101` | 68080 | MDC_ATTR_PHYSICIAN_NAME | Name |  |
`urn:iso:std:iso:11073:10101` | 68081 | MDC_ATTR_PHYSICIAN_NAME_FAMILY | Family-Name |  |
`urn:iso:std:iso:11073:10101` | 68082 | MDC_ATTR_PHYSICIAN_NAME_GIVEN | Given-Name |  |
`urn:iso:std:iso:11073:10101` | 68083 | MDC_ATTR_PHYSICIAN_NAME_MIDDLE | Middle-Name |  |
`urn:iso:std:iso:11073:10101` | 68084 | MDC_ATTR_PHYSICIAN_NAME_TITLE | Title-Name |  |
`urn:iso:std:iso:11073:10101` | 68085 | MDC_ATTR_SCO_HELP_TEXT_STRING | Sco-Help-Text-String |  |
`urn:iso:std:iso:11073:10101` | 68086 | MDC_ATTR_SITE_LIST_BODY_EXT | Body-Site-List-Ext |  |
`urn:iso:std:iso:11073:10101` | 68087 | MDC_ATTR_SITE_LIST_MSMT_EXT | Msmt-Site-List-Ext |  |
`urn:iso:std:iso:11073:10101` | 68088 | MDC_ATTR_MIB_SYS | Mib-Sys |  |
`urn:iso:std:iso:11073:10101` | 68089 | MDC_ATTR_MIB_IP | Mib-IP |  |
`urn:iso:std:iso:11073:10101` | 68090 | MDC_ATTR_MIB_ICMP | Mib-ICMP |  |
`urn:iso:std:iso:11073:10101` | 68091 | MDC_ATTR_MIB_IF | Mib-If |  |
`urn:iso:std:iso:11073:10101` | 68092 | MDC_ATTR_MIB_AT | Mib-At |  |
`urn:iso:std:iso:11073:10101` | 68093 | MDC_ATTR_MIB_UDP | Mib-UDP |  |
`urn:iso:std:iso:11073:10101` | 68094 | MDC_ATTR_SCAN_CFG_LIMIT | Scan-Config-Limit |  |
`urn:iso:std:iso:11073:10101` | 68096 | MDC_ATTR_MSMT_PRINCIPLE | Measurement-Principle |  |
`urn:iso:std:iso:11073:10101` | 68097 | MDC_ATTR_ENUM_RANGE_MSMT | Enum-Measure-Range |  |
`urn:iso:std:iso:11073:10101` | 68100 | MDC_ATTR_EVENT_LOG_ENTRY_LIST | Event-Log-Entry-List |  |
`urn:iso:std:iso:11073:10101` | 68101 | MDC_ATTR_STRING_CURR | Current-String |  |
`urn:iso:std:iso:11073:10101` | 68103 | MDC_ATTR_SET_STRING_SPEC | Set-String-Spec |  |
`urn:iso:std:iso:11073:10101` | 68104 | MDC_ATTR_ENUM_RANGE_MSMT_BIT_STRING | Enum-Measure-Range-Bit-String |  |
`urn:iso:std:iso:11073:10101` | 68105 | MDC_ATTR_ID_PRINTER_NAME | Printer-Name |  |
`urn:iso:std:iso:11073:10101` | 68106 | MDC_ATTR_PRINTER_CMD_LANG | Printer-Cmd-Lang |  |
`urn:iso:std:iso:11073:10101` | 68107 | MDC_ATTR_PRINTER_STAT | Printer-Status |  |
`urn:iso:std:iso:11073:10101` | 68108 | MDC_ATTR_PRINTER_STAT_STRING | Printer-Status_String |  |
`urn:iso:std:iso:11073:10101` | 68109 | MDC_ATTR_PAPER_SIZE | Printer-Paper_size |  |
`urn:iso:std:iso:11073:10101` | 68110 | MDC_ATTR_PRINT_MARGINS | Printer-Margins |  |
`urn:iso:std:iso:11073:10101` | 68111 | MDC_ATTR_PRINTER_GRPH_RES_STD | Printer-Graphics-Resolution |  |
`urn:iso:std:iso:11073:10101` | 68112 | MDC_ATTR_PRINTER_GRPH_RES_COLOR | Printer-Graphics_Resolution-Color |  |
`urn:iso:std:iso:11073:10101` | 68113 | MDC_ATTR_PRINTER_COLOR_SUP | Printer-Color-Support |  |
`urn:iso:std:iso:11073:10101` | 68114 | MDC_ATTR_PRINTER_DUPLX_SUP | Printer-Duplex-Support |  |
`urn:iso:std:iso:11073:10101` | 68115 | MDC_ATTR_PRINTER_LOC_LANG_SUP | Printer-Language-Support |  |
`urn:iso:std:iso:11073:10101` | 68116 | MDC_ATTR_PRINTER_ACC_PCOL | Printer-Color |  |
`urn:iso:std:iso:11073:10101` | 68117 | MDC_ATTR_PRINTER_TFTP_ADDR | Printer-TFTP-Address |  |
`urn:iso:std:iso:11073:10101` | 68118 | MDC_ATTR_SA_MARKER_LIST_I16 | Sa-Marker-List |  |
`urn:iso:std:iso:11073:10101` | 68119 | MDC_ATTR_DELAY_TIME_MAX | Max-Delay-Time |  |
`urn:iso:std:iso:11073:10101` | 68120 | MDC_ATTR_PDMO_CAPAB | Patient Demographics Management Capability |  |
`urn:iso:std:iso:11073:10101` | 68121 | MDC_ATTR_PDMO_IMPL_VERS | Patient Demographics Management Implementation Version |  |
`urn:iso:std:iso:11073:10101` | 68122 | MDC_ATTR_SYS_ADT_ST |  |  |
`urn:iso:std:iso:11073:10101` | 68123 | MDC_ATTR_PT_DEMOG_REF_LIST | Patient Demographics Reference List |  |
`urn:iso:std:iso:11073:10101` | 68124 | MDC_ATTR_PT_DEMOG_ST_SYNCH | Patient Demographics |  |
`urn:iso:std:iso:11073:10101` | 68125 | MDC_ATTR_PT_DEMOG_DATA_LIST | Patient Demographics Data List |  |
`urn:iso:std:iso:11073:10101` | 68126 | MDC_ATTR_PT_PACED_MODE | Patient Demographics Paced Mode |  |
`urn:iso:std:iso:11073:10101` | 68127 | MDC_ATTR_EVENT_LOG_INFO | Event-Log-Info |  |
`urn:iso:std:iso:11073:10101` | 68128 | MDC_ATTR_EVENT_LOG_CHANGE_COUNT | Log-Change-Count |  |
`urn:iso:std:iso:11073:10101` | 68129 | MDC_ATTR_CC_CAPAB | Capability |  |
`urn:iso:std:iso:11073:10101` | 68130 | MDC_ATTR_CC_TYPE | CC-Type |  |
`urn:iso:std:iso:11073:10101` | 68131 | MDC_ATTR_CC_NUM_DIFS | Number-Of-Difs |  |
`urn:iso:std:iso:11073:10101` | 68132 | MDC_ATTR_CC_THIS_DIF_INDEX | This-Connection-Dif-Index |  |
`urn:iso:std:iso:11073:10101` | 68133 | MDC_ATTR_CC_EXT_MNG_PROT | Cc-Ext-Mgmt-Proto-Id |  |
`urn:iso:std:iso:11073:10101` | 68134 | MDC_ATTR_MIB_EXT_OID | Mib-External |  |
`urn:iso:std:iso:11073:10101` | 68136 | MDC_ATTR_LOCALE | Locale |  |
`urn:iso:std:iso:11073:10101` | 68137 | MDC_ATTR_PT_LBM | Patient-Lean-Body-Mass |  |
`urn:iso:std:iso:11073:10101` | 68138 | MDC_ATTR_OP_TEXT_STRING_DYN | Operation-Text-String-Dynamic |  |
`urn:iso:std:iso:11073:10101` | 68139 | MDC_ATTR_SA_MARKER_LIST_I8 | Sa-Marker-List |  |
`urn:iso:std:iso:11073:10101` | 68140 | MDC_ATTR_SA_MARKER_LIST_I32 | Sa-Marker-List |  |
`urn:iso:std:iso:11073:10101` | 68141 | MDC_ATTR_DSA_MARKER_LIST | Dsa-Marker-List |  |
`urn:iso:std:iso:11073:10101` | 68142 | MDC_ATTR_CHAN_NUM_LOGICAL | Logical-Channel-Number |  |
`urn:iso:std:iso:11073:10101` | 68143 | MDC_ATTR_TIME_SUPPORT | Time Capabilities |  |
`urn:iso:std:iso:11073:10101` | 68144 | MDC_ATTR_DATE_TIME_STATUS | Time Status |  |
`urn:iso:std:iso:11073:10101` | 68145 | MDC_ATTR_TIME_ABS_ISO | Date and Time in ISO Format |  |
`urn:iso:std:iso:11073:10101` | 68146 | MDC_ATTR_TIME_STAMP_LIST_EXT | List of External (different format) Time Stamps |  |
`urn:iso:std:iso:11073:10101` | 68147 | MDC_ATTR_TIME_ABS_REL_SYNC | Attribute for synchronization between Abs and Rel Times |  |
`urn:iso:std:iso:11073:10101` | 68148 | MDC_ATTR_TIME_ZONE | Time Zone |  |
`urn:iso:std:iso:11073:10101` | 68149 | MDC_ATTR_TIME_DAYLIGHT_SAVINGS_TRANS | Info for daylight savings time transition |  |
`urn:iso:std:iso:11073:10101` | 68150 | MDC_ATTR_CUM_LEAP_SECONDS | Cumulative leap seconds |  |
`urn:iso:std:iso:11073:10101` | 68151 | MDC_ATTR_NEXT_LEAP_SECOND | Time stamp for next leap second |  |
`urn:iso:std:iso:11073:10101` | 68152 | MDC_ATTR_REPORTING_DELAY_AVG | Average-Reporting-Delay |  |
`urn:iso:std:iso:11073:10101` | 68153 | MDC_ATTR_SAMPLE_TIME_SYNC | Sample-Time-Sync |  |
`urn:iso:std:iso:11073:10101` | 68154 | MDC_ATTR_SAMPLE_TIME_SYNC_HIRES | HiRes-Sample-Time-Sync |  |
`urn:iso:std:iso:11073:10101` | 68155 | MDC_ATTR_CMPLX_INFO | Cmplx-Metric-Info |  |
`urn:iso:std:iso:11073:10101` | 68156 | MDC_ATTR_CMPLX_VAL_OBS | Cmplx-Observed-Value |  |
`urn:iso:std:iso:11073:10101` | 68157 | MDC_ATTR_CMPLX_DYN_ATTR | Cmplx-Dyn-Attr |  |
`urn:iso:std:iso:11073:10101` | 68158 | MDC_ATTR_CMPLX_STATIC_ATTR | Cmplx-Static-Attr |  |
`urn:iso:std:iso:11073:10101` | 68159 | MDC_ATTR_CMPLX_RECURSION_DEPTH | Cmplx-Recursion-Depth |  |
`urn:iso:std:iso:11073:10101` | 68160 | MDC_ATTR_RANGE_CURR | Current-Range |  |
`urn:iso:std:iso:11073:10101` | 68161 | MDC_ATTR_RANGE_OP_TEXT_STRING | Range-Op-Text |  |
`urn:iso:std:iso:11073:10101` | 68609 | MDC_ACT_ACC_SETTINGS |  |  |
`urn:iso:std:iso:11073:10101` | 68610 | MDC_ACT_ADMIT_PT | Admit-Patient |  |
`urn:iso:std:iso:11073:10101` | 68611 | MDC_ACT_CLR_LOG | Clear-Log |  |
`urn:iso:std:iso:11073:10101` | 68612 | MDC_ACT_DISCH_PT | Discharge-Patient |  |
`urn:iso:std:iso:11073:10101` | 68613 | MDC_ACT_GET_CTXT_HELP | Get-Ctxt-Help |  |
`urn:iso:std:iso:11073:10101` | 68614 | MDC_ACT_PRE_ADMIT_PT | Pre-Admit-Patient |  |
`urn:iso:std:iso:11073:10101` | 68615 | MDC_ACT_REFR_CTXT | Refresh-Context |  |
`urn:iso:std:iso:11073:10101` | 68616 | MDC_ACT_REFR_EPI_DATA | Refresh-Episodic-Data |  |
`urn:iso:std:iso:11073:10101` | 68617 | MDC_ACT_REFR_OP_ATTR | Refresh-Operation-Attributes |  |
`urn:iso:std:iso:11073:10101` | 68618 | MDC_ACT_REFR_OP_CTXT | Refresh-Operation-Context |  |
`urn:iso:std:iso:11073:10101` | 68619 | MDC_ACT_SCO_OP_INVOK | Operation-Invoke |  |
`urn:iso:std:iso:11073:10101` | 68620 | MDC_ACT_SEG_CLR | Clear-Segments |  |
`urn:iso:std:iso:11073:10101` | 68621 | MDC_ACT_SEG_GET | Get-Segments |  |
`urn:iso:std:iso:11073:10101` | 68622 | MDC_ACT_SEG_GET_INFO | Get-Segment-Info |  |
`urn:iso:std:iso:11073:10101` | 68623 | MDC_ACT_SET_MDS_STATE | Mds-Set-Status |  |
`urn:iso:std:iso:11073:10101` | 68624 | MDC_ACT_UPLD_TEXT_CTLG |  |  |
`urn:iso:std:iso:11073:10101` | 68625 | MDC_ACT_PDMO_TXN | Patient Demographics Management Object |  |
`urn:iso:std:iso:11073:10101` | 68626 | MDC_ACT_PDMO_PROMPT | Patient Demographics Management Object Prompt |  |
`urn:iso:std:iso:11073:10101` | 68627 | MDC_ACT_PDMO_MSG_BOX | Patient Demographics Management Object Message Box |  |
`urn:iso:std:iso:11073:10101` | 68628 | MDC_ACT_GET_EVENT_LOG_ENTRIES | Get-Event-Log-Entries |  |
`urn:iso:std:iso:11073:10101` | 68629 | MDC_ACT_GET_MIB_DATA | Get-Mdib-Data |  |
`urn:iso:std:iso:11073:10101` | 68630 | MDC_ACT_POLL_MDIB_DATA | Poll-Mdib-Data |  |
`urn:iso:std:iso:11073:10101` | 68631 | MDC_ACT_SET_TIME | Set-Time |  |
`urn:iso:std:iso:11073:10101` | 68632 | MDC_ACT_SET_TIME_ZONE | Set-Time-Zone |  |
`urn:iso:std:iso:11073:10101` | 68633 | MDC_ACT_SET_LEAP_SECONDS | Set-Leap-Seconds |  |
`urn:iso:std:iso:11073:10101` | 68634 | MDC_ACT_SET_TIME_ISO | Set-ISO-Time |  |
`urn:iso:std:iso:11073:10101` | 68864 | MDC_NOTI_NOS | Non-Specific |  |
`urn:iso:std:iso:11073:10101` | 68865 | MDC_NOTI_AL_STAT_SCAN_RPT | Alert-Scan-Report |  |
`urn:iso:std:iso:11073:10101` | 68866 | MDC_NOTI_ATTR_UPDT | Attribute-Update |  |
`urn:iso:std:iso:11073:10101` | 68867 | MDC_NOTI_BUF_SCAN_RPT | Buf-Scan-Report |  |
`urn:iso:std:iso:11073:10101` | 68868 | MDC_NOTI_FAST_BUF_SCAN_RPT | Fast-Buf-Scan-Report |  |
`urn:iso:std:iso:11073:10101` | 68869 | MDC_NOTI_MDS_ATTR_UPDT | Mds-Attribute-Update |  |
`urn:iso:std:iso:11073:10101` | 68870 | MDC_NOTI_MDS_CREAT | Mds-Create-Notification |  |
`urn:iso:std:iso:11073:10101` | 68871 | MDC_NOTI_OBJ_ACTIV | Object-Activated-Notification |  |
`urn:iso:std:iso:11073:10101` | 68872 | MDC_NOTI_OBJ_CREAT | Object-Create-Notification |  |
`urn:iso:std:iso:11073:10101` | 68873 | MDC_NOTI_OBJ_DEACT | Object-Delactivated-Notification |  |
`urn:iso:std:iso:11073:10101` | 68874 | MDC_NOTI_OBJ_DEL | Object-Delete-Notification |  |
`urn:iso:std:iso:11073:10101` | 68875 | MDC_NOTI_OP_ATTR_UPDT | Oper-Attribute-Update |  |
`urn:iso:std:iso:11073:10101` | 68876 | MDC_NOTI_OP_CREAT | Oper-Create-Notification |  |
`urn:iso:std:iso:11073:10101` | 68877 | MDC_NOTI_OP_DEL | Oper-Delete-Notification |  |
`urn:iso:std:iso:11073:10101` | 68878 | MDC_NOTI_PT_DEMOG_MOD | Patient-Demographics-Modified |  |
`urn:iso:std:iso:11073:10101` | 68879 | MDC_NOTI_PT_DEMOG_ST_MOD | Patient-Demographics-State-Change |  |
`urn:iso:std:iso:11073:10101` | 68880 | MDC_NOTI_SCAN_ATTR_UPDT | Scan-Attribute-Update |  |
`urn:iso:std:iso:11073:10101` | 68881 | MDC_NOTI_SCO_ATTR_UPDT | Sco-Attribute-Update |  |
`urn:iso:std:iso:11073:10101` | 68882 | MDC_NOTI_SCO_OP_INVOK_ERR | Sco-Operation-Invoke-Error |  |
`urn:iso:std:iso:11073:10101` | 68883 | MDC_NOTI_SCO_OP_REQ | Sco-Operating-Request |  |
`urn:iso:std:iso:11073:10101` | 68884 | MDC_NOTI_SCO_PROMPT | Sco-Prompt |  |
`urn:iso:std:iso:11073:10101` | 68885 | MDC_NOTI_SYS_ERR | System-Error |  |
`urn:iso:std:iso:11073:10101` | 68886 | MDC_NOTI_UNBUF_SCAN_RPT | Unbuf-Scan-Report |  |
`urn:iso:std:iso:11073:10101` | 68887 | MDC_NOTI_CONN_INDIC | Connection-Indication |  |
`urn:iso:std:iso:11073:10101` | 68888 | MDC_NOTI_PRINTER_PROMPT | Printer-Prompt |  |
`urn:iso:std:iso:11073:10101` | 68889 | MDC_NOTI_PDMO | Patient Demographics Management Object Change |  |
`urn:iso:std:iso:11073:10101` | 68890 | MDC_NOTI_SCO_ST | Sco-Status |  |
`urn:iso:std:iso:11073:10101` | 68891 | MDC_NOTI_DATE_TIME_CHANGED | Date-Time Changed |  |
`urn:iso:std:iso:11073:10101` | 69632 | MDC_DEV | Generic device, may be used as placeholder. |  |
`urn:iso:std:iso:11073:10101` | 69633 | MDC_DEV_MDS | Definition for base term 1::4096 MDC_DEV is: Generic device, may be used as placeholder. |  |
`urn:iso:std:iso:11073:10101` | 69634 | MDC_DEV_VMD | Definition for base term 1::4096 MDC_DEV is: Generic device, may be used as placeholder. |  |
`urn:iso:std:iso:11073:10101` | 69635 | MDC_DEV_CHAN | Definition for base term 1::4096 MDC_DEV is: Generic device, may be used as placeholder. |  |
`urn:iso:std:iso:11073:10101` | 69636 | MDC_DEV_ANALY | Instrument that analyzes acquired patient information. |  |
`urn:iso:std:iso:11073:10101` | 69637 | MDC_DEV_ANALY_MDS | Definition for base term 1::4100 MDC_DEV_ANALY is: Instrument that analyzes acquired patient information. |  |
`urn:iso:std:iso:11073:10101` | 69638 | MDC_DEV_ANALY_VMD | Definition for base term 1::4100 MDC_DEV_ANALY is: Instrument that analyzes acquired patient information. |  |
`urn:iso:std:iso:11073:10101` | 69639 | MDC_DEV_ANALY_CHAN | Definition for base term 1::4100 MDC_DEV_ANALY is: Instrument that analyzes acquired patient information. |  |
`urn:iso:std:iso:11073:10101` | 69640 | MDC_DEV_ANALY_SAT_O2 | Instrument that derives the % of arterial O2 and pulse rate parameters (blood flow). |  |
`urn:iso:std:iso:11073:10101` | 69641 | MDC_DEV_ANALY_SAT_O2_MDS | Definition for base term 1::4104 MDC_DEV_ANALY_SAT_O2 is: Instrument that derives the % of arterial O2 and pulse rate parameters (blood flow). |  |
`urn:iso:std:iso:11073:10101` | 69642 | MDC_DEV_ANALY_SAT_O2_VMD | Definition for base term 1::4104 MDC_DEV_ANALY_SAT_O2 is: Instrument that derives the % of arterial O2 and pulse rate parameters (blood flow). |  |
`urn:iso:std:iso:11073:10101` | 69643 | MDC_DEV_ANALY_SAT_O2_CHAN | Definition for base term 1::4104 MDC_DEV_ANALY_SAT_O2 is: Instrument that derives the % of arterial O2 and pulse rate parameters (blood flow). |  |
`urn:iso:std:iso:11073:10101` | 69644 | MDC_DEV_ANALY_CONC_GAS_IDENT | Instrument for the direct measurement of the concentration of airway chemicals, e.g., CO2, O2, anesthetic agent. |  |
`urn:iso:std:iso:11073:10101` | 69645 | MDC_DEV_ANALY_CONC_GAS_IDENT_MDS | Definition for base term 1::4108 MDC_DEV_ANALY_CONC_GAS_IDENT is: Instrument for the direct measurement of the concentration of airway chemicals, e.g., CO2, O2, anesthetic agent. |  |
`urn:iso:std:iso:11073:10101` | 69646 | MDC_DEV_ANALY_CONC_GAS_IDENT_VMD | Definition for base term 1::4108 MDC_DEV_ANALY_CONC_GAS_IDENT is: Instrument for the direct measurement of the concentration of airway chemicals, e.g., CO2, O2, anesthetic agent. |  |
`urn:iso:std:iso:11073:10101` | 69647 | MDC_DEV_ANALY_CONC_GAS_IDENT_CHAN | Definition for base term 1::4108 MDC_DEV_ANALY_CONC_GAS_IDENT is: Instrument for the direct measurement of the concentration of airway chemicals, e.g., CO2, O2, anesthetic agent. |  |
`urn:iso:std:iso:11073:10101` | 69648 | MDC_DEV_ANALY_CONC_GAS_MULTI_PARAM | Instrument that derives airway gas parameters, e.g., EtCO2, iCO2, iO2. |  |
`urn:iso:std:iso:11073:10101` | 69649 | MDC_DEV_ANALY_CONC_GAS_MULTI_PARAM_MDS | Definition for base term 1::4112 MDC_DEV_ANALY_CONC_GAS_MULTI_PARAM is: Instrument that derives airway gas parameters, e.g., EtCO2, iCO2, iO2. |  |
`urn:iso:std:iso:11073:10101` | 69650 | MDC_DEV_ANALY_CONC_GAS_MULTI_PARAM_VMD | Definition for base term 1::4112 MDC_DEV_ANALY_CONC_GAS_MULTI_PARAM is: Instrument that derives airway gas parameters, e.g., EtCO2, iCO2, iO2. |  |
`urn:iso:std:iso:11073:10101` | 69651 | MDC_DEV_ANALY_CONC_GAS_MULTI_PARAM_CHAN | Definition for base term 1::4112 MDC_DEV_ANALY_CONC_GAS_MULTI_PARAM is: Instrument that derives airway gas parameters, e.g., EtCO2, iCO2, iO2. |  |
`urn:iso:std:iso:11073:10101` | 69652 | MDC_DEV_ANALY_URINE_CHEM | Instrument that derives urine chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69653 | MDC_DEV_ANALY_URINE_CHEM_MDS | Definition for base term 1::4116 MDC_DEV_ANALY_URINE_CHEM is: Instrument that derives urine chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69654 | MDC_DEV_ANALY_URINE_CHEM_VMD | Definition for base term 1::4116 MDC_DEV_ANALY_URINE_CHEM is: Instrument that derives urine chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69655 | MDC_DEV_ANALY_URINE_CHEM_CHAN | Definition for base term 1::4116 MDC_DEV_ANALY_URINE_CHEM is: Instrument that derives urine chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69656 | MDC_DEV_ANALY_ELEC_POTL_BRAIN | Instrument that derives brain activity parameters. |  |
`urn:iso:std:iso:11073:10101` | 69657 | MDC_DEV_ANALY_ELEC_POTL_BRAIN_MDS | Definition for base term 1::4120 MDC_DEV_ANALY_ELEC_POTL_BRAIN is: Instrument that derives brain activity parameters. |  |
`urn:iso:std:iso:11073:10101` | 69658 | MDC_DEV_ANALY_ELEC_POTL_BRAIN_VMD | Definition for base term 1::4120 MDC_DEV_ANALY_ELEC_POTL_BRAIN is: Instrument that derives brain activity parameters. |  |
`urn:iso:std:iso:11073:10101` | 69659 | MDC_DEV_ANALY_ELEC_POTL_BRAIN_CHAN | Definition for base term 1::4120 MDC_DEV_ANALY_ELEC_POTL_BRAIN is: Instrument that derives brain activity parameters. |  |
`urn:iso:std:iso:11073:10101` | 69660 | MDC_DEV_ANALY_ELEC_POTL_HEART_ACTIV | Instrument that derives heart/haemo activity parameters, e.g., cardiotach, arrhythmia monitor, ST analyzer, R-R. |  |
`urn:iso:std:iso:11073:10101` | 69661 | MDC_DEV_ANALY_ELEC_POTL_HEART_ACTIV_MDS | Definition for base term 1::4124 MDC_DEV_ANALY_ELEC_POTL_HEART_ACTIV is: Instrument that derives heart/haemo activity parameters, e.g., cardiotach, arrhythmia monitor, ST analyzer, R-R. |  |
`urn:iso:std:iso:11073:10101` | 69662 | MDC_DEV_ANALY_ELEC_POTL_HEART_ACTIV_VMD | Definition for base term 1::4124 MDC_DEV_ANALY_ELEC_POTL_HEART_ACTIV is: Instrument that derives heart/haemo activity parameters, e.g., cardiotach, arrhythmia monitor, ST analyzer, R-R. |  |
`urn:iso:std:iso:11073:10101` | 69663 | MDC_DEV_ANALY_ELEC_POTL_HEART_ACTIV_CHAN | Definition for base term 1::4124 MDC_DEV_ANALY_ELEC_POTL_HEART_ACTIV is: Instrument that derives heart/haemo activity parameters, e.g., cardiotach, arrhythmia monitor, ST analyzer, R-R. |  |
`urn:iso:std:iso:11073:10101` | 69664 | MDC_DEV_ANALY_FLOW_AWAY | Instrument that derives airway flow parameters. |  |
`urn:iso:std:iso:11073:10101` | 69665 | MDC_DEV_ANALY_FLOW_AWAY_MDS | Definition for base term 1::4128 MDC_DEV_ANALY_FLOW_AWAY is: Instrument that derives airway flow parameters. |  |
`urn:iso:std:iso:11073:10101` | 69666 | MDC_DEV_ANALY_FLOW_AWAY_VMD | Definition for base term 1::4128 MDC_DEV_ANALY_FLOW_AWAY is: Instrument that derives airway flow parameters. |  |
`urn:iso:std:iso:11073:10101` | 69667 | MDC_DEV_ANALY_FLOW_AWAY_CHAN | Definition for base term 1::4128 MDC_DEV_ANALY_FLOW_AWAY is: Instrument that derives airway flow parameters. |  |
`urn:iso:std:iso:11073:10101` | 69668 | MDC_DEV_ANALY_CARD_OUTPUT | Instrument that derives heart output from direct measurement of blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69669 | MDC_DEV_ANALY_CARD_OUTPUT_MDS | Definition for base term 1::4132 MDC_DEV_ANALY_CARD_OUTPUT is: Instrument that derives heart output from direct measurement of blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69670 | MDC_DEV_ANALY_CARD_OUTPUT_VMD | Definition for base term 1::4132 MDC_DEV_ANALY_CARD_OUTPUT is: Instrument that derives heart output from direct measurement of blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69671 | MDC_DEV_ANALY_CARD_OUTPUT_CHAN | Definition for base term 1::4132 MDC_DEV_ANALY_CARD_OUTPUT is: Instrument that derives heart output from direct measurement of blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69672 | MDC_DEV_ANALY_FLOW_LUNG | Instrument that derives lung flow parameters. |  |
`urn:iso:std:iso:11073:10101` | 69673 | MDC_DEV_ANALY_FLOW_LUNG_MDS | Definition for base term 1::4136 MDC_DEV_ANALY_FLOW_LUNG is: Instrument that derives lung flow parameters. |  |
`urn:iso:std:iso:11073:10101` | 69674 | MDC_DEV_ANALY_FLOW_LUNG_VMD | Definition for base term 1::4136 MDC_DEV_ANALY_FLOW_LUNG is: Instrument that derives lung flow parameters. |  |
`urn:iso:std:iso:11073:10101` | 69675 | MDC_DEV_ANALY_FLOW_LUNG_CHAN | Definition for base term 1::4136 MDC_DEV_ANALY_FLOW_LUNG is: Instrument that derives lung flow parameters. |  |
`urn:iso:std:iso:11073:10101` | 69676 | MDC_DEV_ANALY_FLOW_URINE | Instrument that derives urine flow rate. |  |
`urn:iso:std:iso:11073:10101` | 69677 | MDC_DEV_ANALY_FLOW_URINE_MDS | Definition for base term 1::4140 MDC_DEV_ANALY_FLOW_URINE is: Instrument that derives urine flow rate. |  |
`urn:iso:std:iso:11073:10101` | 69678 | MDC_DEV_ANALY_FLOW_URINE_VMD | Definition for base term 1::4140 MDC_DEV_ANALY_FLOW_URINE is: Instrument that derives urine flow rate. |  |
`urn:iso:std:iso:11073:10101` | 69679 | MDC_DEV_ANALY_FLOW_URINE_CHAN | Definition for base term 1::4140 MDC_DEV_ANALY_FLOW_URINE is: Instrument that derives urine flow rate. |  |
`urn:iso:std:iso:11073:10101` | 69680 | MDC_DEV_ANALY_AWAY_MULTI_PARAM | Instrument for analysis and derivation of airway parameters. |  |
`urn:iso:std:iso:11073:10101` | 69681 | MDC_DEV_ANALY_AWAY_MULTI_PARAM_MDS | Definition for base term 1::4144 MDC_DEV_ANALY_AWAY_MULTI_PARAM is: Instrument for analysis and derivation of airway parameters. |  |
`urn:iso:std:iso:11073:10101` | 69682 | MDC_DEV_ANALY_AWAY_MULTI_PARAM_VMD | Definition for base term 1::4144 MDC_DEV_ANALY_AWAY_MULTI_PARAM is: Instrument for analysis and derivation of airway parameters. |  |
`urn:iso:std:iso:11073:10101` | 69683 | MDC_DEV_ANALY_AWAY_MULTI_PARAM_CHAN | Definition for base term 1::4144 MDC_DEV_ANALY_AWAY_MULTI_PARAM is: Instrument for analysis and derivation of airway parameters. |  |
`urn:iso:std:iso:11073:10101` | 69684 | MDC_DEV_ANALY_BLD_CHEM_MULTI_PARAM | Instrument for analysis and derivation of blood chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69685 | MDC_DEV_ANALY_BLD_CHEM_MULTI_PARAM_MDS | Definition for base term 1::4148 MDC_DEV_ANALY_BLD_CHEM_MULTI_PARAM is: Instrument for analysis and derivation of blood chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69686 | MDC_DEV_ANALY_BLD_CHEM_MULTI_PARAM_VMD | Definition for base term 1::4148 MDC_DEV_ANALY_BLD_CHEM_MULTI_PARAM is: Instrument for analysis and derivation of blood chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69687 | MDC_DEV_ANALY_BLD_CHEM_MULTI_PARAM_CHAN | Definition for base term 1::4148 MDC_DEV_ANALY_BLD_CHEM_MULTI_PARAM is: Instrument for analysis and derivation of blood chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69688 | MDC_DEV_ANALY_LUNG | Instrument for analysis and derivation of lung function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69689 | MDC_DEV_ANALY_LUNG_MDS | Definition for base term 1::4152 MDC_DEV_ANALY_LUNG is: Instrument for analysis and derivation of lung function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69690 | MDC_DEV_ANALY_LUNG_VMD | Definition for base term 1::4152 MDC_DEV_ANALY_LUNG is: Instrument for analysis and derivation of lung function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69691 | MDC_DEV_ANALY_LUNG_CHAN | Definition for base term 1::4152 MDC_DEV_ANALY_LUNG is: Instrument for analysis and derivation of lung function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69692 | MDC_DEV_ANALY_MUSCL | Instrument for analysis and derivation of muscle parameters. |  |
`urn:iso:std:iso:11073:10101` | 69693 | MDC_DEV_ANALY_MUSCL_MDS | Definition for base term 1::4156 MDC_DEV_ANALY_MUSCL is: Instrument for analysis and derivation of muscle parameters. |  |
`urn:iso:std:iso:11073:10101` | 69694 | MDC_DEV_ANALY_MUSCL_VMD | Definition for base term 1::4156 MDC_DEV_ANALY_MUSCL is: Instrument for analysis and derivation of muscle parameters. |  |
`urn:iso:std:iso:11073:10101` | 69695 | MDC_DEV_ANALY_MUSCL_CHAN | Definition for base term 1::4156 MDC_DEV_ANALY_MUSCL is: Instrument for analysis and derivation of muscle parameters. |  |
`urn:iso:std:iso:11073:10101` | 69696 | MDC_DEV_ANALY_PT_PHYSIO | Instrument that analyses and derives data from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69697 | MDC_DEV_ANALY_PT_PHYSIO_MDS | Definition for base term 1::4160 MDC_DEV_ANALY_PT_PHYSIO is: Instrument that analyses and derives data from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69698 | MDC_DEV_ANALY_PT_PHYSIO_VMD | Definition for base term 1::4160 MDC_DEV_ANALY_PT_PHYSIO is: Instrument that analyses and derives data from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69699 | MDC_DEV_ANALY_PT_PHYSIO_CHAN | Definition for base term 1::4160 MDC_DEV_ANALY_PT_PHYSIO is: Instrument that analyses and derives data from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69700 | MDC_DEV_ANALY_SKIN_MULTI_PARAM | Instrument for analysis and derivation of skin-related parameters. |  |
`urn:iso:std:iso:11073:10101` | 69701 | MDC_DEV_ANALY_SKIN_MULTI_PARAM_MDS | Definition for base term 1::4164 MDC_DEV_ANALY_SKIN_MULTI_PARAM is: Instrument for analysis and derivation of skin-related parameters. |  |
`urn:iso:std:iso:11073:10101` | 69702 | MDC_DEV_ANALY_SKIN_MULTI_PARAM_VMD | Definition for base term 1::4164 MDC_DEV_ANALY_SKIN_MULTI_PARAM is: Instrument for analysis and derivation of skin-related parameters. |  |
`urn:iso:std:iso:11073:10101` | 69703 | MDC_DEV_ANALY_SKIN_MULTI_PARAM_CHAN | Definition for base term 1::4164 MDC_DEV_ANALY_SKIN_MULTI_PARAM is: Instrument for analysis and derivation of skin-related parameters. |  |
`urn:iso:std:iso:11073:10101` | 69704 | MDC_DEV_ANALY_PRESS_AWAY | Instrument that derives airway parameters. |  |
`urn:iso:std:iso:11073:10101` | 69705 | MDC_DEV_ANALY_PRESS_AWAY_MDS | Definition for base term 1::4168 MDC_DEV_ANALY_PRESS_AWAY is: Instrument that derives airway parameters. |  |
`urn:iso:std:iso:11073:10101` | 69706 | MDC_DEV_ANALY_PRESS_AWAY_VMD | Definition for base term 1::4168 MDC_DEV_ANALY_PRESS_AWAY is: Instrument that derives airway parameters. |  |
`urn:iso:std:iso:11073:10101` | 69707 | MDC_DEV_ANALY_PRESS_AWAY_CHAN | Definition for base term 1::4168 MDC_DEV_ANALY_PRESS_AWAY is: Instrument that derives airway parameters. |  |
`urn:iso:std:iso:11073:10101` | 69708 | MDC_DEV_ANALY_PRESS_BLD | Instrument that derives blood pressure parameters, i.e., systolic, diastolic, mean. |  |
`urn:iso:std:iso:11073:10101` | 69709 | MDC_DEV_ANALY_PRESS_BLD_MDS | Definition for base term 1::4172 MDC_DEV_ANALY_PRESS_BLD is: Instrument that derives blood pressure parameters, i.e., systolic, diastolic, mean. |  |
`urn:iso:std:iso:11073:10101` | 69710 | MDC_DEV_ANALY_PRESS_BLD_VMD | Definition for base term 1::4172 MDC_DEV_ANALY_PRESS_BLD is: Instrument that derives blood pressure parameters, i.e., systolic, diastolic, mean. |  |
`urn:iso:std:iso:11073:10101` | 69711 | MDC_DEV_ANALY_PRESS_BLD_CHAN | Definition for base term 1::4172 MDC_DEV_ANALY_PRESS_BLD is: Instrument that derives blood pressure parameters, i.e., systolic, diastolic, mean. |  |
`urn:iso:std:iso:11073:10101` | 69712 | MDC_DEV_ANALY_PRESS_BRAIN_INTRACRAN | Instrument that derives intracranial pressure parameters. |  |
`urn:iso:std:iso:11073:10101` | 69713 | MDC_DEV_ANALY_PRESS_BRAIN_INTRACRAN_MDS | Definition for base term 1::4176 MDC_DEV_ANALY_PRESS_BRAIN_INTRACRAN is: Instrument that derives intracranial pressure parameters. |  |
`urn:iso:std:iso:11073:10101` | 69714 | MDC_DEV_ANALY_PRESS_BRAIN_INTRACRAN_VMD | Definition for base term 1::4176 MDC_DEV_ANALY_PRESS_BRAIN_INTRACRAN is: Instrument that derives intracranial pressure parameters. |  |
`urn:iso:std:iso:11073:10101` | 69715 | MDC_DEV_ANALY_PRESS_BRAIN_INTRACRAN_CHAN | Definition for base term 1::4176 MDC_DEV_ANALY_PRESS_BRAIN_INTRACRAN is: Instrument that derives intracranial pressure parameters. |  |
`urn:iso:std:iso:11073:10101` | 69716 | MDC_DEV_ANALY_PRESS_LUNG | Instrument that derives lung pressure parameters. |  |
`urn:iso:std:iso:11073:10101` | 69717 | MDC_DEV_ANALY_PRESS_LUNG_MDS | Definition for base term 1::4180 MDC_DEV_ANALY_PRESS_LUNG is: Instrument that derives lung pressure parameters. |  |
`urn:iso:std:iso:11073:10101` | 69718 | MDC_DEV_ANALY_PRESS_LUNG_VMD | Definition for base term 1::4180 MDC_DEV_ANALY_PRESS_LUNG is: Instrument that derives lung pressure parameters. |  |
`urn:iso:std:iso:11073:10101` | 69719 | MDC_DEV_ANALY_PRESS_LUNG_CHAN | Definition for base term 1::4180 MDC_DEV_ANALY_PRESS_LUNG is: Instrument that derives lung pressure parameters. |  |
`urn:iso:std:iso:11073:10101` | 69720 | MDC_DEV_ANALY_RESP_RATE | Instrument that derives the lung breathing rate. |  |
`urn:iso:std:iso:11073:10101` | 69721 | MDC_DEV_ANALY_RESP_RATE_MDS | Definition for base term 1::4184 MDC_DEV_ANALY_RESP_RATE is: Instrument that derives the lung breathing rate. |  |
`urn:iso:std:iso:11073:10101` | 69722 | MDC_DEV_ANALY_RESP_RATE_VMD | Definition for base term 1::4184 MDC_DEV_ANALY_RESP_RATE is: Instrument that derives the lung breathing rate. |  |
`urn:iso:std:iso:11073:10101` | 69723 | MDC_DEV_ANALY_RESP_RATE_CHAN | Definition for base term 1::4184 MDC_DEV_ANALY_RESP_RATE is: Instrument that derives the lung breathing rate. |  |
`urn:iso:std:iso:11073:10101` | 69724 | MDC_DEV_ANALY_RES_LUNG | Instrument that derives the resistance (compliance) of the lungs. |  |
`urn:iso:std:iso:11073:10101` | 69725 | MDC_DEV_ANALY_RES_LUNG_MDS | Definition for base term 1::4188 MDC_DEV_ANALY_RES_LUNG is: Instrument that derives the resistance (compliance) of the lungs. |  |
`urn:iso:std:iso:11073:10101` | 69726 | MDC_DEV_ANALY_RES_LUNG_VMD | Definition for base term 1::4188 MDC_DEV_ANALY_RES_LUNG is: Instrument that derives the resistance (compliance) of the lungs. |  |
`urn:iso:std:iso:11073:10101` | 69727 | MDC_DEV_ANALY_RES_LUNG_CHAN | Definition for base term 1::4188 MDC_DEV_ANALY_RES_LUNG is: Instrument that derives the resistance (compliance) of the lungs. |  |
`urn:iso:std:iso:11073:10101` | 69728 | MDC_DEV_ANALY_TEMP_HEART_OUTPUT | Instrument that derives heart output parameters from blood temperature. |  |
`urn:iso:std:iso:11073:10101` | 69729 | MDC_DEV_ANALY_TEMP_HEART_OUTPUT_MDS | Definition for base term 1::4192 MDC_DEV_ANALY_TEMP_HEART_OUTPUT is: Instrument that derives heart output parameters from blood temperature. |  |
`urn:iso:std:iso:11073:10101` | 69730 | MDC_DEV_ANALY_TEMP_HEART_OUTPUT_VMD | Definition for base term 1::4192 MDC_DEV_ANALY_TEMP_HEART_OUTPUT is: Instrument that derives heart output parameters from blood temperature. |  |
`urn:iso:std:iso:11073:10101` | 69731 | MDC_DEV_ANALY_TEMP_HEART_OUTPUT_CHAN | Definition for base term 1::4192 MDC_DEV_ANALY_TEMP_HEART_OUTPUT is: Instrument that derives heart output parameters from blood temperature. |  |
`urn:iso:std:iso:11073:10101` | 69732 | MDC_DEV_ANALY_VOL_HEART | Instrument for the derivation of the size of the heart. |  |
`urn:iso:std:iso:11073:10101` | 69733 | MDC_DEV_ANALY_VOL_HEART_MDS | Definition for base term 1::4196 MDC_DEV_ANALY_VOL_HEART is: Instrument for the derivation of the size of the heart. |  |
`urn:iso:std:iso:11073:10101` | 69734 | MDC_DEV_ANALY_VOL_HEART_VMD | Definition for base term 1::4196 MDC_DEV_ANALY_VOL_HEART is: Instrument for the derivation of the size of the heart. |  |
`urn:iso:std:iso:11073:10101` | 69735 | MDC_DEV_ANALY_VOL_HEART_CHAN | Definition for base term 1::4196 MDC_DEV_ANALY_VOL_HEART is: Instrument for the derivation of the size of the heart. |  |
`urn:iso:std:iso:11073:10101` | 69736 | MDC_DEV_ANALY_VOL_LUNG | Instrument that derives lung volume parameters. |  |
`urn:iso:std:iso:11073:10101` | 69737 | MDC_DEV_ANALY_VOL_LUNG_MDS | Definition for base term 1::4200 MDC_DEV_ANALY_VOL_LUNG is: Instrument that derives lung volume parameters. |  |
`urn:iso:std:iso:11073:10101` | 69738 | MDC_DEV_ANALY_VOL_LUNG_VMD | Definition for base term 1::4200 MDC_DEV_ANALY_VOL_LUNG is: Instrument that derives lung volume parameters. |  |
`urn:iso:std:iso:11073:10101` | 69739 | MDC_DEV_ANALY_VOL_LUNG_CHAN | Definition for base term 1::4200 MDC_DEV_ANALY_VOL_LUNG is: Instrument that derives lung volume parameters. |  |
`urn:iso:std:iso:11073:10101` | 69740 | MDC_DEV_CALC | Instrument that creates derived parameters. |  |
`urn:iso:std:iso:11073:10101` | 69741 | MDC_DEV_CALC_MDS | Definition for base term 1::4204 MDC_DEV_CALC is: Instrument that creates derived parameters. |  |
`urn:iso:std:iso:11073:10101` | 69742 | MDC_DEV_CALC_VMD | Definition for base term 1::4204 MDC_DEV_CALC is: Instrument that creates derived parameters. |  |
`urn:iso:std:iso:11073:10101` | 69743 | MDC_DEV_CALC_CHAN | Definition for base term 1::4204 MDC_DEV_CALC is: Instrument that creates derived parameters. |  |
`urn:iso:std:iso:11073:10101` | 69744 | MDC_DEV_CALC_HEMO | Instrument that derives haemodynamics parameters. |  |
`urn:iso:std:iso:11073:10101` | 69745 | MDC_DEV_CALC_HEMO_MDS | Definition for base term 1::4208 MDC_DEV_CALC_HEMO is: Instrument that derives haemodynamics parameters. |  |
`urn:iso:std:iso:11073:10101` | 69746 | MDC_DEV_CALC_HEMO_VMD | Definition for base term 1::4208 MDC_DEV_CALC_HEMO is: Instrument that derives haemodynamics parameters. |  |
`urn:iso:std:iso:11073:10101` | 69747 | MDC_DEV_CALC_HEMO_CHAN | Definition for base term 1::4208 MDC_DEV_CALC_HEMO is: Instrument that derives haemodynamics parameters. |  |
`urn:iso:std:iso:11073:10101` | 69748 | MDC_DEV_CALC_RENAL | Instrument that derives renal function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69749 | MDC_DEV_CALC_RENAL_MDS | Definition for base term 1::4212 MDC_DEV_CALC_RENAL is: Instrument that derives renal function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69750 | MDC_DEV_CALC_RENAL_VMD | Definition for base term 1::4212 MDC_DEV_CALC_RENAL is: Instrument that derives renal function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69751 | MDC_DEV_CALC_RENAL_CHAN | Definition for base term 1::4212 MDC_DEV_CALC_RENAL is: Instrument that derives renal function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69752 | MDC_DEV_FILTER_CONC | Instrument that filters out one or more chemicals. |  |
`urn:iso:std:iso:11073:10101` | 69753 | MDC_DEV_FILTER_CONC_MDS | Definition for base term 1::4216 MDC_DEV_FILTER_CONC is: Instrument that filters out one or more chemicals. |  |
`urn:iso:std:iso:11073:10101` | 69754 | MDC_DEV_FILTER_CONC_VMD | Definition for base term 1::4216 MDC_DEV_FILTER_CONC is: Instrument that filters out one or more chemicals. |  |
`urn:iso:std:iso:11073:10101` | 69755 | MDC_DEV_FILTER_CONC_CHAN | Definition for base term 1::4216 MDC_DEV_FILTER_CONC is: Instrument that filters out one or more chemicals. |  |
`urn:iso:std:iso:11073:10101` | 69756 | MDC_DEV_FILTER_CONC_AWAY | Instrument for removing components from the chemistry of delivered air. |  |
`urn:iso:std:iso:11073:10101` | 69757 | MDC_DEV_FILTER_CONC_AWAY_MDS | Definition for base term 1::4220 MDC_DEV_FILTER_CONC_AWAY is: Instrument for removing components from the chemistry of delivered air. |  |
`urn:iso:std:iso:11073:10101` | 69758 | MDC_DEV_FILTER_CONC_AWAY_VMD | Definition for base term 1::4220 MDC_DEV_FILTER_CONC_AWAY is: Instrument for removing components from the chemistry of delivered air. |  |
`urn:iso:std:iso:11073:10101` | 69759 | MDC_DEV_FILTER_CONC_AWAY_CHAN | Definition for base term 1::4220 MDC_DEV_FILTER_CONC_AWAY is: Instrument for removing components from the chemistry of delivered air. |  |
`urn:iso:std:iso:11073:10101` | 69760 | MDC_DEV_GEN | Instrument that generates heat, electricity, etc. |  |
`urn:iso:std:iso:11073:10101` | 69761 | MDC_DEV_GEN_MDS | Definition for base term 1::4224 MDC_DEV_GEN is: Instrument that generates heat, electricity, etc. |  |
`urn:iso:std:iso:11073:10101` | 69762 | MDC_DEV_GEN_VMD | Definition for base term 1::4224 MDC_DEV_GEN is: Instrument that generates heat, electricity, etc. |  |
`urn:iso:std:iso:11073:10101` | 69763 | MDC_DEV_GEN_CHAN | Definition for base term 1::4224 MDC_DEV_GEN is: Instrument that generates heat, electricity, etc. |  |
`urn:iso:std:iso:11073:10101` | 69764 | MDC_DEV_GEN_CONC_AWAY | Instrument for adding components to the chemistry of delivered air. |  |
`urn:iso:std:iso:11073:10101` | 69765 | MDC_DEV_GEN_CONC_AWAY_MDS | Definition for base term 1::4228 MDC_DEV_GEN_CONC_AWAY is: Instrument for adding components to the chemistry of delivered air. |  |
`urn:iso:std:iso:11073:10101` | 69766 | MDC_DEV_GEN_CONC_AWAY_VMD | Definition for base term 1::4228 MDC_DEV_GEN_CONC_AWAY is: Instrument for adding components to the chemistry of delivered air. |  |
`urn:iso:std:iso:11073:10101` | 69767 | MDC_DEV_GEN_CONC_AWAY_CHAN | Definition for base term 1::4228 MDC_DEV_GEN_CONC_AWAY is: Instrument for adding components to the chemistry of delivered air. |  |
`urn:iso:std:iso:11073:10101` | 69768 | MDC_DEV_GEN_ELEC_POTL_HEART_DEFIB | Instrument for delivering a controlled heart electrical potential. |  |
`urn:iso:std:iso:11073:10101` | 69769 | MDC_DEV_GEN_ELEC_POTL_HEART_DEFIB_MDS | Definition for base term 1::4232 MDC_DEV_GEN_ELEC_POTL_HEART_DEFIB is: Instrument for delivering a controlled heart electrical potential. |  |
`urn:iso:std:iso:11073:10101` | 69770 | MDC_DEV_GEN_ELEC_POTL_HEART_DEFIB_VMD | Definition for base term 1::4232 MDC_DEV_GEN_ELEC_POTL_HEART_DEFIB is: Instrument for delivering a controlled heart electrical potential. |  |
`urn:iso:std:iso:11073:10101` | 69771 | MDC_DEV_GEN_ELEC_POTL_HEART_DEFIB_CHAN | Definition for base term 1::4232 MDC_DEV_GEN_ELEC_POTL_HEART_DEFIB is: Instrument for delivering a controlled heart electrical potential. |  |
`urn:iso:std:iso:11073:10101` | 69772 | MDC_DEV_GEN_ELEC_POTL_MUSCL | Instrument for delivering a controlled electrical potential to the musculature. |  |
`urn:iso:std:iso:11073:10101` | 69773 | MDC_DEV_GEN_ELEC_POTL_MUSCL_MDS | Definition for base term 1::4236 MDC_DEV_GEN_ELEC_POTL_MUSCL is: Instrument for delivering a controlled electrical potential to the musculature. |  |
`urn:iso:std:iso:11073:10101` | 69774 | MDC_DEV_GEN_ELEC_POTL_MUSCL_VMD | Definition for base term 1::4236 MDC_DEV_GEN_ELEC_POTL_MUSCL is: Instrument for delivering a controlled electrical potential to the musculature. |  |
`urn:iso:std:iso:11073:10101` | 69775 | MDC_DEV_GEN_ELEC_POTL_MUSCL_CHAN | Definition for base term 1::4236 MDC_DEV_GEN_ELEC_POTL_MUSCL is: Instrument for delivering a controlled electrical potential to the musculature. |  |
`urn:iso:std:iso:11073:10101` | 69776 | MDC_DEV_GEN_ELEC_POTL_SKIN | Instrument for delivering a controlled electrical potential to the skin. |  |
`urn:iso:std:iso:11073:10101` | 69777 | MDC_DEV_GEN_ELEC_POTL_SKIN_MDS | Definition for base term 1::4240 MDC_DEV_GEN_ELEC_POTL_SKIN is: Instrument for delivering a controlled electrical potential to the skin. |  |
`urn:iso:std:iso:11073:10101` | 69778 | MDC_DEV_GEN_ELEC_POTL_SKIN_VMD | Definition for base term 1::4240 MDC_DEV_GEN_ELEC_POTL_SKIN is: Instrument for delivering a controlled electrical potential to the skin. |  |
`urn:iso:std:iso:11073:10101` | 69779 | MDC_DEV_GEN_ELEC_POTL_SKIN_CHAN | Definition for base term 1::4240 MDC_DEV_GEN_ELEC_POTL_SKIN is: Instrument for delivering a controlled electrical potential to the skin. |  |
`urn:iso:std:iso:11073:10101` | 69780 | MDC_DEV_GEN_EVOK_POTL_BRAIN_MULTI_PARAM | Instrument that derives brain activity parameters via stimulation. |  |
`urn:iso:std:iso:11073:10101` | 69781 | MDC_DEV_GEN_EVOK_POTL_BRAIN_MULTI_PARAM_MDS | Definition for base term 1::4244 MDC_DEV_GEN_EVOK_POTL_BRAIN_MULTI_PARAM is: Instrument that derives brain activity parameters via stimulation. |  |
`urn:iso:std:iso:11073:10101` | 69782 | MDC_DEV_GEN_EVOK_POTL_BRAIN_MULTI_PARAM_VMD | Definition for base term 1::4244 MDC_DEV_GEN_EVOK_POTL_BRAIN_MULTI_PARAM is: Instrument that derives brain activity parameters via stimulation. |  |
`urn:iso:std:iso:11073:10101` | 69783 | MDC_DEV_GEN_EVOK_POTL_BRAIN_MULTI_PARAM_CHAN | Definition for base term 1::4244 MDC_DEV_GEN_EVOK_POTL_BRAIN_MULTI_PARAM is: Instrument that derives brain activity parameters via stimulation. |  |
`urn:iso:std:iso:11073:10101` | 69784 | MDC_DEV_GEN_RATE_HEART | Instrument for controlling the rate of heart contractions. |  |
`urn:iso:std:iso:11073:10101` | 69785 | MDC_DEV_GEN_RATE_HEART_MDS | Definition for base term 1::4248 MDC_DEV_GEN_RATE_HEART is: Instrument for controlling the rate of heart contractions. |  |
`urn:iso:std:iso:11073:10101` | 69786 | MDC_DEV_GEN_RATE_HEART_VMD | Definition for base term 1::4248 MDC_DEV_GEN_RATE_HEART is: Instrument for controlling the rate of heart contractions. |  |
`urn:iso:std:iso:11073:10101` | 69787 | MDC_DEV_GEN_RATE_HEART_CHAN | Definition for base term 1::4248 MDC_DEV_GEN_RATE_HEART is: Instrument for controlling the rate of heart contractions. |  |
`urn:iso:std:iso:11073:10101` | 69788 | MDC_DEV_GEN_TEMP_MUSCL | Instrument for delivering a controlled temperature to the musculature. |  |
`urn:iso:std:iso:11073:10101` | 69789 | MDC_DEV_GEN_TEMP_MUSCL_MDS | Definition for base term 1::4252 MDC_DEV_GEN_TEMP_MUSCL is: Instrument for delivering a controlled temperature to the musculature. |  |
`urn:iso:std:iso:11073:10101` | 69790 | MDC_DEV_GEN_TEMP_MUSCL_VMD | Definition for base term 1::4252 MDC_DEV_GEN_TEMP_MUSCL is: Instrument for delivering a controlled temperature to the musculature. |  |
`urn:iso:std:iso:11073:10101` | 69791 | MDC_DEV_GEN_TEMP_MUSCL_CHAN | Definition for base term 1::4252 MDC_DEV_GEN_TEMP_MUSCL is: Instrument for delivering a controlled temperature to the musculature. |  |
`urn:iso:std:iso:11073:10101` | 69792 | MDC_DEV_METER | Instrument for the direct measurement of physiological parameters. |  |
`urn:iso:std:iso:11073:10101` | 69793 | MDC_DEV_METER_MDS | Definition for base term 1::4256 MDC_DEV_METER is: Instrument for the direct measurement of physiological parameters. |  |
`urn:iso:std:iso:11073:10101` | 69794 | MDC_DEV_METER_VMD | Definition for base term 1::4256 MDC_DEV_METER is: Instrument for the direct measurement of physiological parameters. |  |
`urn:iso:std:iso:11073:10101` | 69795 | MDC_DEV_METER_CHAN | Definition for base term 1::4256 MDC_DEV_METER is: Instrument for the direct measurement of physiological parameters. |  |
`urn:iso:std:iso:11073:10101` | 69796 | MDC_DEV_ECG | Instrument for the direct measurement of heart electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69797 | MDC_DEV_ECG_MDS | Definition for base term 1::4260 MDC_DEV_ECG is: Instrument for the direct measurement of heart electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69798 | MDC_DEV_ECG_VMD | Definition for base term 1::4260 MDC_DEV_ECG is: Instrument for the direct measurement of heart electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69799 | MDC_DEV_ECG_CHAN | Definition for base term 1::4260 MDC_DEV_ECG is: Instrument for the direct measurement of heart electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69800 | MDC_DEV_METER_CONC_SKIN_GAS | Instrument for the measurement of the level and concentration of gases in the tissue. |  |
`urn:iso:std:iso:11073:10101` | 69801 | MDC_DEV_METER_CONC_SKIN_GAS_MDS | Definition for base term 1::4264 MDC_DEV_METER_CONC_SKIN_GAS is: Instrument for the measurement of the level and concentration of gases in the tissue. |  |
`urn:iso:std:iso:11073:10101` | 69802 | MDC_DEV_METER_CONC_SKIN_GAS_VMD | Definition for base term 1::4264 MDC_DEV_METER_CONC_SKIN_GAS is: Instrument for the measurement of the level and concentration of gases in the tissue. |  |
`urn:iso:std:iso:11073:10101` | 69803 | MDC_DEV_METER_CONC_SKIN_GAS_CHAN | Definition for base term 1::4264 MDC_DEV_METER_CONC_SKIN_GAS is: Instrument for the measurement of the level and concentration of gases in the tissue. |  |
`urn:iso:std:iso:11073:10101` | 69804 | MDC_DEV_METER_CONC_URINE | Instrument for the direct measurement of urine chemistry. |  |
`urn:iso:std:iso:11073:10101` | 69805 | MDC_DEV_METER_CONC_URINE_MDS | Definition for base term 1::4268 MDC_DEV_METER_CONC_URINE is: Instrument for the direct measurement of urine chemistry. |  |
`urn:iso:std:iso:11073:10101` | 69806 | MDC_DEV_METER_CONC_URINE_VMD | Definition for base term 1::4268 MDC_DEV_METER_CONC_URINE is: Instrument for the direct measurement of urine chemistry. |  |
`urn:iso:std:iso:11073:10101` | 69807 | MDC_DEV_METER_CONC_URINE_CHAN | Definition for base term 1::4268 MDC_DEV_METER_CONC_URINE is: Instrument for the direct measurement of urine chemistry. |  |
`urn:iso:std:iso:11073:10101` | 69808 | MDC_DEV_EEG | Instrument for the direct measurement of the level of brain electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69809 | MDC_DEV_EEG_MDS | Definition for base term 1::4272 MDC_DEV_EEG is: Instrument for the direct measurement of the level of brain electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69810 | MDC_DEV_EEG_VMD | Definition for base term 1::4272 MDC_DEV_EEG is: Instrument for the direct measurement of the level of brain electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69811 | MDC_DEV_EEG_CHAN | Definition for base term 1::4272 MDC_DEV_EEG is: Instrument for the direct measurement of the level of brain electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69812 | MDC_DEV_EMG | Instrument for the direct measurement of musculature electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69813 | MDC_DEV_EMG_MDS | Definition for base term 1::4276 MDC_DEV_EMG is: Instrument for the direct measurement of musculature electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69814 | MDC_DEV_EMG_VMD | Definition for base term 1::4276 MDC_DEV_EMG is: Instrument for the direct measurement of musculature electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69815 | MDC_DEV_EMG_CHAN | Definition for base term 1::4276 MDC_DEV_EMG is: Instrument for the direct measurement of musculature electrical activity. |  |
`urn:iso:std:iso:11073:10101` | 69816 | MDC_DEV_METER_FLOW_AWAY | Instrument for the direct measurement of the level of air flow. |  |
`urn:iso:std:iso:11073:10101` | 69817 | MDC_DEV_METER_FLOW_AWAY_MDS | Definition for base term 1::4280 MDC_DEV_METER_FLOW_AWAY is: Instrument for the direct measurement of the level of air flow. |  |
`urn:iso:std:iso:11073:10101` | 69818 | MDC_DEV_METER_FLOW_AWAY_VMD | Definition for base term 1::4280 MDC_DEV_METER_FLOW_AWAY is: Instrument for the direct measurement of the level of air flow. |  |
`urn:iso:std:iso:11073:10101` | 69819 | MDC_DEV_METER_FLOW_AWAY_CHAN | Definition for base term 1::4280 MDC_DEV_METER_FLOW_AWAY is: Instrument for the direct measurement of the level of air flow. |  |
`urn:iso:std:iso:11073:10101` | 69820 | MDC_DEV_METER_FLOW_BLD | Instrument for the direct measurement of the level of blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69821 | MDC_DEV_METER_FLOW_BLD_MDS | Definition for base term 1::4284 MDC_DEV_METER_FLOW_BLD is: Instrument for the direct measurement of the level of blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69822 | MDC_DEV_METER_FLOW_BLD_VMD | Definition for base term 1::4284 MDC_DEV_METER_FLOW_BLD is: Instrument for the direct measurement of the level of blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69823 | MDC_DEV_METER_FLOW_BLD_CHAN | Definition for base term 1::4284 MDC_DEV_METER_FLOW_BLD is: Instrument for the direct measurement of the level of blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69824 | MDC_DEV_METER_FLOW_CARD | Instrument for the direct measurement of the level of heart blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69825 | MDC_DEV_METER_FLOW_CARD_MDS | Definition for base term 1::4288 MDC_DEV_METER_FLOW_CARD is: Instrument for the direct measurement of the level of heart blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69826 | MDC_DEV_METER_FLOW_CARD_VMD | Definition for base term 1::4288 MDC_DEV_METER_FLOW_CARD is: Instrument for the direct measurement of the level of heart blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69827 | MDC_DEV_METER_FLOW_CARD_CHAN | Definition for base term 1::4288 MDC_DEV_METER_FLOW_CARD is: Instrument for the direct measurement of the level of heart blood flow. |  |
`urn:iso:std:iso:11073:10101` | 69828 | MDC_DEV_METER_FLOW_LUNG | Instrument for the direct measurement of the level of lung air flow. |  |
`urn:iso:std:iso:11073:10101` | 69829 | MDC_DEV_METER_FLOW_LUNG_MDS | Definition for base term 1::4292 MDC_DEV_METER_FLOW_LUNG is: Instrument for the direct measurement of the level of lung air flow. |  |
`urn:iso:std:iso:11073:10101` | 69830 | MDC_DEV_METER_FLOW_LUNG_VMD | Definition for base term 1::4292 MDC_DEV_METER_FLOW_LUNG is: Instrument for the direct measurement of the level of lung air flow. |  |
`urn:iso:std:iso:11073:10101` | 69831 | MDC_DEV_METER_FLOW_LUNG_CHAN | Definition for base term 1::4292 MDC_DEV_METER_FLOW_LUNG is: Instrument for the direct measurement of the level of lung air flow. |  |
`urn:iso:std:iso:11073:10101` | 69832 | MDC_DEV_METER_FLOW_URINE | Instrument for the direct measurement of the level of urinary flow. |  |
`urn:iso:std:iso:11073:10101` | 69833 | MDC_DEV_METER_FLOW_URINE_MDS | Definition for base term 1::4296 MDC_DEV_METER_FLOW_URINE is: Instrument for the direct measurement of the level of urinary flow. |  |
`urn:iso:std:iso:11073:10101` | 69834 | MDC_DEV_METER_FLOW_URINE_VMD | Definition for base term 1::4296 MDC_DEV_METER_FLOW_URINE is: Instrument for the direct measurement of the level of urinary flow. |  |
`urn:iso:std:iso:11073:10101` | 69835 | MDC_DEV_METER_FLOW_URINE_CHAN | Definition for base term 1::4296 MDC_DEV_METER_FLOW_URINE is: Instrument for the direct measurement of the level of urinary flow. |  |
`urn:iso:std:iso:11073:10101` | 69836 | MDC_DEV_METER_PHYSIO_MULTI_PARAM | Instrument that acquires data through direct measurement from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69837 | MDC_DEV_METER_PHYSIO_MULTI_PARAM_MDS | Definition for base term 1::4300 MDC_DEV_METER_PHYSIO_MULTI_PARAM is: Instrument that acquires data through direct measurement from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69838 | MDC_DEV_METER_PHYSIO_MULTI_PARAM_VMD | Definition for base term 1::4300 MDC_DEV_METER_PHYSIO_MULTI_PARAM is: Instrument that acquires data through direct measurement from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69839 | MDC_DEV_METER_PHYSIO_MULTI_PARAM_CHAN | Definition for base term 1::4300 MDC_DEV_METER_PHYSIO_MULTI_PARAM is: Instrument that acquires data through direct measurement from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69840 | MDC_DEV_METER_SKIN_MULTI_PARAM | Instrument for direct measurement of skin parameters. |  |
`urn:iso:std:iso:11073:10101` | 69841 | MDC_DEV_METER_SKIN_MULTI_PARAM_MDS | Definition for base term 1::4304 MDC_DEV_METER_SKIN_MULTI_PARAM is: Instrument for direct measurement of skin parameters. |  |
`urn:iso:std:iso:11073:10101` | 69842 | MDC_DEV_METER_SKIN_MULTI_PARAM_VMD | Definition for base term 1::4304 MDC_DEV_METER_SKIN_MULTI_PARAM is: Instrument for direct measurement of skin parameters. |  |
`urn:iso:std:iso:11073:10101` | 69843 | MDC_DEV_METER_SKIN_MULTI_PARAM_CHAN | Definition for base term 1::4304 MDC_DEV_METER_SKIN_MULTI_PARAM is: Instrument for direct measurement of skin parameters. |  |
`urn:iso:std:iso:11073:10101` | 69844 | MDC_DEV_METER_BLD_CHEM | Instrument for the direct measurement of the level and concentration of chemicals, gases and electrolytes in the blood. |  |
`urn:iso:std:iso:11073:10101` | 69845 | MDC_DEV_METER_BLD_CHEM_MDS | Definition for base term 1::4308 MDC_DEV_METER_BLD_CHEM is: Instrument for the direct measurement of the level and concentration of chemicals, gases and electrolytes in the blood. |  |
`urn:iso:std:iso:11073:10101` | 69846 | MDC_DEV_METER_BLD_CHEM_VMD | Definition for base term 1::4308 MDC_DEV_METER_BLD_CHEM is: Instrument for the direct measurement of the level and concentration of chemicals, gases and electrolytes in the blood. |  |
`urn:iso:std:iso:11073:10101` | 69847 | MDC_DEV_METER_BLD_CHEM_CHAN | Definition for base term 1::4308 MDC_DEV_METER_BLD_CHEM is: Instrument for the direct measurement of the level and concentration of chemicals, gases and electrolytes in the blood. |  |
`urn:iso:std:iso:11073:10101` | 69848 | MDC_DEV_METER_PRESS_AIR | Instrument for the direct measurement of the level of delivered air pressure. |  |
`urn:iso:std:iso:11073:10101` | 69849 | MDC_DEV_METER_PRESS_AIR_MDS | Definition for base term 1::4312 MDC_DEV_METER_PRESS_AIR is: Instrument for the direct measurement of the level of delivered air pressure. |  |
`urn:iso:std:iso:11073:10101` | 69850 | MDC_DEV_METER_PRESS_AIR_VMD | Definition for base term 1::4312 MDC_DEV_METER_PRESS_AIR is: Instrument for the direct measurement of the level of delivered air pressure. |  |
`urn:iso:std:iso:11073:10101` | 69851 | MDC_DEV_METER_PRESS_AIR_CHAN | Definition for base term 1::4312 MDC_DEV_METER_PRESS_AIR is: Instrument for the direct measurement of the level of delivered air pressure. |  |
`urn:iso:std:iso:11073:10101` | 69852 | MDC_DEV_METER_PRESS_BLD | Instrument for the direct measurement of the level of blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 69853 | MDC_DEV_METER_PRESS_BLD_MDS | Definition for base term 1::4316 MDC_DEV_METER_PRESS_BLD is: Instrument for the direct measurement of the level of blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 69854 | MDC_DEV_METER_PRESS_BLD_VMD | Definition for base term 1::4316 MDC_DEV_METER_PRESS_BLD is: Instrument for the direct measurement of the level of blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 69855 | MDC_DEV_METER_PRESS_BLD_CHAN | Definition for base term 1::4316 MDC_DEV_METER_PRESS_BLD is: Instrument for the direct measurement of the level of blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 69856 | MDC_DEV_METER_PRESS_INTRA_CRAN | Instrument for the direct measurement of the level of cranial pressure. |  |
`urn:iso:std:iso:11073:10101` | 69857 | MDC_DEV_METER_PRESS_INTRA_CRAN_MDS | Definition for base term 1::4320 MDC_DEV_METER_PRESS_INTRA_CRAN is: Instrument for the direct measurement of the level of cranial pressure. |  |
`urn:iso:std:iso:11073:10101` | 69858 | MDC_DEV_METER_PRESS_INTRA_CRAN_VMD | Definition for base term 1::4320 MDC_DEV_METER_PRESS_INTRA_CRAN is: Instrument for the direct measurement of the level of cranial pressure. |  |
`urn:iso:std:iso:11073:10101` | 69859 | MDC_DEV_METER_PRESS_INTRA_CRAN_CHAN | Definition for base term 1::4320 MDC_DEV_METER_PRESS_INTRA_CRAN is: Instrument for the direct measurement of the level of cranial pressure. |  |
`urn:iso:std:iso:11073:10101` | 69860 | MDC_DEV_METER_PRESS_HEART | Instrument for the direct measurement of the level of heart blood pressures. |  |
`urn:iso:std:iso:11073:10101` | 69861 | MDC_DEV_METER_PRESS_HEART_MDS | Definition for base term 1::4324 MDC_DEV_METER_PRESS_HEART is: Instrument for the direct measurement of the level of heart blood pressures. |  |
`urn:iso:std:iso:11073:10101` | 69862 | MDC_DEV_METER_PRESS_HEART_VMD | Definition for base term 1::4324 MDC_DEV_METER_PRESS_HEART is: Instrument for the direct measurement of the level of heart blood pressures. |  |
`urn:iso:std:iso:11073:10101` | 69863 | MDC_DEV_METER_PRESS_HEART_CHAN | Definition for base term 1::4324 MDC_DEV_METER_PRESS_HEART is: Instrument for the direct measurement of the level of heart blood pressures. |  |
`urn:iso:std:iso:11073:10101` | 69864 | MDC_DEV_METER_PRESS_LUNG | Instrument for the direct measurement of the level of lung air pressure. |  |
`urn:iso:std:iso:11073:10101` | 69865 | MDC_DEV_METER_PRESS_LUNG_MDS | Definition for base term 1::4328 MDC_DEV_METER_PRESS_LUNG is: Instrument for the direct measurement of the level of lung air pressure. |  |
`urn:iso:std:iso:11073:10101` | 69866 | MDC_DEV_METER_PRESS_LUNG_VMD | Definition for base term 1::4328 MDC_DEV_METER_PRESS_LUNG is: Instrument for the direct measurement of the level of lung air pressure. |  |
`urn:iso:std:iso:11073:10101` | 69867 | MDC_DEV_METER_PRESS_LUNG_CHAN | Definition for base term 1::4328 MDC_DEV_METER_PRESS_LUNG is: Instrument for the direct measurement of the level of lung air pressure. |  |
`urn:iso:std:iso:11073:10101` | 69868 | MDC_DEV_METER_RES_AIR | Instrument for the direct measurement of the level of airway resistance. |  |
`urn:iso:std:iso:11073:10101` | 69869 | MDC_DEV_METER_RES_AIR_MDS | Definition for base term 1::4332 MDC_DEV_METER_RES_AIR is: Instrument for the direct measurement of the level of airway resistance. |  |
`urn:iso:std:iso:11073:10101` | 69870 | MDC_DEV_METER_RES_AIR_VMD | Definition for base term 1::4332 MDC_DEV_METER_RES_AIR is: Instrument for the direct measurement of the level of airway resistance. |  |
`urn:iso:std:iso:11073:10101` | 69871 | MDC_DEV_METER_RES_AIR_CHAN | Definition for base term 1::4332 MDC_DEV_METER_RES_AIR is: Instrument for the direct measurement of the level of airway resistance. |  |
`urn:iso:std:iso:11073:10101` | 69872 | MDC_DEV_METER_RES_LUNG | Instrument for the direct measurement of the level of lung resistance. |  |
`urn:iso:std:iso:11073:10101` | 69873 | MDC_DEV_METER_RES_LUNG_MDS | Definition for base term 1::4336 MDC_DEV_METER_RES_LUNG is: Instrument for the direct measurement of the level of lung resistance. |  |
`urn:iso:std:iso:11073:10101` | 69874 | MDC_DEV_METER_RES_LUNG_VMD | Definition for base term 1::4336 MDC_DEV_METER_RES_LUNG is: Instrument for the direct measurement of the level of lung resistance. |  |
`urn:iso:std:iso:11073:10101` | 69875 | MDC_DEV_METER_RES_LUNG_CHAN | Definition for base term 1::4336 MDC_DEV_METER_RES_LUNG is: Instrument for the direct measurement of the level of lung resistance. |  |
`urn:iso:std:iso:11073:10101` | 69876 | MDC_DEV_METER_STRENGTH_MUSCL | Instrument for the direct measurement of the level of muscle strength. |  |
`urn:iso:std:iso:11073:10101` | 69877 | MDC_DEV_METER_STRENGTH_MUSCL_MDS | Definition for base term 1::4340 MDC_DEV_METER_STRENGTH_MUSCL is: Instrument for the direct measurement of the level of muscle strength. |  |
`urn:iso:std:iso:11073:10101` | 69878 | MDC_DEV_METER_STRENGTH_MUSCL_VMD | Definition for base term 1::4340 MDC_DEV_METER_STRENGTH_MUSCL is: Instrument for the direct measurement of the level of muscle strength. |  |
`urn:iso:std:iso:11073:10101` | 69879 | MDC_DEV_METER_STRENGTH_MUSCL_CHAN | Definition for base term 1::4340 MDC_DEV_METER_STRENGTH_MUSCL is: Instrument for the direct measurement of the level of muscle strength. |  |
`urn:iso:std:iso:11073:10101` | 69880 | MDC_DEV_METER_TEMP_AIR | Instrument for the measurement of the level of delivered air temperature. |  |
`urn:iso:std:iso:11073:10101` | 69881 | MDC_DEV_METER_TEMP_AIR_MDS | Definition for base term 1::4344 MDC_DEV_METER_TEMP_AIR is: Instrument for the measurement of the level of delivered air temperature. |  |
`urn:iso:std:iso:11073:10101` | 69882 | MDC_DEV_METER_TEMP_AIR_VMD | Definition for base term 1::4344 MDC_DEV_METER_TEMP_AIR is: Instrument for the measurement of the level of delivered air temperature. |  |
`urn:iso:std:iso:11073:10101` | 69883 | MDC_DEV_METER_TEMP_AIR_CHAN | Definition for base term 1::4344 MDC_DEV_METER_TEMP_AIR is: Instrument for the measurement of the level of delivered air temperature. |  |
`urn:iso:std:iso:11073:10101` | 69884 | MDC_DEV_METER_TEMP_BLD | Instrument for the direct measurement of the level of blood temperature. |  |
`urn:iso:std:iso:11073:10101` | 69885 | MDC_DEV_METER_TEMP_BLD_MDS | Definition for base term 1::4348 MDC_DEV_METER_TEMP_BLD is: Instrument for the direct measurement of the level of blood temperature. |  |
`urn:iso:std:iso:11073:10101` | 69886 | MDC_DEV_METER_TEMP_BLD_VMD | Definition for base term 1::4348 MDC_DEV_METER_TEMP_BLD is: Instrument for the direct measurement of the level of blood temperature. |  |
`urn:iso:std:iso:11073:10101` | 69887 | MDC_DEV_METER_TEMP_BLD_CHAN | Definition for base term 1::4348 MDC_DEV_METER_TEMP_BLD is: Instrument for the direct measurement of the level of blood temperature. |  |
`urn:iso:std:iso:11073:10101` | 69888 | MDC_DEV_METER_TEMP_BRAIN | Instrument for the direct measurement of the level of brain temperature. |  |
`urn:iso:std:iso:11073:10101` | 69889 | MDC_DEV_METER_TEMP_BRAIN_MDS | Definition for base term 1::4352 MDC_DEV_METER_TEMP_BRAIN is: Instrument for the direct measurement of the level of brain temperature. |  |
`urn:iso:std:iso:11073:10101` | 69890 | MDC_DEV_METER_TEMP_BRAIN_VMD | Definition for base term 1::4352 MDC_DEV_METER_TEMP_BRAIN is: Instrument for the direct measurement of the level of brain temperature. |  |
`urn:iso:std:iso:11073:10101` | 69891 | MDC_DEV_METER_TEMP_BRAIN_CHAN | Definition for base term 1::4352 MDC_DEV_METER_TEMP_BRAIN is: Instrument for the direct measurement of the level of brain temperature. |  |
`urn:iso:std:iso:11073:10101` | 69892 | MDC_DEV_METER_TEMP_HEART | Instrument for the direct measurement of the level of heart temperatures. |  |
`urn:iso:std:iso:11073:10101` | 69893 | MDC_DEV_METER_TEMP_HEART_MDS | Definition for base term 1::4356 MDC_DEV_METER_TEMP_HEART is: Instrument for the direct measurement of the level of heart temperatures. |  |
`urn:iso:std:iso:11073:10101` | 69894 | MDC_DEV_METER_TEMP_HEART_VMD | Definition for base term 1::4356 MDC_DEV_METER_TEMP_HEART is: Instrument for the direct measurement of the level of heart temperatures. |  |
`urn:iso:std:iso:11073:10101` | 69895 | MDC_DEV_METER_TEMP_HEART_CHAN | Definition for base term 1::4356 MDC_DEV_METER_TEMP_HEART is: Instrument for the direct measurement of the level of heart temperatures. |  |
`urn:iso:std:iso:11073:10101` | 69896 | MDC_DEV_METER_TEMP_LUNG | Instrument for the direct measurement of the level of lung temperature. |  |
`urn:iso:std:iso:11073:10101` | 69897 | MDC_DEV_METER_TEMP_LUNG_MDS | Definition for base term 1::4360 MDC_DEV_METER_TEMP_LUNG is: Instrument for the direct measurement of the level of lung temperature. |  |
`urn:iso:std:iso:11073:10101` | 69898 | MDC_DEV_METER_TEMP_LUNG_VMD | Definition for base term 1::4360 MDC_DEV_METER_TEMP_LUNG is: Instrument for the direct measurement of the level of lung temperature. |  |
`urn:iso:std:iso:11073:10101` | 69899 | MDC_DEV_METER_TEMP_LUNG_CHAN | Definition for base term 1::4360 MDC_DEV_METER_TEMP_LUNG is: Instrument for the direct measurement of the level of lung temperature. |  |
`urn:iso:std:iso:11073:10101` | 69900 | MDC_DEV_METER_TEMP | Instrument that measures temperature from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69901 | MDC_DEV_METER_TEMP_MDS | Definition for base term 1::4364 MDC_DEV_METER_TEMP is: Instrument that measures temperature from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69902 | MDC_DEV_METER_TEMP_VMD | Definition for base term 1::4364 MDC_DEV_METER_TEMP is: Instrument that measures temperature from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69903 | MDC_DEV_METER_TEMP_CHAN | Definition for base term 1::4364 MDC_DEV_METER_TEMP is: Instrument that measures temperature from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69904 | MDC_DEV_METER_TEMP_RENAL | Instrument for the direct measurement of the level of renal temperature. |  |
`urn:iso:std:iso:11073:10101` | 69905 | MDC_DEV_METER_TEMP_RENAL_MDS | Definition for base term 1::4368 MDC_DEV_METER_TEMP_RENAL is: Instrument for the direct measurement of the level of renal temperature. |  |
`urn:iso:std:iso:11073:10101` | 69906 | MDC_DEV_METER_TEMP_RENAL_VMD | Definition for base term 1::4368 MDC_DEV_METER_TEMP_RENAL is: Instrument for the direct measurement of the level of renal temperature. |  |
`urn:iso:std:iso:11073:10101` | 69907 | MDC_DEV_METER_TEMP_RENAL_CHAN | Definition for base term 1::4368 MDC_DEV_METER_TEMP_RENAL is: Instrument for the direct measurement of the level of renal temperature. |  |
`urn:iso:std:iso:11073:10101` | 69908 | MDC_DEV_METER_TEMP_SKIN | Instrument for the direct measurement of the level of skin temperature. |  |
`urn:iso:std:iso:11073:10101` | 69909 | MDC_DEV_METER_TEMP_SKIN_MDS | Definition for base term 1::4372 MDC_DEV_METER_TEMP_SKIN is: Instrument for the direct measurement of the level of skin temperature. |  |
`urn:iso:std:iso:11073:10101` | 69910 | MDC_DEV_METER_TEMP_SKIN_VMD | Definition for base term 1::4372 MDC_DEV_METER_TEMP_SKIN is: Instrument for the direct measurement of the level of skin temperature. |  |
`urn:iso:std:iso:11073:10101` | 69911 | MDC_DEV_METER_TEMP_SKIN_CHAN | Definition for base term 1::4372 MDC_DEV_METER_TEMP_SKIN is: Instrument for the direct measurement of the level of skin temperature. |  |
`urn:iso:std:iso:11073:10101` | 69912 | MDC_DEV_METER_VOL_AIR | Instrument for the direct measurement of the level of delivered air volume. |  |
`urn:iso:std:iso:11073:10101` | 69913 | MDC_DEV_METER_VOL_AIR_MDS | Definition for base term 1::4376 MDC_DEV_METER_VOL_AIR is: Instrument for the direct measurement of the level of delivered air volume. |  |
`urn:iso:std:iso:11073:10101` | 69914 | MDC_DEV_METER_VOL_AIR_VMD | Definition for base term 1::4376 MDC_DEV_METER_VOL_AIR is: Instrument for the direct measurement of the level of delivered air volume. |  |
`urn:iso:std:iso:11073:10101` | 69915 | MDC_DEV_METER_VOL_AIR_CHAN | Definition for base term 1::4376 MDC_DEV_METER_VOL_AIR is: Instrument for the direct measurement of the level of delivered air volume. |  |
`urn:iso:std:iso:11073:10101` | 69916 | MDC_DEV_METER_VOL_HEART | Instrument for the direct measurement of the size of the heart. |  |
`urn:iso:std:iso:11073:10101` | 69917 | MDC_DEV_METER_VOL_HEART_MDS | Definition for base term 1::4380 MDC_DEV_METER_VOL_HEART is: Instrument for the direct measurement of the size of the heart. |  |
`urn:iso:std:iso:11073:10101` | 69918 | MDC_DEV_METER_VOL_HEART_VMD | Definition for base term 1::4380 MDC_DEV_METER_VOL_HEART is: Instrument for the direct measurement of the size of the heart. |  |
`urn:iso:std:iso:11073:10101` | 69919 | MDC_DEV_METER_VOL_HEART_CHAN | Definition for base term 1::4380 MDC_DEV_METER_VOL_HEART is: Instrument for the direct measurement of the size of the heart. |  |
`urn:iso:std:iso:11073:10101` | 69920 | MDC_DEV_METER_VOL_MUSCL | Instrument for the direct measurement of the level of muscle bulk. |  |
`urn:iso:std:iso:11073:10101` | 69921 | MDC_DEV_METER_VOL_MUSCL_MDS | Definition for base term 1::4384 MDC_DEV_METER_VOL_MUSCL is: Instrument for the direct measurement of the level of muscle bulk. |  |
`urn:iso:std:iso:11073:10101` | 69922 | MDC_DEV_METER_VOL_MUSCL_VMD | Definition for base term 1::4384 MDC_DEV_METER_VOL_MUSCL is: Instrument for the direct measurement of the level of muscle bulk. |  |
`urn:iso:std:iso:11073:10101` | 69923 | MDC_DEV_METER_VOL_MUSCL_CHAN | Definition for base term 1::4384 MDC_DEV_METER_VOL_MUSCL is: Instrument for the direct measurement of the level of muscle bulk. |  |
`urn:iso:std:iso:11073:10101` | 69924 | MDC_DEV_MON | Instrument for the direct measurement and analysis of patient information. |  |
`urn:iso:std:iso:11073:10101` | 69925 | MDC_DEV_MON_MDS | Definition for base term 1::4388 MDC_DEV_MON is: Instrument for the direct measurement and analysis of patient information. |  |
`urn:iso:std:iso:11073:10101` | 69926 | MDC_DEV_MON_VMD | Definition for base term 1::4388 MDC_DEV_MON is: Instrument for the direct measurement and analysis of patient information. |  |
`urn:iso:std:iso:11073:10101` | 69927 | MDC_DEV_MON_CHAN | Definition for base term 1::4388 MDC_DEV_MON is: Instrument for the direct measurement and analysis of patient information. |  |
`urn:iso:std:iso:11073:10101` | 69928 | MDC_DEV_MON_URINE_CHEM | Instrument for the direct measurement and analysis of urine chemistry. |  |
`urn:iso:std:iso:11073:10101` | 69929 | MDC_DEV_MON_URINE_CHEM_MDS | Definition for base term 1::4392 MDC_DEV_MON_URINE_CHEM is: Instrument for the direct measurement and analysis of urine chemistry. |  |
`urn:iso:std:iso:11073:10101` | 69930 | MDC_DEV_MON_URINE_CHEM_VMD | Definition for base term 1::4392 MDC_DEV_MON_URINE_CHEM is: Instrument for the direct measurement and analysis of urine chemistry. |  |
`urn:iso:std:iso:11073:10101` | 69931 | MDC_DEV_MON_URINE_CHEM_CHAN | Definition for base term 1::4392 MDC_DEV_MON_URINE_CHEM is: Instrument for the direct measurement and analysis of urine chemistry. |  |
`urn:iso:std:iso:11073:10101` | 69932 | MDC_DEV_MON_BLD_CHEM_MULTI_PARAM | Instrument for acquisition, analysis, and derivation of blood chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69933 | MDC_DEV_MON_BLD_CHEM_MULTI_PARAM_MDS | Definition for base term 1::4396 MDC_DEV_MON_BLD_CHEM_MULTI_PARAM is: Instrument for acquisition, analysis, and derivation of blood chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69934 | MDC_DEV_MON_BLD_CHEM_MULTI_PARAM_VMD | Definition for base term 1::4396 MDC_DEV_MON_BLD_CHEM_MULTI_PARAM is: Instrument for acquisition, analysis, and derivation of blood chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69935 | MDC_DEV_MON_BLD_CHEM_MULTI_PARAM_CHAN | Definition for base term 1::4396 MDC_DEV_MON_BLD_CHEM_MULTI_PARAM is: Instrument for acquisition, analysis, and derivation of blood chemistry parameters. |  |
`urn:iso:std:iso:11073:10101` | 69936 | MDC_DEV_MON_BRAIN_FUNC | Instrument that implements brain transduction and analysis. |  |
`urn:iso:std:iso:11073:10101` | 69937 | MDC_DEV_MON_BRAIN_FUNC_MDS | Definition for base term 1::4400 MDC_DEV_MON_BRAIN_FUNC is: Instrument that implements brain transduction and analysis. |  |
`urn:iso:std:iso:11073:10101` | 69938 | MDC_DEV_MON_BRAIN_FUNC_VMD | Definition for base term 1::4400 MDC_DEV_MON_BRAIN_FUNC is: Instrument that implements brain transduction and analysis. |  |
`urn:iso:std:iso:11073:10101` | 69939 | MDC_DEV_MON_BRAIN_FUNC_CHAN | Definition for base term 1::4400 MDC_DEV_MON_BRAIN_FUNC is: Instrument that implements brain transduction and analysis. |  |
`urn:iso:std:iso:11073:10101` | 69940 | MDC_DEV_MON_HEART_MULTI_PARAM | Instrument for acquisition, analysis, and derivation of heart parameters. |  |
`urn:iso:std:iso:11073:10101` | 69941 | MDC_DEV_MON_HEART_MULTI_PARAM_MDS | Definition for base term 1::4404 MDC_DEV_MON_HEART_MULTI_PARAM is: Instrument for acquisition, analysis, and derivation of heart parameters. |  |
`urn:iso:std:iso:11073:10101` | 69942 | MDC_DEV_MON_HEART_MULTI_PARAM_VMD | Definition for base term 1::4404 MDC_DEV_MON_HEART_MULTI_PARAM is: Instrument for acquisition, analysis, and derivation of heart parameters. |  |
`urn:iso:std:iso:11073:10101` | 69943 | MDC_DEV_MON_HEART_MULTI_PARAM_CHAN | Definition for base term 1::4404 MDC_DEV_MON_HEART_MULTI_PARAM is: Instrument for acquisition, analysis, and derivation of heart parameters. |  |
`urn:iso:std:iso:11073:10101` | 69944 | MDC_DEV_MON_LUNG_FUNC | Instrument for acquisition and analysis of lung function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69945 | MDC_DEV_MON_LUNG_FUNC_MDS | Definition for base term 1::4408 MDC_DEV_MON_LUNG_FUNC is: Instrument for acquisition and analysis of lung function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69946 | MDC_DEV_MON_LUNG_FUNC_VMD | Definition for base term 1::4408 MDC_DEV_MON_LUNG_FUNC is: Instrument for acquisition and analysis of lung function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69947 | MDC_DEV_MON_LUNG_FUNC_CHAN | Definition for base term 1::4408 MDC_DEV_MON_LUNG_FUNC is: Instrument for acquisition and analysis of lung function parameters. |  |
`urn:iso:std:iso:11073:10101` | 69948 | MDC_DEV_MON_MUSCL | Instrument that implements a combination of muscle transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 69949 | MDC_DEV_MON_MUSCL_MDS | Definition for base term 1::4412 MDC_DEV_MON_MUSCL is: Instrument that implements a combination of muscle transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 69950 | MDC_DEV_MON_MUSCL_VMD | Definition for base term 1::4412 MDC_DEV_MON_MUSCL is: Instrument that implements a combination of muscle transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 69951 | MDC_DEV_MON_MUSCL_CHAN | Definition for base term 1::4412 MDC_DEV_MON_MUSCL is: Instrument that implements a combination of muscle transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 69952 | MDC_DEV_MON_PT_PHYSIO_MULTI_PARAM | Instrument for direct measurement and analysis of multiple body system parameters. |  |
`urn:iso:std:iso:11073:10101` | 69953 | MDC_DEV_MON_PT_PHYSIO_MULTI_PARAM_MDS | Definition for base term 1::4416 MDC_DEV_MON_PT_PHYSIO_MULTI_PARAM is: Instrument for direct measurement and analysis of multiple body system parameters. |  |
`urn:iso:std:iso:11073:10101` | 69954 | MDC_DEV_MON_PT_PHYSIO_MULTI_PARAM_VMD | Definition for base term 1::4416 MDC_DEV_MON_PT_PHYSIO_MULTI_PARAM is: Instrument for direct measurement and analysis of multiple body system parameters. |  |
`urn:iso:std:iso:11073:10101` | 69955 | MDC_DEV_MON_PT_PHYSIO_MULTI_PARAM_CHAN | Definition for base term 1::4416 MDC_DEV_MON_PT_PHYSIO_MULTI_PARAM is: Instrument for direct measurement and analysis of multiple body system parameters. |  |
`urn:iso:std:iso:11073:10101` | 69956 | MDC_DEV_MON_RENAL_FUNC_MULTI_PARAM | Instrument for renal data acquisition and analysis. |  |
`urn:iso:std:iso:11073:10101` | 69957 | MDC_DEV_MON_RENAL_FUNC_MULTI_PARAM_MDS | Definition for base term 1::4420 MDC_DEV_MON_RENAL_FUNC_MULTI_PARAM is: Instrument for renal data acquisition and analysis. |  |
`urn:iso:std:iso:11073:10101` | 69958 | MDC_DEV_MON_RENAL_FUNC_MULTI_PARAM_VMD | Definition for base term 1::4420 MDC_DEV_MON_RENAL_FUNC_MULTI_PARAM is: Instrument for renal data acquisition and analysis. |  |
`urn:iso:std:iso:11073:10101` | 69959 | MDC_DEV_MON_RENAL_FUNC_MULTI_PARAM_CHAN | Definition for base term 1::4420 MDC_DEV_MON_RENAL_FUNC_MULTI_PARAM is: Instrument for renal data acquisition and analysis. |  |
`urn:iso:std:iso:11073:10101` | 69960 | MDC_DEV_MON_SKIN_MULTI_PARAM | Instrument for direct measurement and analysis of skin-related parameters. |  |
`urn:iso:std:iso:11073:10101` | 69961 | MDC_DEV_MON_SKIN_MULTI_PARAM_MDS | Definition for base term 1::4424 MDC_DEV_MON_SKIN_MULTI_PARAM is: Instrument for direct measurement and analysis of skin-related parameters. |  |
`urn:iso:std:iso:11073:10101` | 69962 | MDC_DEV_MON_SKIN_MULTI_PARAM_VMD | Definition for base term 1::4424 MDC_DEV_MON_SKIN_MULTI_PARAM is: Instrument for direct measurement and analysis of skin-related parameters. |  |
`urn:iso:std:iso:11073:10101` | 69963 | MDC_DEV_MON_SKIN_MULTI_PARAM_CHAN | Definition for base term 1::4424 MDC_DEV_MON_SKIN_MULTI_PARAM is: Instrument for direct measurement and analysis of skin-related parameters. |  |
`urn:iso:std:iso:11073:10101` | 69964 | MDC_DEV_MON_PHYSIO_MULTI_PARAM | Instrument that acquires and analyses patient data from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69965 | MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS | Definition for base term 1::4428 MDC_DEV_MON_PHYSIO_MULTI_PARAM is: Instrument that acquires and analyses patient data from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69966 | MDC_DEV_MON_PHYSIO_MULTI_PARAM_VMD | Definition for base term 1::4428 MDC_DEV_MON_PHYSIO_MULTI_PARAM is: Instrument that acquires and analyses patient data from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69967 | MDC_DEV_MON_PHYSIO_MULTI_PARAM_CHAN | Definition for base term 1::4428 MDC_DEV_MON_PHYSIO_MULTI_PARAM is: Instrument that acquires and analyses patient data from multiple or unspecified body systems. |  |
`urn:iso:std:iso:11073:10101` | 69968 | MDC_DEV_PUMP | Instrument that delivers fluid to the patient. |  |
`urn:iso:std:iso:11073:10101` | 69969 | MDC_DEV_PUMP_MDS | Definition for base term 1::4432 MDC_DEV_PUMP is: Instrument that delivers fluid to the patient. |  |
`urn:iso:std:iso:11073:10101` | 69970 | MDC_DEV_PUMP_VMD | Definition for base term 1::4432 MDC_DEV_PUMP is: Instrument that delivers fluid to the patient. |  |
`urn:iso:std:iso:11073:10101` | 69971 | MDC_DEV_PUMP_CHAN | Definition for base term 1::4432 MDC_DEV_PUMP is: Instrument that delivers fluid to the patient. |  |
`urn:iso:std:iso:11073:10101` | 69972 | MDC_DEV_PUMP_HEART_LUNG | Instrument that implements blood transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 69973 | MDC_DEV_PUMP_HEART_LUNG_MDS | Definition for base term 1::4436 MDC_DEV_PUMP_HEART_LUNG is: Instrument that implements blood transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 69974 | MDC_DEV_PUMP_HEART_LUNG_VMD | Definition for base term 1::4436 MDC_DEV_PUMP_HEART_LUNG is: Instrument that implements blood transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 69975 | MDC_DEV_PUMP_HEART_LUNG_CHAN | Definition for base term 1::4436 MDC_DEV_PUMP_HEART_LUNG is: Instrument that implements blood transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 69976 | MDC_DEV_PUMP_FLOW_HEART | Instrument for modifying the flow of blood from the heart. |  |
`urn:iso:std:iso:11073:10101` | 69977 | MDC_DEV_PUMP_FLOW_HEART_MDS | Definition for base term 1::4440 MDC_DEV_PUMP_FLOW_HEART is: Instrument for modifying the flow of blood from the heart. |  |
`urn:iso:std:iso:11073:10101` | 69978 | MDC_DEV_PUMP_FLOW_HEART_VMD | Definition for base term 1::4440 MDC_DEV_PUMP_FLOW_HEART is: Instrument for modifying the flow of blood from the heart. |  |
`urn:iso:std:iso:11073:10101` | 69979 | MDC_DEV_PUMP_FLOW_HEART_CHAN | Definition for base term 1::4440 MDC_DEV_PUMP_FLOW_HEART is: Instrument for modifying the flow of blood from the heart. |  |
`urn:iso:std:iso:11073:10101` | 69980 | MDC_DEV_PUMP_PRESS_BLD_INTRAAORT | Instrument for improving blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 69981 | MDC_DEV_PUMP_PRESS_BLD_INTRAAORT_MDS | Definition for base term 1::4444 MDC_DEV_PUMP_PRESS_BLD_INTRAAORT is: Instrument for improving blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 69982 | MDC_DEV_PUMP_PRESS_BLD_INTRAAORT_VMD | Definition for base term 1::4444 MDC_DEV_PUMP_PRESS_BLD_INTRAAORT is: Instrument for improving blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 69983 | MDC_DEV_PUMP_PRESS_BLD_INTRAAORT_CHAN | Definition for base term 1::4444 MDC_DEV_PUMP_PRESS_BLD_INTRAAORT is: Instrument for improving blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 69984 | MDC_DEV_PUMP_INFUS | Instrument for delivering a controlled volume of liquids to the blood. |  |
`urn:iso:std:iso:11073:10101` | 69985 | MDC_DEV_PUMP_INFUS_MDS | Definition for base term 1::4448 MDC_DEV_PUMP_INFUS is: Instrument for delivering a controlled volume of liquids to the blood. |  |
`urn:iso:std:iso:11073:10101` | 69986 | MDC_DEV_PUMP_INFUS_VMD | Definition for base term 1::4448 MDC_DEV_PUMP_INFUS is: Instrument for delivering a controlled volume of liquids to the blood. |  |
`urn:iso:std:iso:11073:10101` | 69987 | MDC_DEV_PUMP_INFUS_CHAN | Definition for base term 1::4448 MDC_DEV_PUMP_INFUS is: Instrument for delivering a controlled volume of liquids to the blood. |  |
`urn:iso:std:iso:11073:10101` | 69988 | MDC_DEV_REGUL | Instrument that controls specific aspects of a patient's physiological function. |  |
`urn:iso:std:iso:11073:10101` | 69989 | MDC_DEV_REGUL_MDS | Definition for base term 1::4452 MDC_DEV_REGUL is: Instrument that controls specific aspects of a patient's physiological function. |  |
`urn:iso:std:iso:11073:10101` | 69990 | MDC_DEV_REGUL_VMD | Definition for base term 1::4452 MDC_DEV_REGUL is: Instrument that controls specific aspects of a patient's physiological function. |  |
`urn:iso:std:iso:11073:10101` | 69991 | MDC_DEV_REGUL_CHAN | Definition for base term 1::4452 MDC_DEV_REGUL is: Instrument that controls specific aspects of a patient's physiological function. |  |
`urn:iso:std:iso:11073:10101` | 69992 | MDC_DEV_REGUL_FLOW_AWAY_VENT | Instrument for delivering a controlled flow of airway gas. (i.e., respirator). |  |
`urn:iso:std:iso:11073:10101` | 69993 | MDC_DEV_REGUL_FLOW_AWAY_VENT_MDS | Definition for base term 1::4456 MDC_DEV_REGUL_FLOW_AWAY_VENT is: Instrument for delivering a controlled flow of airway gas. (i.e., respirator). |  |
`urn:iso:std:iso:11073:10101` | 69994 | MDC_DEV_REGUL_FLOW_AWAY_VENT_VMD | Definition for base term 1::4456 MDC_DEV_REGUL_FLOW_AWAY_VENT is: Instrument for delivering a controlled flow of airway gas. (i.e., respirator). |  |
`urn:iso:std:iso:11073:10101` | 69995 | MDC_DEV_REGUL_FLOW_AWAY_VENT_CHAN | Definition for base term 1::4456 MDC_DEV_REGUL_FLOW_AWAY_VENT is: Instrument for delivering a controlled flow of airway gas. (i.e., respirator). |  |
`urn:iso:std:iso:11073:10101` | 69996 | MDC_DEV_REGUL_BLD_CHEM | Instrument for modifying the chemistry of blood. |  |
`urn:iso:std:iso:11073:10101` | 69997 | MDC_DEV_REGUL_BLD_CHEM_MDS | Definition for base term 1::4460 MDC_DEV_REGUL_BLD_CHEM is: Instrument for modifying the chemistry of blood. |  |
`urn:iso:std:iso:11073:10101` | 69998 | MDC_DEV_REGUL_BLD_CHEM_VMD | Definition for base term 1::4460 MDC_DEV_REGUL_BLD_CHEM is: Instrument for modifying the chemistry of blood. |  |
`urn:iso:std:iso:11073:10101` | 69999 | MDC_DEV_REGUL_BLD_CHEM_CHAN | Definition for base term 1::4460 MDC_DEV_REGUL_BLD_CHEM is: Instrument for modifying the chemistry of blood. |  |
`urn:iso:std:iso:11073:10101` | 70000 | MDC_DEV_SYS_PT_VENT | Instrument for data acquisition, analysis and therapy for the lung system. |  |
`urn:iso:std:iso:11073:10101` | 70001 | MDC_DEV_SYS_PT_VENT_MDS | Definition for base term 1::4464 MDC_DEV_SYS_PT_VENT is: Instrument for data acquisition, analysis and therapy for the lung system. |  |
`urn:iso:std:iso:11073:10101` | 70002 | MDC_DEV_SYS_PT_VENT_VMD | Definition for base term 1::4464 MDC_DEV_SYS_PT_VENT is: Instrument for data acquisition, analysis and therapy for the lung system. |  |
`urn:iso:std:iso:11073:10101` | 70003 | MDC_DEV_SYS_PT_VENT_CHAN | Definition for base term 1::4464 MDC_DEV_SYS_PT_VENT is: Instrument for data acquisition, analysis and therapy for the lung system. |  |
`urn:iso:std:iso:11073:10101` | 70004 | MDC_DEV_REGUL_DECOMPRESS | Instrument for sustaining the lungs in a controlled pressure. |  |
`urn:iso:std:iso:11073:10101` | 70005 | MDC_DEV_REGUL_DECOMPRESS_MDS | Definition for base term 1::4468 MDC_DEV_REGUL_DECOMPRESS is: Instrument for sustaining the lungs in a controlled pressure. |  |
`urn:iso:std:iso:11073:10101` | 70006 | MDC_DEV_REGUL_DECOMPRESS_VMD | Definition for base term 1::4468 MDC_DEV_REGUL_DECOMPRESS is: Instrument for sustaining the lungs in a controlled pressure. |  |
`urn:iso:std:iso:11073:10101` | 70007 | MDC_DEV_REGUL_DECOMPRESS_CHAN | Definition for base term 1::4468 MDC_DEV_REGUL_DECOMPRESS is: Instrument for sustaining the lungs in a controlled pressure. |  |
`urn:iso:std:iso:11073:10101` | 70008 | MDC_DEV_REGUL_PRESS_LUNG | Instrument for delivering a controlled flow/volume of airway gas. |  |
`urn:iso:std:iso:11073:10101` | 70009 | MDC_DEV_REGUL_PRESS_LUNG_MDS | Definition for base term 1::4472 MDC_DEV_REGUL_PRESS_LUNG is: Instrument for delivering a controlled flow/volume of airway gas. |  |
`urn:iso:std:iso:11073:10101` | 70010 | MDC_DEV_REGUL_PRESS_LUNG_VMD | Definition for base term 1::4472 MDC_DEV_REGUL_PRESS_LUNG is: Instrument for delivering a controlled flow/volume of airway gas. |  |
`urn:iso:std:iso:11073:10101` | 70011 | MDC_DEV_REGUL_PRESS_LUNG_CHAN | Definition for base term 1::4472 MDC_DEV_REGUL_PRESS_LUNG is: Instrument for delivering a controlled flow/volume of airway gas. |  |
`urn:iso:std:iso:11073:10101` | 70012 | MDC_DEV_REGUL_RATE_VENT | Instrument for controlling the rate of breathing. |  |
`urn:iso:std:iso:11073:10101` | 70013 | MDC_DEV_REGUL_RATE_VENT_MDS | Definition for base term 1::4476 MDC_DEV_REGUL_RATE_VENT is: Instrument for controlling the rate of breathing. |  |
`urn:iso:std:iso:11073:10101` | 70014 | MDC_DEV_REGUL_RATE_VENT_VMD | Definition for base term 1::4476 MDC_DEV_REGUL_RATE_VENT is: Instrument for controlling the rate of breathing. |  |
`urn:iso:std:iso:11073:10101` | 70015 | MDC_DEV_REGUL_RATE_VENT_CHAN | Definition for base term 1::4476 MDC_DEV_REGUL_RATE_VENT is: Instrument for controlling the rate of breathing. |  |
`urn:iso:std:iso:11073:10101` | 70016 | MDC_DEV_REGUL_TEMP_BLD | Instrument for delivering a controlled temperature of blood. |  |
`urn:iso:std:iso:11073:10101` | 70017 | MDC_DEV_REGUL_TEMP_BLD_MDS | Definition for base term 1::4480 MDC_DEV_REGUL_TEMP_BLD is: Instrument for delivering a controlled temperature of blood. |  |
`urn:iso:std:iso:11073:10101` | 70018 | MDC_DEV_REGUL_TEMP_BLD_VMD | Definition for base term 1::4480 MDC_DEV_REGUL_TEMP_BLD is: Instrument for delivering a controlled temperature of blood. |  |
`urn:iso:std:iso:11073:10101` | 70019 | MDC_DEV_REGUL_TEMP_BLD_CHAN | Definition for base term 1::4480 MDC_DEV_REGUL_TEMP_BLD is: Instrument for delivering a controlled temperature of blood. |  |
`urn:iso:std:iso:11073:10101` | 70020 | MDC_DEV_REGUL_TEMP_SKIN | Instrument for modifying the temperature of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70021 | MDC_DEV_REGUL_TEMP_SKIN_MDS | Definition for base term 1::4484 MDC_DEV_REGUL_TEMP_SKIN is: Instrument for modifying the temperature of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70022 | MDC_DEV_REGUL_TEMP_SKIN_VMD | Definition for base term 1::4484 MDC_DEV_REGUL_TEMP_SKIN is: Instrument for modifying the temperature of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70023 | MDC_DEV_REGUL_TEMP_SKIN_CHAN | Definition for base term 1::4484 MDC_DEV_REGUL_TEMP_SKIN is: Instrument for modifying the temperature of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70024 | MDC_DEV_REGUL_VOL_VENT | Instrument for delivering a controlled volume of airway gas. |  |
`urn:iso:std:iso:11073:10101` | 70025 | MDC_DEV_REGUL_VOL_VENT_MDS | Definition for base term 1::4488 MDC_DEV_REGUL_VOL_VENT is: Instrument for delivering a controlled volume of airway gas. |  |
`urn:iso:std:iso:11073:10101` | 70026 | MDC_DEV_REGUL_VOL_VENT_VMD | Definition for base term 1::4488 MDC_DEV_REGUL_VOL_VENT is: Instrument for delivering a controlled volume of airway gas. |  |
`urn:iso:std:iso:11073:10101` | 70027 | MDC_DEV_REGUL_VOL_VENT_CHAN | Definition for base term 1::4488 MDC_DEV_REGUL_VOL_VENT is: Instrument for delivering a controlled volume of airway gas. |  |
`urn:iso:std:iso:11073:10101` | 70028 | MDC_DEV_SYS_MULTI_MODAL | Instrument that consists of multiple device modalities. |  |
`urn:iso:std:iso:11073:10101` | 70029 | MDC_DEV_SYS_MULTI_MODAL_MDS | Definition for base term 1::4492 MDC_DEV_SYS_MULTI_MODAL is: Instrument that consists of multiple device modalities. |  |
`urn:iso:std:iso:11073:10101` | 70030 | MDC_DEV_SYS_MULTI_MODAL_VMD | Definition for base term 1::4492 MDC_DEV_SYS_MULTI_MODAL is: Instrument that consists of multiple device modalities. |  |
`urn:iso:std:iso:11073:10101` | 70031 | MDC_DEV_SYS_MULTI_MODAL_CHAN | Definition for base term 1::4492 MDC_DEV_SYS_MULTI_MODAL is: Instrument that consists of multiple device modalities. |  |
`urn:iso:std:iso:11073:10101` | 70032 | MDC_DEV_SYS_BRAIN_MULTI_PARAM | Instrument that implements brain transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 70033 | MDC_DEV_SYS_BRAIN_MULTI_PARAM_MDS | Definition for base term 1::4496 MDC_DEV_SYS_BRAIN_MULTI_PARAM is: Instrument that implements brain transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 70034 | MDC_DEV_SYS_BRAIN_MULTI_PARAM_VMD | Definition for base term 1::4496 MDC_DEV_SYS_BRAIN_MULTI_PARAM is: Instrument that implements brain transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 70035 | MDC_DEV_SYS_BRAIN_MULTI_PARAM_CHAN | Definition for base term 1::4496 MDC_DEV_SYS_BRAIN_MULTI_PARAM is: Instrument that implements brain transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 70036 | MDC_DEV_SYS_CARD_MULTI_PARAM | Instrument for heart transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 70037 | MDC_DEV_SYS_CARD_MULTI_PARAM_MDS | Definition for base term 1::4500 MDC_DEV_SYS_CARD_MULTI_PARAM is: Instrument for heart transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 70038 | MDC_DEV_SYS_CARD_MULTI_PARAM_VMD | Definition for base term 1::4500 MDC_DEV_SYS_CARD_MULTI_PARAM is: Instrument for heart transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 70039 | MDC_DEV_SYS_CARD_MULTI_PARAM_CHAN | Definition for base term 1::4500 MDC_DEV_SYS_CARD_MULTI_PARAM is: Instrument for heart transduction, analysis, and therapy. |  |
`urn:iso:std:iso:11073:10101` | 70040 | MDC_DEV_SYS_ANESTH | Instrument that implements a combination of transduction, analysis, and/or therapy on multiple body systems. |  |
`urn:iso:std:iso:11073:10101` | 70041 | MDC_DEV_SYS_ANESTH_MDS | Definition for base term 1::4504 MDC_DEV_SYS_ANESTH is: Instrument that implements a combination of transduction, analysis, and/or therapy on multiple body systems. |  |
`urn:iso:std:iso:11073:10101` | 70042 | MDC_DEV_SYS_ANESTH_VMD | Definition for base term 1::4504 MDC_DEV_SYS_ANESTH is: Instrument that implements a combination of transduction, analysis, and/or therapy on multiple body systems. |  |
`urn:iso:std:iso:11073:10101` | 70043 | MDC_DEV_SYS_ANESTH_CHAN | Definition for base term 1::4504 MDC_DEV_SYS_ANESTH is: Instrument that implements a combination of transduction, analysis, and/or therapy on multiple body systems. |  |
`urn:iso:std:iso:11073:10101` | 70044 | MDC_DEV_SYS_PHYSIO_MULTI_PARAM | Instrument that acquires, analyses, and provides therapy from and to multiple or unspecified body systems |  |
`urn:iso:std:iso:11073:10101` | 70045 | MDC_DEV_SYS_PHYSIO_MULTI_PARAM_MDS | Definition for base term 1::4508 MDC_DEV_SYS_PHYSIO_MULTI_PARAM is: Instrument that acquires, analyses, and provides therapy from and to multiple or unspecified body systems |  |
`urn:iso:std:iso:11073:10101` | 70046 | MDC_DEV_SYS_PHYSIO_MULTI_PARAM_VMD | Definition for base term 1::4508 MDC_DEV_SYS_PHYSIO_MULTI_PARAM is: Instrument that acquires, analyses, and provides therapy from and to multiple or unspecified body systems |  |
`urn:iso:std:iso:11073:10101` | 70047 | MDC_DEV_SYS_PHYSIO_MULTI_PARAM_CHAN | Definition for base term 1::4508 MDC_DEV_SYS_PHYSIO_MULTI_PARAM is: Instrument that acquires, analyses, and provides therapy from and to multiple or unspecified body systems |  |
`urn:iso:std:iso:11073:10101` | 70656 | MDC_DEV_GENERAL | Generic device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70657 | MDC_DEV_GENERAL_MDS | Definition for base term 1::5120 MDC_DEV_GENERAL is: Generic device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70658 | MDC_DEV_GENERAL_VMD | Definition for base term 1::5120 MDC_DEV_GENERAL is: Generic device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70659 | MDC_DEV_GENERAL_CHAN | Definition for base term 1::5120 MDC_DEV_GENERAL is: Generic device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70660 | MDC_DEV_AUX | Generic device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70661 | MDC_DEV_AUX_MDS | Definition for base term 1::5124 MDC_DEV_AUX is: Generic device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70662 | MDC_DEV_AUX_VMD | Definition for base term 1::5124 MDC_DEV_AUX is: Generic device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70663 | MDC_DEV_AUX_CHAN | Definition for base term 1::5124 MDC_DEV_AUX is: Generic device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70664 | MDC_DEV_ECG_RESP | Instrument for the indirect measurement of respiration rate by estimating transthoracic impedance using the ECG leads. |  |
`urn:iso:std:iso:11073:10101` | 70665 | MDC_DEV_ECG_RESP_MDS | Definition for base term 1::5128 MDC_DEV_ECG_RESP is: Instrument for the indirect measurement of respiration rate by estimating transthoracic impedance using the ECG leads. |  |
`urn:iso:std:iso:11073:10101` | 70666 | MDC_DEV_ECG_RESP_VMD | Definition for base term 1::5128 MDC_DEV_ECG_RESP is: Instrument for the indirect measurement of respiration rate by estimating transthoracic impedance using the ECG leads. |  |
`urn:iso:std:iso:11073:10101` | 70667 | MDC_DEV_ECG_RESP_CHAN | Definition for base term 1::5128 MDC_DEV_ECG_RESP is: Instrument for the indirect measurement of respiration rate by estimating transthoracic impedance using the ECG leads. |  |
`urn:iso:std:iso:11073:10101` | 70668 | MDC_DEV_ARRHY | Instrument for acquisition, analysis and detection of cardiac arrhythmias or conduction disturbances. |  |
`urn:iso:std:iso:11073:10101` | 70669 | MDC_DEV_ARRHY_MDS | Definition for base term 1::5132 MDC_DEV_ARRHY is: Instrument for acquisition, analysis and detection of cardiac arrhythmias or conduction disturbances. |  |
`urn:iso:std:iso:11073:10101` | 70670 | MDC_DEV_ARRHY_VMD | Definition for base term 1::5132 MDC_DEV_ARRHY is: Instrument for acquisition, analysis and detection of cardiac arrhythmias or conduction disturbances. |  |
`urn:iso:std:iso:11073:10101` | 70671 | MDC_DEV_ARRHY_CHAN | Definition for base term 1::5132 MDC_DEV_ARRHY is: Instrument for acquisition, analysis and detection of cardiac arrhythmias or conduction disturbances. |  |
`urn:iso:std:iso:11073:10101` | 70672 | MDC_DEV_PULS | Instrument for acquisition, analysis and detection of haemodynamic pulse rate and other information. |  |
`urn:iso:std:iso:11073:10101` | 70673 | MDC_DEV_PULS_MDS | Definition for base term 1::5136 MDC_DEV_PULS is: Instrument for acquisition, analysis and detection of haemodynamic pulse rate and other information. |  |
`urn:iso:std:iso:11073:10101` | 70674 | MDC_DEV_PULS_VMD | Definition for base term 1::5136 MDC_DEV_PULS is: Instrument for acquisition, analysis and detection of haemodynamic pulse rate and other information. |  |
`urn:iso:std:iso:11073:10101` | 70675 | MDC_DEV_PULS_CHAN | Definition for base term 1::5136 MDC_DEV_PULS is: Instrument for acquisition, analysis and detection of haemodynamic pulse rate and other information. |  |
`urn:iso:std:iso:11073:10101` | 70676 | MDC_DEV_ST | Instrument for acquisition, analysis and detection of ST deviation and cardiac repolarization disturbances. |  |
`urn:iso:std:iso:11073:10101` | 70677 | MDC_DEV_ST_MDS | Definition for base term 1::5140 MDC_DEV_ST is: Instrument for acquisition, analysis and detection of ST deviation and cardiac repolarization disturbances. |  |
`urn:iso:std:iso:11073:10101` | 70678 | MDC_DEV_ST_VMD | Definition for base term 1::5140 MDC_DEV_ST is: Instrument for acquisition, analysis and detection of ST deviation and cardiac repolarization disturbances. |  |
`urn:iso:std:iso:11073:10101` | 70679 | MDC_DEV_ST_CHAN | Definition for base term 1::5140 MDC_DEV_ST is: Instrument for acquisition, analysis and detection of ST deviation and cardiac repolarization disturbances. |  |
`urn:iso:std:iso:11073:10101` | 70680 | MDC_DEV_CO2 | Instrument for the direct measurement of airway CO2 concentration and respiration rate. |  |
`urn:iso:std:iso:11073:10101` | 70681 | MDC_DEV_CO2_MDS | Definition for base term 1::5144 MDC_DEV_CO2 is: Instrument for the direct measurement of airway CO2 concentration and respiration rate. |  |
`urn:iso:std:iso:11073:10101` | 70682 | MDC_DEV_CO2_VMD | Definition for base term 1::5144 MDC_DEV_CO2 is: Instrument for the direct measurement of airway CO2 concentration and respiration rate. |  |
`urn:iso:std:iso:11073:10101` | 70683 | MDC_DEV_CO2_CHAN | Definition for base term 1::5144 MDC_DEV_CO2 is: Instrument for the direct measurement of airway CO2 concentration and respiration rate. |  |
`urn:iso:std:iso:11073:10101` | 70684 | MDC_DEV_PRESS_BLD_NONINV | Instrument for the non-invasive measurement of blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 70685 | MDC_DEV_PRESS_BLD_NONINV_MDS | Definition for base term 1::5148 MDC_DEV_PRESS_BLD_NONINV is: Instrument for the non-invasive measurement of blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 70686 | MDC_DEV_PRESS_BLD_NONINV_VMD | Definition for base term 1::5148 MDC_DEV_PRESS_BLD_NONINV is: Instrument for the non-invasive measurement of blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 70687 | MDC_DEV_PRESS_BLD_NONINV_CHAN | Definition for base term 1::5148 MDC_DEV_PRESS_BLD_NONINV is: Instrument for the non-invasive measurement of blood pressure. |  |
`urn:iso:std:iso:11073:10101` | 70688 | MDC_DEV_CEREB_PERF | Instrument for the measurement of the level of blood perfusion in cerebral tissue. |  |
`urn:iso:std:iso:11073:10101` | 70689 | MDC_DEV_CEREB_PERF_MDS | Definition for base term 1::5152 MDC_DEV_CEREB_PERF is: Instrument for the measurement of the level of blood perfusion in cerebral tissue. |  |
`urn:iso:std:iso:11073:10101` | 70690 | MDC_DEV_CEREB_PERF_VMD | Definition for base term 1::5152 MDC_DEV_CEREB_PERF is: Instrument for the measurement of the level of blood perfusion in cerebral tissue. |  |
`urn:iso:std:iso:11073:10101` | 70691 | MDC_DEV_CEREB_PERF_CHAN | Definition for base term 1::5152 MDC_DEV_CEREB_PERF is: Instrument for the measurement of the level of blood perfusion in cerebral tissue. |  |
`urn:iso:std:iso:11073:10101` | 70692 | MDC_DEV_CO2_CTS | Instrument for the direct and continuous measurement of CO2 concentration or partial pressure. |  |
`urn:iso:std:iso:11073:10101` | 70693 | MDC_DEV_CO2_CTS_MDS | Definition for base term 1::5156 MDC_DEV_CO2_CTS is: Instrument for the direct and continuous measurement of CO2 concentration or partial pressure. |  |
`urn:iso:std:iso:11073:10101` | 70694 | MDC_DEV_CO2_CTS_VMD | Definition for base term 1::5156 MDC_DEV_CO2_CTS is: Instrument for the direct and continuous measurement of CO2 concentration or partial pressure. |  |
`urn:iso:std:iso:11073:10101` | 70695 | MDC_DEV_CO2_CTS_CHAN | Definition for base term 1::5156 MDC_DEV_CO2_CTS is: Instrument for the direct and continuous measurement of CO2 concentration or partial pressure. |  |
`urn:iso:std:iso:11073:10101` | 70696 | MDC_DEV_CO2_TCUT | Instrument for the indirect measurement of pCO2 partial pressure on the surface of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70697 | MDC_DEV_CO2_TCUT_MDS | Definition for base term 1::5160 MDC_DEV_CO2_TCUT is: Instrument for the indirect measurement of pCO2 partial pressure on the surface of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70698 | MDC_DEV_CO2_TCUT_VMD | Definition for base term 1::5160 MDC_DEV_CO2_TCUT is: Instrument for the indirect measurement of pCO2 partial pressure on the surface of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70699 | MDC_DEV_CO2_TCUT_CHAN | Definition for base term 1::5160 MDC_DEV_CO2_TCUT is: Instrument for the indirect measurement of pCO2 partial pressure on the surface of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70700 | MDC_DEV_O2 | Instrument for the direct measurement of airway O2 concentration and respiration rate. |  |
`urn:iso:std:iso:11073:10101` | 70701 | MDC_DEV_O2_MDS | Definition for base term 1::5164 MDC_DEV_O2 is: Instrument for the direct measurement of airway O2 concentration and respiration rate. |  |
`urn:iso:std:iso:11073:10101` | 70702 | MDC_DEV_O2_VMD | Definition for base term 1::5164 MDC_DEV_O2 is: Instrument for the direct measurement of airway O2 concentration and respiration rate. |  |
`urn:iso:std:iso:11073:10101` | 70703 | MDC_DEV_O2_CHAN | Definition for base term 1::5164 MDC_DEV_O2 is: Instrument for the direct measurement of airway O2 concentration and respiration rate. |  |
`urn:iso:std:iso:11073:10101` | 70704 | MDC_DEV_O2_CTS | Instrument for the direct and continuous measurement of O2 concentration or partial pressure. |  |
`urn:iso:std:iso:11073:10101` | 70705 | MDC_DEV_O2_CTS_MDS | Definition for base term 1::5168 MDC_DEV_O2_CTS is: Instrument for the direct and continuous measurement of O2 concentration or partial pressure. |  |
`urn:iso:std:iso:11073:10101` | 70706 | MDC_DEV_O2_CTS_VMD | Definition for base term 1::5168 MDC_DEV_O2_CTS is: Instrument for the direct and continuous measurement of O2 concentration or partial pressure. |  |
`urn:iso:std:iso:11073:10101` | 70707 | MDC_DEV_O2_CTS_CHAN | Definition for base term 1::5168 MDC_DEV_O2_CTS is: Instrument for the direct and continuous measurement of O2 concentration or partial pressure. |  |
`urn:iso:std:iso:11073:10101` | 70708 | MDC_DEV_O2_TCUT | Instrument for the indirect measurement of pO2 partial pressure on the surface of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70709 | MDC_DEV_O2_TCUT_MDS | Definition for base term 1::5172 MDC_DEV_O2_TCUT is: Instrument for the indirect measurement of pO2 partial pressure on the surface of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70710 | MDC_DEV_O2_TCUT_VMD | Definition for base term 1::5172 MDC_DEV_O2_TCUT is: Instrument for the indirect measurement of pO2 partial pressure on the surface of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70711 | MDC_DEV_O2_TCUT_CHAN | Definition for base term 1::5172 MDC_DEV_O2_TCUT is: Instrument for the indirect measurement of pO2 partial pressure on the surface of the skin. |  |
`urn:iso:std:iso:11073:10101` | 70712 | MDC_DEV_TEMP_DIFF | Instrument that measures temperature difference between two body sites or temperature reference. |  |
`urn:iso:std:iso:11073:10101` | 70713 | MDC_DEV_TEMP_DIFF_MDS | Definition for base term 1::5176 MDC_DEV_TEMP_DIFF is: Instrument that measures temperature difference between two body sites or temperature reference. |  |
`urn:iso:std:iso:11073:10101` | 70714 | MDC_DEV_TEMP_DIFF_VMD | Definition for base term 1::5176 MDC_DEV_TEMP_DIFF is: Instrument that measures temperature difference between two body sites or temperature reference. |  |
`urn:iso:std:iso:11073:10101` | 70715 | MDC_DEV_TEMP_DIFF_CHAN | Definition for base term 1::5176 MDC_DEV_TEMP_DIFF is: Instrument that measures temperature difference between two body sites or temperature reference. |  |
`urn:iso:std:iso:11073:10101` | 70716 | MDC_DEV_CNTRL | Instrument that controls specific aspects of a device. |  |
`urn:iso:std:iso:11073:10101` | 70717 | MDC_DEV_CNTRL_MDS | Definition for base term 1::5180 MDC_DEV_CNTRL is: Instrument that controls specific aspects of a device. |  |
`urn:iso:std:iso:11073:10101` | 70718 | MDC_DEV_CNTRL_VMD | Definition for base term 1::5180 MDC_DEV_CNTRL is: Instrument that controls specific aspects of a device. |  |
`urn:iso:std:iso:11073:10101` | 70719 | MDC_DEV_CNTRL_CHAN | Definition for base term 1::5180 MDC_DEV_CNTRL is: Instrument that controls specific aspects of a device. |  |
`urn:iso:std:iso:11073:10101` | 70720 | MDC_DEV_AL | Instrument that processes or annunciates an alarm. |  |
`urn:iso:std:iso:11073:10101` | 70721 | MDC_DEV_AL_MDS | Definition for base term 1::5184 MDC_DEV_AL is: Instrument that processes or annunciates an alarm. |  |
`urn:iso:std:iso:11073:10101` | 70722 | MDC_DEV_AL_VMD | Definition for base term 1::5184 MDC_DEV_AL is: Instrument that processes or annunciates an alarm. |  |
`urn:iso:std:iso:11073:10101` | 70723 | MDC_DEV_AL_CHAN | Definition for base term 1::5184 MDC_DEV_AL is: Instrument that processes or annunciates an alarm. |  |
`urn:iso:std:iso:11073:10101` | 70724 | MDC_DEV_WEDGE | Instrument for the direct measurement of the pulmonary artery wedge pressure. |  |
`urn:iso:std:iso:11073:10101` | 70725 | MDC_DEV_WEDGE_MDS | Definition for base term 1::5188 MDC_DEV_WEDGE is: Instrument for the direct measurement of the pulmonary artery wedge pressure. |  |
`urn:iso:std:iso:11073:10101` | 70726 | MDC_DEV_WEDGE_VMD | Definition for base term 1::5188 MDC_DEV_WEDGE is: Instrument for the direct measurement of the pulmonary artery wedge pressure. |  |
`urn:iso:std:iso:11073:10101` | 70727 | MDC_DEV_WEDGE_CHAN | Definition for base term 1::5188 MDC_DEV_WEDGE is: Instrument for the direct measurement of the pulmonary artery wedge pressure. |  |
`urn:iso:std:iso:11073:10101` | 70728 | MDC_DEV_O2_VEN_SAT | Instrument that derives the % of venous O2. |  |
`urn:iso:std:iso:11073:10101` | 70729 | MDC_DEV_O2_VEN_SAT_MDS | Definition for base term 1::5192 MDC_DEV_O2_VEN_SAT is: Instrument that derives the % of venous O2. |  |
`urn:iso:std:iso:11073:10101` | 70730 | MDC_DEV_O2_VEN_SAT_VMD | Definition for base term 1::5192 MDC_DEV_O2_VEN_SAT is: Instrument that derives the % of venous O2. |  |
`urn:iso:std:iso:11073:10101` | 70731 | MDC_DEV_O2_VEN_SAT_CHAN | Definition for base term 1::5192 MDC_DEV_O2_VEN_SAT is: Instrument that derives the % of venous O2. |  |
`urn:iso:std:iso:11073:10101` | 70732 | MDC_DEV_PMSTORE | Device that stores physiologic information. |  |
`urn:iso:std:iso:11073:10101` | 70733 | MDC_DEV_PMSTORE_MDS | Definition for base term 1::5196 MDC_DEV_PMSTORE is: Device that stores physiologic information. |  |
`urn:iso:std:iso:11073:10101` | 70734 | MDC_DEV_PMSTORE_VMD | Definition for base term 1::5196 MDC_DEV_PMSTORE is: Device that stores physiologic information. |  |
`urn:iso:std:iso:11073:10101` | 70735 | MDC_DEV_PMSTORE_CHAN | Definition for base term 1::5196 MDC_DEV_PMSTORE is: Device that stores physiologic information. |  |
`urn:iso:std:iso:11073:10101` | 70736 | MDC_DEV_CARD_RATE | Instrument for measuring the rate of heart contractions. |  |
`urn:iso:std:iso:11073:10101` | 70737 | MDC_DEV_CARD_RATE_MDS | Definition for base term 1::5200 MDC_DEV_CARD_RATE is: Instrument for measuring the rate of heart contractions. |  |
`urn:iso:std:iso:11073:10101` | 70738 | MDC_DEV_CARD_RATE_VMD | Definition for base term 1::5200 MDC_DEV_CARD_RATE is: Instrument for measuring the rate of heart contractions. |  |
`urn:iso:std:iso:11073:10101` | 70739 | MDC_DEV_CARD_RATE_CHAN | Definition for base term 1::5200 MDC_DEV_CARD_RATE is: Instrument for measuring the rate of heart contractions. |  |
`urn:iso:std:iso:11073:10101` | 70740 | MDC_DEV_SYS_VS | Instrument for direct measurement and analysis of vital signs such as temperature, pulse or heart rate, blood pressure and respiratory rate. |  |
`urn:iso:std:iso:11073:10101` | 70741 | MDC_DEV_SYS_VS_MDS | Definition for base term 1::5204 MDC_DEV_SYS_VS is: Instrument for direct measurement and analysis of vital signs such as temperature, pulse or heart rate, blood pressure and respiratory rate. |  |
`urn:iso:std:iso:11073:10101` | 70742 | MDC_DEV_SYS_VS_VMD | Definition for base term 1::5204 MDC_DEV_SYS_VS is: Instrument for direct measurement and analysis of vital signs such as temperature, pulse or heart rate, blood pressure and respiratory rate. |  |
`urn:iso:std:iso:11073:10101` | 70743 | MDC_DEV_SYS_VS_CHAN | Definition for base term 1::5204 MDC_DEV_SYS_VS is: Instrument for direct measurement and analysis of vital signs such as temperature, pulse or heart rate, blood pressure and respiratory rate. |  |
`urn:iso:std:iso:11073:10101` | 70744 | MDC_DEV_SYS_VS_CONFIG | Configurable (modular) instrument for direct measurement and analysis of vital signs. |  |
`urn:iso:std:iso:11073:10101` | 70745 | MDC_DEV_SYS_VS_CONFIG_MDS | Definition for base term 1::5208 MDC_DEV_SYS_VS_CONFIG is: Configurable (modular) instrument for direct measurement and analysis of vital signs. |  |
`urn:iso:std:iso:11073:10101` | 70746 | MDC_DEV_SYS_VS_CONFIG_VMD | Definition for base term 1::5208 MDC_DEV_SYS_VS_CONFIG is: Configurable (modular) instrument for direct measurement and analysis of vital signs. |  |
`urn:iso:std:iso:11073:10101` | 70747 | MDC_DEV_SYS_VS_CONFIG_CHAN | Definition for base term 1::5208 MDC_DEV_SYS_VS_CONFIG is: Configurable (modular) instrument for direct measurement and analysis of vital signs. |  |
`urn:iso:std:iso:11073:10101` | 70748 | MDC_DEV_SYS_VS_UNCONFIG | Non-configurable (fixed functionality) instrument for direct measurement and analysis of vital signs. |  |
`urn:iso:std:iso:11073:10101` | 70749 | MDC_DEV_SYS_VS_UNCONFIG_MDS | Definition for base term 1::5212 MDC_DEV_SYS_VS_UNCONFIG is: Non-configurable (fixed functionality) instrument for direct measurement and analysis of vital signs. |  |
`urn:iso:std:iso:11073:10101` | 70750 | MDC_DEV_SYS_VS_UNCONFIG_VMD | Definition for base term 1::5212 MDC_DEV_SYS_VS_UNCONFIG is: Non-configurable (fixed functionality) instrument for direct measurement and analysis of vital signs. |  |
`urn:iso:std:iso:11073:10101` | 70751 | MDC_DEV_SYS_VS_UNCONFIG_CHAN | Definition for base term 1::5212 MDC_DEV_SYS_VS_UNCONFIG is: Non-configurable (fixed functionality) instrument for direct measurement and analysis of vital signs. |  |
`urn:iso:std:iso:11073:10101` | 70752 | MDC_DEV_AL_STAT | Instrument displays alarm status. |  |
`urn:iso:std:iso:11073:10101` | 70753 | MDC_DEV_AL_STAT_MDS | Definition for base term 1::5216 MDC_DEV_AL_STAT is: Instrument displays alarm status. |  |
`urn:iso:std:iso:11073:10101` | 70754 | MDC_DEV_AL_STAT_VMD | Definition for base term 1::5216 MDC_DEV_AL_STAT is: Instrument displays alarm status. |  |
`urn:iso:std:iso:11073:10101` | 70755 | MDC_DEV_AL_STAT_CHAN | Definition for base term 1::5216 MDC_DEV_AL_STAT is: Instrument displays alarm status. |  |
`urn:iso:std:iso:11073:10101` | 70756 | MDC_DEV_WV_GENERAL | Generic waveform device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70757 | MDC_DEV_WV_GENERAL_MDS | Definition for base term 1::5220 MDC_DEV_WV_GENERAL is: Generic waveform device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70758 | MDC_DEV_WV_GENERAL_VMD | Definition for base term 1::5220 MDC_DEV_WV_GENERAL is: Generic waveform device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70759 | MDC_DEV_WV_GENERAL_CHAN | Definition for base term 1::5220 MDC_DEV_WV_GENERAL is: Generic waveform device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70760 | MDC_DEV_NU_GENERAL | Generic numeric device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70761 | MDC_DEV_NU_GENERAL_MDS | Definition for base term 1::5224 MDC_DEV_NU_GENERAL is: Generic numeric device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70762 | MDC_DEV_NU_GENERAL_VMD | Definition for base term 1::5224 MDC_DEV_NU_GENERAL is: Generic numeric device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70763 | MDC_DEV_NU_GENERAL_CHAN | Definition for base term 1::5224 MDC_DEV_NU_GENERAL is: Generic numeric device, of any type. |  |
`urn:iso:std:iso:11073:10101` | 70764 | MDC_DEV_METER_PRESS | Instrument or sensor for the direct measurement of pressure. |  |
`urn:iso:std:iso:11073:10101` | 70765 | MDC_DEV_METER_PRESS_MDS | Definition for base term 1::5228 MDC_DEV_METER_PRESS is: Instrument or sensor for the direct measurement of pressure. |  |
`urn:iso:std:iso:11073:10101` | 70766 | MDC_DEV_METER_PRESS_VMD | Definition for base term 1::5228 MDC_DEV_METER_PRESS is: Instrument or sensor for the direct measurement of pressure. |  |
`urn:iso:std:iso:11073:10101` | 70767 | MDC_DEV_METER_PRESS_CHAN | Definition for base term 1::5228 MDC_DEV_METER_PRESS is: Instrument or sensor for the direct measurement of pressure. |  |
`urn:iso:std:iso:11073:10101` | 70768 | MDC_DEV_ANALY_PERF_REL | Instrument for the measurement of blood perfusion. |  |
`urn:iso:std:iso:11073:10101` | 70769 | MDC_DEV_ANALY_PERF_REL_MDS | Definition for base term 1::5232 MDC_DEV_ANALY_PERF_REL is: Instrument for the measurement of blood perfusion. |  |
`urn:iso:std:iso:11073:10101` | 70770 | MDC_DEV_ANALY_PERF_REL_VMD | Definition for base term 1::5232 MDC_DEV_ANALY_PERF_REL is: Instrument for the measurement of blood perfusion. |  |
`urn:iso:std:iso:11073:10101` | 70771 | MDC_DEV_ANALY_PERF_REL_CHAN | Definition for base term 1::5232 MDC_DEV_ANALY_PERF_REL is: Instrument for the measurement of blood perfusion. |  |
`urn:iso:std:iso:11073:10101` | 70772 | MDC_DEV_PLETH | Instrument for measuring changes in volume within an organ or body part due to fluctuations in the amount of blood or air it contains. |  |
`urn:iso:std:iso:11073:10101` | 70773 | MDC_DEV_PLETH_MDS | Definition for base term 1::5236 MDC_DEV_PLETH is: Instrument for measuring changes in volume within an organ or body part due to fluctuations in the amount of blood or air it contains. |  |
`urn:iso:std:iso:11073:10101` | 70774 | MDC_DEV_PLETH_VMD | Definition for base term 1::5236 MDC_DEV_PLETH is: Instrument for measuring changes in volume within an organ or body part due to fluctuations in the amount of blood or air it contains. |  |
`urn:iso:std:iso:11073:10101` | 70775 | MDC_DEV_PLETH_CHAN | Definition for base term 1::5236 MDC_DEV_PLETH is: Instrument for measuring changes in volume within an organ or body part due to fluctuations in the amount of blood or air it contains. |  |
`urn:iso:std:iso:11073:10101` | 70776 | MDC_DEV_CALC_CARD | Instrument that derives cardiac parameters. |  |
`urn:iso:std:iso:11073:10101` | 70780 | MDC_DEV_CALC_PULM | Instrument that derives pulmonary parameters. |  |
`urn:iso:std:iso:11073:10101` | 70784 | MDC_DEV_CALC_PULM_EST | Instrument that derives pulmonary parameters, where one or more inputs to the calculation may be clinically acceptable approximations or alternative values. |  |
`urn:iso:std:iso:11073:10101` | 70788 | MDC_DEV_ANALY_SAT_O2_ART | Instrument that derives the % of arterial O2 and pulse rate parameters (blood flow) and other analytes. |  |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code