Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Measurement status codes - JSON Representation

Page standards status: Trial-use | Maturity Level: 2

Raw json | Download

    {
      "resourceType" : "CodeSystem",
      "id" : "measurement-status",
      "meta" : {
        "profile" : [
          🔗 "http://hl7.org/fhir/StructureDefinition/shareablecodesystem"
        ]
      },
      "text" : {
        "status" : "generated",
        "div" : "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p class=\"res-header-id\"><b>Generated Narrative: CodeSystem measurement-status</b></p><a name=\"measurement-status\"> </a><a name=\"hcmeasurement-status\"> </a><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\"/><p style=\"margin-bottom: 0px\">Profile: <a href=\"http://hl7.org/fhir/R4/shareablecodesystem.html\">Shareable CodeSystem</a></p></div><p>This case-insensitive code system <code>http://terminology.hl7.org/CodeSystem/measurement-status</code> defines the following codes:</p><table class=\"codes\"><tr><td style=\"white-space:nowrap\"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style=\"white-space:nowrap\">questionable<a name=\"measurement-status-questionable\"> </a></td><td>Questionable</td><td>Data may not be reliable</td></tr><tr><td style=\"white-space:nowrap\">calibration-ongoing<a name=\"measurement-status-calibration-ongoing\"> </a></td><td>Calibration ongoing</td><td>Calibration is ongoing</td></tr><tr><td style=\"white-space:nowrap\">validated-data<a name=\"measurement-status-validated-data\"> </a></td><td>Validated data</td><td>Relevant, e.g., in an archive</td></tr><tr><td style=\"white-space:nowrap\">early-indication<a name=\"measurement-status-early-indication\"> </a></td><td>Early indication</td><td>Early estimate of value</td></tr><tr><td style=\"white-space:nowrap\">msmt-ongoing<a name=\"measurement-status-msmt-ongoing\"> </a></td><td>Measurement ongoing</td><td>Indicates that a new measurement is just being taken</td></tr><tr><td style=\"white-space:nowrap\">in-alarm<a name=\"measurement-status-in-alarm\"> </a></td><td>Measurement in alarm</td><td>Measurement has an active alarm condition</td></tr><tr><td style=\"white-space:nowrap\">alarm-inhibited<a name=\"measurement-status-alarm-inhibited\"> </a></td><td>Measurement alarms inhibited</td><td>Measurement supports alarming and alarms are turned off</td></tr></table></div>"
      },
      "extension" : [
        {
          "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-wg",
          "valueCode" : "dev"
        },
        {
          "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-fmm",
          "valueInteger" : 2,
          "_valueInteger" : {
            "extension" : [
              {
                "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
                "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
              }
            ]
          }
        },
        {
          "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-standards-status",
          "valueCode" : "trial-use",
          "_valueCode" : {
            "extension" : [
              {
                "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
                "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
              }
            ]
          }
        }
      ],
      "url" : "http://terminology.hl7.org/CodeSystem/measurement-status",
      "version" : "1.0.0",
      "name" : "MeasurementStatus",
      "title" : "Measurement status codes",
      "status" : "active",
      "experimental" : false,
      "date" : "2019-09-28",
      "publisher" : "HL7 International / Devices",
      "contact" : [
        {
          "telecom" : [
            {
              "system" : "url",
              "value" : "http://www.hl7.org/Special/committees/healthcaredevices"
            }
          ]
        }
      ],
      "description" : "Measurement status definitions from the ISO/IEEE 11073-10201 DIM. This CodeSystem is intended to be part of THO (terminology.hl7.org) and the URL already assumes that.",
      "jurisdiction" : [
        {
          "coding" : [
            {
              "system" : "http://unstats.un.org/unsd/methods/m49/m49.htm",
              "code" : "001"
            }
          ]
        }
      ],
      "caseSensitive" : false,
      "content" : "complete",
      "concept" : [
        {
          "code" : "questionable",
          "display" : "Questionable",
          "definition" : "Data may not be reliable"
        },
        {
          "code" : "calibration-ongoing",
          "display" : "Calibration ongoing",
          "definition" : "Calibration is ongoing"
        },
        {
          "code" : "validated-data",
          "display" : "Validated data",
          "definition" : "Relevant, e.g., in an archive"
        },
        {
          "code" : "early-indication",
          "display" : "Early indication",
          "definition" : "Early estimate of value"
        },
        {
          "code" : "msmt-ongoing",
          "display" : "Measurement ongoing",
          "definition" : "Indicates that a new measurement is just being taken"
        },
        {
          "code" : "in-alarm",
          "display" : "Measurement in alarm",
          "definition" : "Measurement has an active alarm condition"
        },
        {
          "code" : "alarm-inhibited",
          "display" : "Measurement alarms inhibited",
          "definition" : "Measurement supports alarming and alarms are turned off"
        }
      ]
    }