Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## ValueSet: Safety classification value set

Official URL: http://terminology.hl7.org/ValueSet/safety-classification | Version: 1.0.0
Standards status: Trial-use | Maturity Level: 2 | Computable Name: SafetyClassification

CodeSystem for IEEE 11073-10207 SafetyClassification. This ValueSet is intended to be part of THO (terminology.hl7.org) and the URL already assumes that.

References

- Channel Device profile
- MDS Device profile
- VMD Device profile

### Logical Definition (CLD)

Profile: Shareable ValueSet

- Include all codes defined in `http://terminology.hl7.org/CodeSystem/safety-classification` version 📦1.0.0

### Expansion

Expansion performed internally based on codesystem Safety v1.0.0 (CodeSystem)

This value set contains 4 concepts

System | Code | Display (en) | Definition | JSON | XML
`http://terminology.hl7.org/CodeSystem/safety-classification` | Inf | Informational | The descriptor and the related state information are intended to be used for information purposes only. They are not intended to be used in clinical functions. |  |
`http://terminology.hl7.org/CodeSystem/safety-classification` | MedA | Medical Class A | Medical Class A. The descriptor and related state information are intended to be used in clinical functions, specifically for general display in order to support patient and device monitoring. The displayed data is not intended to be used as sole source for diagnostic or therapeutic decisions. Deviations from this intended use are in the sole responsibility of the SERVICE CONSUMER. |  |
`http://terminology.hl7.org/CodeSystem/safety-classification` | MedB | Medical Class B | The descriptor and related state information are intended to be used in clinical functions. The manufacturer has specified and considered a specific intended use for the data, which could result in nonserious injury. Deviations from this intended use are in the sole responsibility of the SERVICE CONSUMER. |  |
`http://terminology.hl7.org/CodeSystem/safety-classification` | MedC | Medical Class C | The descriptor and related state information are intended to be used in clinical functions. The manufacturer has specified and considered a specific intended use for the data, which could result in serious injury. Deviations from this intended use are in the sole responsibility of the SERVICE CONSUMER. |  |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code