Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example Observation: NBP Numeric observation example

Page standards status: Informative

Profile: Compound Numeric Observation profile

status: Final

category: Vital Signs

code: Blood pressure panel with all children optional

subject: John Doe Male, DoB: 1967-05-04 ( Medical record number)

effective: 2021-07-09 11:30:12+0200

device: DeviceMetric: extension = intr; type = MDC_PRESS_BLD_NONINV; unit = MDC_DIM_MMHG; operationalStatus = on; color = red; category = measurement; measurementPeriod = Once per 15 minutes

> component

> code: Systolic blood pressure

> value: 120 mmHg (Details: UCUM codemm[Hg] = 'mm[Hg]')

> component

> code: Diastolic blood pressure

> value: 80 mmHg (Details: UCUM codemm[Hg] = 'mm[Hg]')

> component

> code: Mean blood pressure

> value: 90 mmHg (Details: UCUM codemm[Hg] = 'mm[Hg]')