Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Resource Profile: SampleArrayDeviceMetric - Mappings

Page standards status: Trial-use | Maturity Level: 2

Mappings for the SampleArrayDeviceMetric resource profile.

#### Mappings to Structures in this Implementation Guide

No Mappings Found

#### Mappings to other Structures

No Mappings Found

#### Other Mappings

Name | IEEE 11073-10201 DIM | IEEE 11073-10207 SDC | FiveWs Pattern Mapping | RIM Mapping
--- | --- | --- | --- | ---
DeviceMetric |  |  |  | Entity. Role or Act
id |  |  |  |
meta |  |  |  |
implicitRules |  |  |  |
language |  |  |  |
text |  |  |  | Act.text?
contained |  |  |  | N/A
Slices for extension |  |  |  |
extension:instance |  |  |  |
id |  |  |  | n/a
Slices for extension |  |  |  |
extension:number |  |  |  |
id |  |  |  | n/a
extension |  |  |  | n/a
url |  |  |  | N/A
Slices for value[x] |  |  |  | N/A
value[x]:valueUnsignedInt |  | AbstractMetricState/PhysicalConnector/Number |  | N/A
extension:label |  |  |  |
id |  |  |  | n/a
extension |  |  |  | n/a
url |  |  |  | N/A
Slices for value[x] |  |  |  | N/A
value[x]:valueString |  | AbstractMetricState/PhysicalConnector/Label |  | N/A
url |  |  |  | N/A
value[x] |  |  |  | N/A
extension:relation |  |  |  |
extension:metricAvailability |  | DistributionSampleArrayMetricDescriptor/MetricAvailability RealTimeSampleArrayMetricDescriptor/MetricAvailability |  |
extension:technicalRange |  |  |  |
extension:resolution | :Sa-Measure-Resolution | DistributionSampleArrayMetricDescriptor/Resolution RealTimeSampleArrayMetricDescriptor/Resolution |  |
extension:sweep-speed | :Sweep-Speed |  |  |
extension:visual-grid | :Visual-Grid |  |  |
modifierExtension |  |  |  | N/A
identifier |  |  | FiveWs.identifier |
type |  | According to ISO/IEEE 11073-20701 this element can't be empty | FiveWs.class |
id |  |  |  | n/a
extension |  |  |  | n/a
coding |  |  |  | union(. ./translation)
id |  |  |  | n/a
extension |  |  |  | n/a
system |  | DistributionSampleArrayMetricDescriptor/Type/CodingSystem RealTimeSampleArrayMetricDescriptor/Type/CodingSystem |  | ./codeSystem
version |  | DistributionSampleArrayMetricDescriptor/Type/CodingSystemVersion RealTimeSampleArrayMetricDescriptor/Type/CodingSystemVersion |  | ./codeSystemVersion
code | :Type | DistributionSampleArrayMetricDescriptor/Type/Code RealTimeSampleArrayMetricDescriptor/Type/Code |  | ./code
display |  |  |  | CV.displayName
userSelected |  |  |  | CD.codingRationale
text | :Label-String |  |  | ./originalText[mediaType/code="text/plain"]/data
unit |  |  |  |
id |  |  |  | n/a
extension |  |  |  | n/a
coding |  |  |  | union(. ./translation)
id |  |  |  | n/a
extension |  |  |  | n/a
system |  | DistributionSampleArrayMetricDescriptor/Unit/CodingSystem RealTimeSampleArrayMetricDescriptor/Unit/CodingSystem |  | ./codeSystem
version |  | DistributionSampleArrayMetricDescriptor/Type/CodingSystemVersion RealTimeSampleArrayMetricDescriptor/Type/CodingSystemVersion |  | ./codeSystemVersion
code | :Unit-Code | DistributionSampleArrayMetricDescriptor/Unit/Code RealTimeSampleArrayMetricDescriptor/Unit/Code |  | ./code
display |  |  |  | CV.displayName
userSelected |  |  |  | CD.codingRationale
text | :Unit-LabelString |  |  | ./originalText[mediaType/code="text/plain"]/data
source |  |  |  |
parent |  |  |  |
operationalStatus | :Metric-Status | DistributionSampleArrayMetricState/ActivationState RealTimeSampleArrayMetricState/ActivationState note the mapping of the value set |  |
color | :Color |  |  |
category | :Metric-Specification::category | DistributionSampleArrayMetricDescriptor/MetricCategory RealTimeSampleArrayMetricDescriptor/MetricCategory note the mapping of the value set | FiveWs.class |
measurementPeriod |  |  |  |
id |  |  |  | n/a
extension |  |  |  | n/a
modifierExtension |  |  |  | N/A
event |  |  |  | QLIST<TS>
repeat |  |  |  | Implies PIVL or EIVL
id |  |  |  | n/a
extension |  |  |  | n/a
bounds[x] |  |  |  | IVL(TS) used in a QSI
count |  |  |  | PIVL.count
countMax |  |  |  | PIVL.count
duration |  | DistributionSampleArrayMetricDescriptor/DeterminationPeriod RealTimeSampleArrayMetricDescriptor/DeterminationPeriod Unit can be specified by durationUnit |  | PIVL.phase
durationMax |  |  |  | PIVL.phase
durationUnit |  |  |  | PIVL.phase.unit
frequency |  |  |  | PIVL.phase
frequencyMax |  |  |  | PIVL.phase
period | :Sample-Period |  |  | PIVL.phase
periodMax |  |  |  | PIVL.phase
periodUnit |  |  |  | PIVL.phase.unit
dayOfWeek |  |  |  | n/a
timeOfDay |  |  |  | n/a
when |  |  |  | EIVL.event
offset |  |  |  | EIVL.offset
code |  |  |  | QSC.code
calibration |  |  |  |
id |  |  |  | n/a
extension |  |  |  | n/a
modifierExtension |  |  |  | N/A
type | :Metric-Calibration::cal-type |  |  |
state | :Metric-Calibration::cal-state |  |  |
time | :Metric-Calibration::cal-time |  |  |
Documentation for this format