Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example DeviceMetric: ECG Sample Array metric example

Page standards status: Informative

Profile: Sample Array DeviceMetric profile

Resolution extension: 0.001

Sweep Speed extension: 25 mm/s (Details: UCUM codemm/s = 'mm/s')

type: ECG

unit: mV

source: Device: extension = ,->Practitioner Alice B. Careful ,8760,156,Dmo; identifier = urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680#01-23-45-67-89-AB-CD-EF; status = active; manufacturer = MyCompany; serialNumber = 123456; modelNumber = PM1; type = MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS

parent: Device: status = active; type = MDC_DEV_ECG_CHAN

operationalStatus: On

color: Color Green

category: Measurement