Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Rhythm Status Enumeration metric example - TTL Representation

Page standards status: Informative

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdf: <http://www.w3.org/1999/02/22-rdf-syntax-ns#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:DeviceMetric ;
      fhir:nodeRole fhir:treeRoot ;
      fhir:id [ fhir:v "RhythmStatusEnumerationDeviceMetric"] ; #
      fhir:meta [
        ( fhir:profile [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/EnumerationDeviceMetric"^^xsd:anyURI ;
    fhir:l <http://hl7.org/fhir/uv/pocd/StructureDefinition/EnumerationDeviceMetric>     ] )
      ] ; #
      fhir:text [
    fhir:status [ fhir:v "generated" ] ;
    fhir:div [ fhir:v "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p class=\"res-header-id\"><b>Generated Narrative: DeviceMetric RhythmStatusEnumerationDeviceMetric</b></p><a name=\"RhythmStatusEnumerationDeviceMetric\"> </a><a name=\"hcRhythmStatusEnumerationDeviceMetric\"> </a><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\"/><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-EnumerationDeviceMetric.html\">Enumeration DeviceMetric profile</a></p></div><p><b>type</b>: <span title=\"Codes:{urn:iso:std:iso:11073:10101 184327}\">Rhythm</span></p><p><b>source</b>: <a href=\"Device-PhysioMonitorMdsDevice.html\">Device: extension = ,-&gt;Practitioner Alice B. Careful ,8760,156,Dmo; identifier = urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680#01-23-45-67-89-AB-CD-EF; status = active; manufacturer = MyCompany; serialNumber = 123456; modelNumber = PM1; type = MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS</a></p><p><b>parent</b>: <a href=\"Device-ECGChannelDevice.html\">Device: status = active; type = MDC_DEV_ECG_CHAN</a></p><p><b>operationalStatus</b>: On</p><p><b>category</b>: Measurement</p></div>"^^rdf:XMLLiteral ]
      ] ; #
      fhir:type [
        ( fhir:coding [
    fhir:system [
    fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ;
    fhir:l <urn:iso:std:iso:11073:10101>       ] ;
    fhir:code [ fhir:v "184327" ] ;
    fhir:display [ fhir:v "MDC_ECG_STAT_RHY" ]     ] ) ;
    fhir:text [ fhir:v "Rhythm" ]
      ] ; #
      fhir:source [
    fhir:l fhir:Device/PhysioMonitorMdsDevice ;
    fhir:reference [ fhir:v "Device/PhysioMonitorMdsDevice" ]
      ] ; #
      fhir:parent [
    fhir:l fhir:Device/ECGChannelDevice ;
    fhir:reference [ fhir:v "Device/ECGChannelDevice" ]
      ] ; #
      fhir:operationalStatus [ fhir:v "on"] ; #
      fhir:category [ fhir:v "measurement"] . #