## Profile Comparison between http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayDeviceMetric vs http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayDeviceMetric

Left: | Sample Array DeviceMetric profile (http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayDeviceMetric)
Right: | Sample Array DeviceMetric profile (http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayDeviceMetric)

### Messages

Error | StructureDefinition.version | Values for version differ: '0.3.0' vs '1.0.0'
Information | StructureDefinition.status | Values for status differ: 'draft' vs 'active'
Information | StructureDefinition.date | Values for date differ: '2021-08-04' vs '2022-01-16'
Information | StructureDefinition.publisher | Values for publisher differ: 'HL7 International - Devices Work Group' vs 'HL7 International / Devices'
Information | DeviceMetric.language | Example/preferred bindings differ at DeviceMetric.language using binding from SampleArrayDeviceMetric
Information | DeviceMetric.measurementPeriod.code | Example/preferred bindings differ at DeviceMetric.measurementPeriod.code using binding from SampleArrayDeviceMetric

### Metadata

Name | Value | Comments
--- | --- | ---
abstract | false |
baseDefinition | http://hl7.org/fhir/StructureDefinition/DeviceMetric |
copyright |  |
date | 2021-08-04 | 2022-01-16 | Values Differ
description | StructureDefinition for DeviceMetric resources that represent real-time waveforms or wave snippets characteristics and capabilities. |
experimental |  |
fhirVersion | 4.0.1 |
jurisdiction |  |
jurisdiction[0] | http://unstats.un.org/unsd/methods/m49/m49.htm#001 |
kind | resource |
name | SampleArrayDeviceMetric |
publisher | HL7 International - Devices Work Group | HL7 International / Devices | Values Differ
purpose |  |
status | draft | active | Values Differ
title | Sample Array DeviceMetric profile |
type | DeviceMetric |
url | http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayDeviceMetric |
version | 0.3.0 | 1.0.0 | Values Differ

### Structure

Name | L Flags | L Card. | L Type | L Description & Constraints | R Flags | R Card. | R Type | R Description & Constraints | Comments
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
DeviceMetric |  | 0..* | DeviceMetric | Measurement, calculation or setting capability of a medical device |  | 0..* | DeviceMetric | Measurement, calculation or setting capability of a medical device |
id | Σ | 0..1 | string | Logical id of this artifact | Σ | 0..1 | id | Logical id of this artifact |
meta | Σ | 0..1 | Meta | Metadata about the resource | Σ | 0..1 | Meta | Metadata about the resource |
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created | ?!Σ | 0..1 | uri | A set of rules under which this content was created |
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
|  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
| Example/preferred bindings differ at DeviceMetric.language using binding from SampleArrayDeviceMetric
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements |
contained |  | 0..* | Resource | Contained, inline Resources |  | 0..* | Resource | Contained, inline Resources |
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url |
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored | ?! | 0..* | Extension | Extensions that cannot be ignored |
identifier | Σ | 0..* | Identifier | Instance identifier | Σ | 0..* | Identifier | Instance identifier |
type | S Σ | 1..1 | CodeableConcept | Identity of metric, for example Heart Rate or PEEP Setting Binding: ?? (extensible) | S Σ | 1..1 | CodeableConcept | Identity of metric, for example Heart Rate or PEEP Setting Binding: ?? (extensible) |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
Slices for extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |
coding | Σ | 0..* | Coding | Code defined by a terminology system | Σ | 0..* | Coding | Code defined by a terminology system |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
Slices for extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |
system | Σ | 0..1 | uri | Identity of the terminology system | Σ | 0..1 | uri | Identity of the terminology system |
version | Σ | 0..1 | string | Version of the system - if relevant | Σ | 0..1 | string | Version of the system - if relevant |
code | Σ | 0..1 | code | Symbol in syntax defined by the system | Σ | 0..1 | code | Symbol in syntax defined by the system |
display | Σ | 0..1 | string | Representation defined by the system | Σ | 0..1 | string | Representation defined by the system |
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user | Σ | 0..1 | boolean | If this coding was chosen directly by the user |
text | Σ | 0..1 | string | Plain text representation of the concept | Σ | 0..1 | string | Plain text representation of the concept |
unit | S Σ | 0..1 | CodeableConcept | Unit of Measure for the Metric Binding: ?? (extensible) | S Σ | 0..1 | CodeableConcept | Unit of Measure for the Metric Binding: ?? (extensible) |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
Slices for extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |
coding | Σ | 0..* | Coding | Code defined by a terminology system | Σ | 0..* | Coding | Code defined by a terminology system |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
Slices for extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |
system | Σ | 0..1 | uri | Identity of the terminology system | Σ | 0..1 | uri | Identity of the terminology system |
version | Σ | 0..1 | string | Version of the system - if relevant | Σ | 0..1 | string | Version of the system - if relevant |
code | Σ | 0..1 | code | Symbol in syntax defined by the system | Σ | 0..1 | code | Symbol in syntax defined by the system |
display | Σ | 0..1 | string | Representation defined by the system | Σ | 0..1 | string | Representation defined by the system |
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user | Σ | 0..1 | boolean | If this coding was chosen directly by the user |
text | Σ | 0..1 | string | Plain text representation of the concept | Σ | 0..1 | string | Plain text representation of the concept |
source | S Σ | 1..1 | Reference(MDS Device profile) | Describes the link to the source Device | S Σ | 1..1 | Reference(MDS Device profile) | Describes the link to the source Device |
parent | S Σ | 1..1 | Reference(Channel Device profile) | Describes the link to the parent Device | S Σ | 1..1 | Reference(Channel Device profile) | Describes the link to the parent Device |
operationalStatus | S Σ | 0..1 | code | on | off | standby | entered-in-error Binding: ?? (required): Describes the operational status of the DeviceMetric. | S Σ | 0..1 | code | on | off | standby | entered-in-error Binding: ?? (required): Describes the operational status of the DeviceMetric. |
color | Σ | 0..1 | code | black | red | green | yellow | blue | magenta | cyan | white Binding: ?? (required): Describes the typical color of representation. | Σ | 0..1 | code | black | red | green | yellow | blue | magenta | cyan | white Binding: ?? (required): Describes the typical color of representation. |
category | S Σ | 1..1 | code | measurement | setting | calculation | unspecified Binding: ?? (required): Describes the category of the metric. | S Σ | 1..1 | code | measurement | setting | calculation | unspecified Binding: ?? (required): Describes the category of the metric. |
measurementPeriod | S Σ | 0..1 | Timing | Describes the measurement repetition time | S Σ | 0..1 | Timing | Describes the measurement repetition time |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
Slices for extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
event | Σ | 0..* | dateTime | When the event occurs | Σ | 0..* | dateTime | When the event occurs |
repeat | Σ C | 0..1 | Element | When the event is to occur | Σ C | 0..1 | Element | When the event is to occur |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
Slices for extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url |
bounds[x] | Σ | 0..1 | Duration, Range, Period | Length/Range of lengths, or (Start and/or end) limits | Σ | 0..1 | Duration, Range, Period | Length/Range of lengths, or (Start and/or end) limits |
count | Σ | 0..1 | positiveInt | Number of times to repeat | Σ | 0..1 | positiveInt | Number of times to repeat |
countMax | Σ | 0..1 | positiveInt | Maximum number of times to repeat | Σ | 0..1 | positiveInt | Maximum number of times to repeat |
duration | Σ | 0..1 | decimal | How long when it happens | Σ | 0..1 | decimal | How long when it happens |
durationMax | Σ | 0..1 | decimal | How long when it happens (Max) | Σ | 0..1 | decimal | How long when it happens (Max) |
durationUnit | Σ | 0..1 | code | s | min | h | d | wk | mo | a - unit of time (UCUM) Binding: ?? (required): A unit of time (units from UCUM). | Σ | 0..1 | code | s | min | h | d | wk | mo | a - unit of time (UCUM) Binding: ?? (required): A unit of time (units from UCUM). |
frequency | Σ | 0..1 | positiveInt | Event occurs frequency times per period | Σ | 0..1 | positiveInt | Event occurs frequency times per period |
frequencyMax | Σ | 0..1 | positiveInt | Event occurs up to frequencyMax times per period | Σ | 0..1 | positiveInt | Event occurs up to frequencyMax times per period |
period | Σ | 0..1 | decimal | Event occurs frequency times per period | Σ | 0..1 | decimal | Event occurs frequency times per period |
periodMax | Σ | 0..1 | decimal | Upper limit of period (3-4 hours) | Σ | 0..1 | decimal | Upper limit of period (3-4 hours) |
periodUnit | Σ | 0..1 | code | s | min | h | d | wk | mo | a - unit of time (UCUM) Binding: ?? (required): A unit of time (units from UCUM). | Σ | 0..1 | code | s | min | h | d | wk | mo | a - unit of time (UCUM) Binding: ?? (required): A unit of time (units from UCUM). |
dayOfWeek | Σ | 0..* | code | mon | tue | wed | thu | fri | sat | sun Binding: ?? (required) | Σ | 0..* | code | mon | tue | wed | thu | fri | sat | sun Binding: ?? (required) |
timeOfDay | Σ | 0..* | time | Time of day for action | Σ | 0..* | time | Time of day for action |
when | Σ | 0..* | code | Code for time period of occurrence Binding: ?? (required): Real world event relating to the schedule. | Σ | 0..* | code | Code for time period of occurrence Binding: ?? (required): Real world event relating to the schedule. |
offset | Σ | 0..1 | unsignedInt | Minutes from event (before or after) | Σ | 0..1 | unsignedInt | Minutes from event (before or after) |
code | Σ | 0..1 | CodeableConcept | BID | TID | QID | AM | PM | QD | QOD | + Binding: ?? (preferred): Code for a known / defined timing pattern. | Σ | 0..1 | CodeableConcept | BID | TID | QID | AM | PM | QD | QOD | + Binding: ?? (preferred): Code for a known / defined timing pattern. | Example/preferred bindings differ at DeviceMetric.measurementPeriod.code using binding from SampleArrayDeviceMetric
calibration | S Σ | 0..* | BackboneElement | Describes the calibrations that have been performed or that are required to be performed | S Σ | 0..* | BackboneElement | Describes the calibrations that have been performed or that are required to be performed |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
type | Σ | 0..1 | code | unspecified | offset | gain | two-point Binding: ?? (required): Describes the type of a metric calibration. | Σ | 0..1 | code | unspecified | offset | gain | two-point Binding: ?? (required): Describes the type of a metric calibration. |
state | Σ | 0..1 | code | not-calibrated | calibration-required | calibrated | unspecified Binding: ?? (required): Describes the state of a metric calibration. | Σ | 0..1 | code | not-calibrated | calibration-required | calibrated | unspecified Binding: ?? (required): Describes the state of a metric calibration. |
time | Σ | 0..1 | instant | Describes the time last calibration has been performed | Σ | 0..1 | instant | Describes the time last calibration has been performed |
Documentation for this format