Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## ValueSet: Reference range type value set

Official URL: http://hl7.org/fhir/uv/pocd/ValueSet/reference-range-type | Version: 1.0.0
Standards status: Trial-use | Maturity Level: 2 | Computable Name: ReferenceRangeType

ValueSet for classifying the type of reference range applied to a DeviceMetric.

References

- Reference range extension

### Logical Definition (CLD)

Profile: Shareable ValueSet

This value set includes codes based on the following rules:

- Include all codes defined in `http://hl7.org/fhir/uv/pocd/CodeSystem/reference-range-type` version 📦1.0.0
- Include all codes defined in `http://terminology.hl7.org/CodeSystem/referencerange-meaning` version 📦1.0.1

### Expansion

Expansion performed internally based on:

- codesystem Reference Range Type v1.0.0 (CodeSystem)
- codesystem Observation Reference Range Meaning Codes v1.0.1 (CodeSystem)

This value set contains 16 concepts

System | Code | Display (en) | Definition | JSON | XML
`http://hl7.org/fhir/uv/pocd/CodeSystem/reference-range-type` | alarm-limits | Alarm limits | The range defines the alarm limits configured on the device. Values outside this range trigger an alert. |  |
`http://hl7.org/fhir/uv/pocd/CodeSystem/reference-range-type` | physiological-range | Physiological range | The range defines the physiologically normal or expected values for the measured parameter. |  |
`http://hl7.org/fhir/uv/pocd/CodeSystem/reference-range-type` | technical-range | Technical range | The range defines the technical measurement capability of the device — the minimum and maximum values the device can report. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | type | Type | General types of reference range. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | normal | Normal Range | Values expected for a normal member of the relevant control population being measured. Typically each results producer such as a laboratory has specific normal ranges and they are usually defined as within two standard deviations from the mean and account for 95.45% of this population. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | recommended | Recommended Range | The range that is recommended by a relevant professional body. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | treatment | Treatment Range | The range at which treatment would/should be considered. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | therapeutic | Therapeutic Desired Level | The optimal range for best therapeutic outcomes. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | pre | Pre Therapeutic Desired Level | The optimal range for best therapeutic outcomes for a specimen taken immediately before administration. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | post | Post Therapeutic Desired Level | The optimal range for best therapeutic outcomes for a specimen taken immediately after administration. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | endocrine | Endocrine | Endocrine related states that change the expected value. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | pre-puberty | Pre-Puberty | An expected range in an individual prior to puberty. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | follicular | Follicular Stage | An expected range in an individual during the follicular stage of the cycle. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | midcycle | MidCycle | An expected range in an individual during the midcycle stage of the cycle. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | luteal | Luteal | An expected range in an individual during the luteal stage of the cycle. |  |
`http://terminology.hl7.org/CodeSystem/referencerange-meaning` | postmenopausal | Post-Menopause | An expected range in an individual post-menopause. |  |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code