# ECG VMD example - Point-of-Care Device Implementation Guide v1.0.0

* [**Table of Contents**](toc.md)
* [**Artifact List**](artifacts.md)
* **ECG VMD example**

## Example Device: ECG VMD example

| |
| :--- |
| *Page standards status:*[Informative](http://hl7.org/fhir/R4/versions.html#std-process) |

Profile: [VMD Device profile](StructureDefinition-VmdDevice.md)

**status**: Active

**type**: MDC_DEV_ECG_VMD

**parent**: [Device: extension = ,->Practitioner Alice B. Careful ,8760,156,Dmo; identifier = urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680#01-23-45-67-89-AB-CD-EF; status = active; manufacturer = MyCompany; serialNumber = 123456; modelNumber = PM1; type = MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS](Device-PhysioMonitorMdsDevice.md)



## Resource Content

```json
{
  "resourceType" : "Device",
  "id" : "ECGVmdDevice",
  "meta" : {
    "profile" : ["http://hl7.org/fhir/uv/pocd/StructureDefinition/VmdDevice"]
  },
  "status" : "active",
  "type" : {
    "coding" : [{
      "system" : "urn:iso:std:iso:11073:10101",
      "code" : "69798",
      "display" : "MDC_DEV_ECG_VMD"
    }]
  },
  "parent" : {
    "reference" : "Device/PhysioMonitorMdsDevice"
  }
}

```
