Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Artifact List

Page standards status: Informative

This page provides a list of the FHIR artifacts defined as part of this implementation guide.

### Behavior: Capability Statements

The following artifacts define the specific capabilities that different types of systems are expected to have in order to comply with this implementation guide. Systems conforming to this implementation guide are expected to declare conformance to one or more of the following capability statements.

Server CapabilityStatement | CapabilityStatement that describes the expected capabilities of a server processing data from Point-of-Care devices.

### Structures: Abstract Profiles

These are profiles on resources or data types that describe patterns used by other profiles, but cannot be instantiated directly. I.e. instances can conform to profiles based on these abstract profiles but do not declare conformance to the abstract profiles themselves.

Observation profile | StructureDefinition for measurements and simple assertions made about a patient, device or other subject.
Patient profile | StructureDefinition for Patient resources that represent demographics and other administrative information.
Practitioner profile | StructureDefinition for Practitioner resources that represent demographics and other administrative information.

### Structures: Resource Profiles

These define constraints on FHIR resources for systems conforming to this implementation guide.

Channel Device profile | StructureDefinition for Device resources that represent Channels, which are used for grouping metrics together.
Compound Numeric Observation profile | StructureDefinition for Observation resources that represent numerical measurements, calculations, or settings with multiple components.
Enumeration DeviceMetric profile | StructureDefinition for DeviceMetric resources that represent coded or text status, annotations, or settings characteristics and capabilities.
Enumeration Observation profile | StructureDefinition for Observation resources that represent coded or text status, annotations, or settings.
MDS Device profile | StructureDefinition for Device resources that represent a Medical Device System (MDS). This is the top-level resource in the hierarchical model of a Point-of-Care device.
Numeric DeviceMetric profile | StructureDefinition for DeviceMetric resources that represent numerical measurements, calculations, or settings characteristics and capabilities.
Numeric Observation profile | StructureDefinition for Observation resources that represent numerical measurements, calculations, or settings.
Sample Array DeviceMetric profile | StructureDefinition for DeviceMetric resources that represent real-time waveforms or wave snippets characteristics and capabilities.
Sample Array Observation profile | StructureDefinition for Observation resources that represent real-time waveforms or wave snippets.
VMD Device profile | StructureDefinition for Device resources that represent Virtual Medical Devices (VMD). These are medical-related subsystems in the hierarchical model of a Point-of-Care device.

### Structures: Extension Definitions

These define constraints on FHIR data types for systems conforming to this implementation guide.

Approved Jurisdictions extension | StructureDefinition that adds approved jurisdictions to a Device.
Device Instance extension | StructureDefinition that adds an instance number or label to Device or DeviceMetric.
Metric availability extension | StructureDefinition that adds metric availability to a DeviceMetric.
Operating cycles extension | StructureDefinition that adds operating cycles to a Device.
Operating hours extension | StructureDefinition that adds operating hours to a Device.
Operating mode extension | StructureDefinition that adds an operating mode to a Device.
Operator extension | StructureDefinition that adds an operator to a Device.
Reference range extension | StructureDefinition that adds a typed reference range (low, high, and range type) to a DeviceMetric.
Relation extension | StructureDefinition that adds relations to a DeviceMetric.
Resolution extension | StructureDefinition that adds resolution to a DeviceMetric.
Sweep Speed extension | StructureDefinition that adds default sweep speed to a DeviceMetric.
Technical range extension | StructureDefinition that adds technical range and accuracy to a DeviceMetric.
Visual Grid extension | StructureDefinition that adds grid line definitions to a DeviceMetric.

### Terminology: Value Sets

These define sets of codes used by systems conforming to this implementation guide.

Kind of relation value set | ValueSet for IEEE 11073-10207 Relation/Kind.
MDC Metric nomenclature | ValueSet for the ISO/IEEE 11073-10101 Nomenclature filtered by Metric (SCADA or Settings) partition.
MDC Object infrastructure and Device nomenclature | ValueSet for the ISO/IEEE 11073-10101 Nomenclature filtered by Object partition.
MDC Unit of Measurement | ValueSet for the ISO/IEEE 11073-10101 Nomenclature filtered by Dimension partition.
Metric availability value set | ValueSet for IEEE 11073-10207 MetricAvailability.
Observation interpretation codes | Observation interpretation codes including measurement status.
Operating mode value set | ValueSet for IEEE 11073-10207 MdsState/OperatingMode.
Reference range type value set | ValueSet for classifying the type of reference range applied to a DeviceMetric.
Safety | CodeSystem for IEEE 11073-10207 SafetyClassification
Safety classification value set | ValueSet for IEEE 11073-10207 SafetyClassification.

### Terminology: Code Systems

These define new code systems used by systems conforming to this implementation guide.

Kind of relation code system | Relation definitions from the ISO/IEEE 11073-10207.
Measurement status codes | Measurement status definitions from the ISO/IEEE 11073-10201 DIM.
Metric availability code system | Metric availability definitions from the ISO/IEEE 11073-10207.
Operating mode code system | Operating mode definitions from the ISO/IEEE 11073-10207.
Reference range type code system | CodeSystem for classifying the type of reference range applied to a DeviceMetric.
Safety classification code system | Safety classification definitions from the ISO/IEEE 11073-10207.

### Example: Example Instances

These are example instances that show what data produced and consumed by systems conforming with this implementation guide might look like.

Blood Pressure Channel example | Example of a Device resource that represents an invasive blood pressure channel.
Blood Pressure VMD example | Example of a Device resource that represents an invasive blood pressure subsystem.
CVP Sample Array metric example | Example of a DeviceMetric resource that represents a central venous pressure metric.
CVP Sample Array observation example | Example of an Observation resource that represents central venous pressure waveform.
ECG Channel example | Example of a Device resource that represents an ECG channel.
ECG Sample Array metric example | Example of a DeviceMetric resource that represents an ECG metric.
ECG Sample Array observation example | Example of an Observation resource that represents ECG waveforms.
ECG VMD example | Example of a Device resource that represents an ECG subsystem.
Heart Rate Channel example | Example of a Device resource that represents a heart rate channel.
Heart Rate Numeric metric example | Example of a DeviceMetric resource that represents a heart rate metric.
Heart Rate Numeric observation example | Example of an Observation resource that represents heart rate measurement.
NBP Channel example | Example of a Device resource that represents a non-invasive blood pressure channel.
NBP Numeric metric example | Example of a DeviceMetric resource that represents a non-invasive blood pressure metric.
NBP Numeric observation example | Example of an Observation resource that represents non-invasive blood pressure measurement.
NBP VMD example | Example of a Device resource that represents a non-invasive blood pressure subsystem.
Patient Monitor MDS example | Example of a Device resource that represents a patient monitor.
Rhythm Status Enumeration metric example | Example of a DeviceMetric resource that represents a rhythm status metric.
Rhythm Status Enumeration observation example | Example of an Observation resource that represents coded rhythm status.
Some Location example | Example of a Location resource.
Some Patient example | Example of a Patient resource.
Some Practitioner example | Example of a Practitioner resource.