# Measurement status codes - Point-of-Care Device Implementation Guide v1.0.0

* [**Table of Contents**](toc.md)
* [**Artifact List**](artifacts.md)
* **Measurement status codes**

## CodeSystem: Measurement status codes 

| | | |
| :--- | :--- | :--- |
| *Official URL*:http://terminology.hl7.org/CodeSystem/measurement-status | *Version*:1.0.0 | |
| * Standards status: *[Trial-use](http://hl7.org/fhir/R4/versions.html#std-process) | [Maturity Level](http://hl7.org/fhir/versions.html#maturity): 2 | *Computable Name*:MeasurementStatus |

 
Measurement status definitions from the ISO/IEEE 11073-10201 DIM. This CodeSystem is intended to be part of THO (terminology.hl7.org) and the URL already assumes that. 

 This Code system is referenced in the content logical definition of the following value sets: 

* [ObservationInterpretation](ValueSet-observation-interpretation.md)



## Resource Content

```json
{
  "resourceType" : "CodeSystem",
  "id" : "measurement-status",
  "meta" : {
    "profile" : ["http://hl7.org/fhir/StructureDefinition/shareablecodesystem"]
  },
  "extension" : [{
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-wg",
    "valueCode" : "dev"
  },
  {
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-fmm",
    "valueInteger" : 2,
    "_valueInteger" : {
      "extension" : [{
        "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
        "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
      }]
    }
  },
  {
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-standards-status",
    "valueCode" : "trial-use",
    "_valueCode" : {
      "extension" : [{
        "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
        "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
      }]
    }
  }],
  "url" : "http://terminology.hl7.org/CodeSystem/measurement-status",
  "version" : "1.0.0",
  "name" : "MeasurementStatus",
  "title" : "Measurement status codes",
  "status" : "active",
  "experimental" : false,
  "date" : "2019-09-28",
  "publisher" : "HL7 International / Devices",
  "contact" : [{
    "telecom" : [{
      "system" : "url",
      "value" : "http://www.hl7.org/Special/committees/healthcaredevices"
    }]
  }],
  "description" : "Measurement status definitions from the ISO/IEEE 11073-10201 DIM. This CodeSystem is intended to be part of THO (terminology.hl7.org) and the URL already assumes that.",
  "jurisdiction" : [{
    "coding" : [{
      "system" : "http://unstats.un.org/unsd/methods/m49/m49.htm",
      "code" : "001"
    }]
  }],
  "caseSensitive" : false,
  "content" : "complete",
  "concept" : [{
    "code" : "questionable",
    "display" : "Questionable",
    "definition" : "Data may not be reliable"
  },
  {
    "code" : "calibration-ongoing",
    "display" : "Calibration ongoing",
    "definition" : "Calibration is ongoing"
  },
  {
    "code" : "validated-data",
    "display" : "Validated data",
    "definition" : "Relevant, e.g., in an archive"
  },
  {
    "code" : "early-indication",
    "display" : "Early indication",
    "definition" : "Early estimate of value"
  },
  {
    "code" : "msmt-ongoing",
    "display" : "Measurement ongoing",
    "definition" : "Indicates that a new measurement is just being taken"
  },
  {
    "code" : "in-alarm",
    "display" : "Measurement in alarm",
    "definition" : "Measurement has an active alarm condition"
  },
  {
    "code" : "alarm-inhibited",
    "display" : "Measurement alarms inhibited",
    "definition" : "Measurement supports alarming and alarms are turned off"
  }]
}

```
