# Heart Rate Numeric observation example - Point-of-Care Device Implementation Guide v1.0.0

* [**Table of Contents**](toc.md)
* [**Artifact List**](artifacts.md)
* **Heart Rate Numeric observation example**

## Example Observation: Heart Rate Numeric observation example

| |
| :--- |
| *Page standards status:*[Informative](http://hl7.org/fhir/R4/versions.html#std-process) |

Profile: [Numeric Observation profile](StructureDefinition-NumericObservation.md)

**status**: Final

**category**: Vital Signs

**code**: Heart rate

**subject**: [John Doe Male, DoB: 1967-05-04 ( Medical record number)](Patient-SomePatient.md)

**effective**: 2021-07-09 11:33:24+0200

**value**: 60 bpm (Details: UCUM code/min = '/min')

**device**: [DeviceMetric: extension = ,,; type = MDC_ECG_HEART_RATE; unit = MDC_DIM_BEAT_PER_MIN; operationalStatus = on; color = green; category = measurement](DeviceMetric-HeartRateNumericDeviceMetric.md)



## Resource Content

```json
{
  "resourceType" : "Observation",
  "id" : "HeartRateNumericObservation",
  "meta" : {
    "profile" : ["http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericObservation"]
  },
  "status" : "final",
  "category" : [{
    "coding" : [{
      "system" : "http://terminology.hl7.org/CodeSystem/observation-category",
      "code" : "vital-signs",
      "display" : "Vital Signs"
    }]
  }],
  "code" : {
    "coding" : [{
      "system" : "http://loinc.org",
      "code" : "8867-4",
      "display" : "Heart rate"
    },
    {
      "system" : "urn:iso:std:iso:11073:10101",
      "code" : "147842",
      "display" : "MDC_ECG_HEART_RATE"
    }]
  },
  "subject" : {
    "reference" : "Patient/SomePatient"
  },
  "effectiveDateTime" : "2021-07-09T11:33:24+02:00",
  "valueQuantity" : {
    "value" : 60,
    "unit" : "bpm",
    "system" : "http://unitsofmeasure.org",
    "code" : "/min"
  },
  "device" : {
    "reference" : "DeviceMetric/HeartRateNumericDeviceMetric"
  }
}

```
