Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : NBP Numeric metric example - JSON Representation

Page standards status: Informative

Raw json | Download

    {
      "resourceType" : "DeviceMetric",
      "id" : "NBPNumericDeviceMetric",
      "meta" : {
        "profile" : [
          🔗 "http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericDeviceMetric"
        ]
      },
      "text" : {
        "status" : "extensions",
        "div" : "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p class=\"res-header-id\"><b>Generated Narrative: DeviceMetric NBPNumericDeviceMetric</b></p><a name=\"NBPNumericDeviceMetric\"> </a><a name=\"hcNBPNumericDeviceMetric\"> </a><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\"/><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-NumericDeviceMetric.html\">Numeric DeviceMetric profile</a></p></div><p><b>Metric availability extension</b>: intr</p><p><b>type</b>: <span title=\"Codes:{urn:iso:std:iso:11073:10101 150020}\">NBP</span></p><p><b>unit</b>: <span title=\"Codes:{urn:iso:std:iso:11073:10101 266016}\">mmHg</span></p><p><b>source</b>: <a href=\"Device-PhysioMonitorMdsDevice.html\">Device: extension = ,-&gt;Practitioner Alice B. Careful ,8760,156,Dmo; identifier = urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680#01-23-45-67-89-AB-CD-EF; status = active; manufacturer = MyCompany; serialNumber = 123456; modelNumber = PM1; type = MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS</a></p><p><b>parent</b>: <a href=\"Device-NBPChannelDevice.html\">Device: status = active; type = MDC_DEV_PRESS_BLD_NONINV_CHAN</a></p><p><b>operationalStatus</b>: On</p><p><b>color</b>: Color Red</p><p><b>category</b>: Measurement</p><p><b>measurementPeriod</b>: Once per 15 minutes</p></div>"
      },
      "extension" : [
        {
          "url" : "http://hl7.org/fhir/uv/pocd/StructureDefinition/metric-availability",
          "valueCode" : "intr"
        }
      ],
      "type" : {
        "coding" : [
          {
            "system" : "urn:iso:std:iso:11073:10101",
            "code" : "150020",
            "display" : "MDC_PRESS_BLD_NONINV"
          }
        ],
        "text" : "NBP"
      },
      "unit" : {
        "coding" : [
          {
            "system" : "urn:iso:std:iso:11073:10101",
            "code" : "266016",
            "display" : "MDC_DIM_MMHG"
          }
        ],
        "text" : "mmHg"
      },
      "source" : {
        🔗 "reference" : "Device/PhysioMonitorMdsDevice"
      },
      "parent" : {
        🔗 "reference" : "Device/NBPChannelDevice"
      },
      "operationalStatus" : "on",
      "color" : "red",
      "category" : "measurement",
      "measurementPeriod" : {
        "repeat" : {
          "frequency" : 1,
          "period" : 15,
          "periodUnit" : "min"
        }
      }
    }