Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : NBP Channel example - XML Representation

Page standards status: Informative

Raw xml | Download

    <Device xmlns="http://hl7.org/fhir">
      <id value="NBPChannelDevice"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/uv/pocd/StructureDefinition/ChannelDevice"/>
      </meta>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p class="res-header-id"><b>Generated Narrative: Device NBPChannelDevice</b></p><a name="NBPChannelDevice"> </a><a name="hcNBPChannelDevice"> </a><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px"/><p style="margin-bottom: 0px">Profile: <a href="StructureDefinition-ChannelDevice.html">Channel Device profile</a></p></div><p><b>status</b>: Active</p><p><b>type</b>: <span title="Codes:{urn:iso:std:iso:11073:10101 70687}">MDC_DEV_PRESS_BLD_NONINV_CHAN</span></p><p><b>parent</b>: <a href="Device-NBPVmdDevice.html">Device: status = active; manufacturer = MyCompany; serialNumber = 567890; partNumber = 1122-3344; type = MDC_DEV_PRESS_BLD_NONINV_VMD</a></p></div>
      </text>
      <status value="active"/>
      <type>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="70687"/>
          <display value="MDC_DEV_PRESS_BLD_NONINV_CHAN"/>
        </coding>
      </type>
      <parent>🔗
        <reference value="Device/NBPVmdDevice"/>
      </parent>
    </Device>