Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : NBP Numeric metric example - XML Representation

Page standards status: Informative

Raw xml | Download

    <DeviceMetric xmlns="http://hl7.org/fhir">
      <id value="NBPNumericDeviceMetric"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericDeviceMetric"/>
      </meta>
      <text>
        <status value="extensions"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p class="res-header-id"><b>Generated Narrative: DeviceMetric NBPNumericDeviceMetric</b></p><a name="NBPNumericDeviceMetric"> </a><a name="hcNBPNumericDeviceMetric"> </a><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px"/><p style="margin-bottom: 0px">Profile: <a href="StructureDefinition-NumericDeviceMetric.html">Numeric DeviceMetric profile</a></p></div><p><b>Metric availability extension</b>: intr</p><p><b>type</b>: <span title="Codes:{urn:iso:std:iso:11073:10101 150020}">NBP</span></p><p><b>unit</b>: <span title="Codes:{urn:iso:std:iso:11073:10101 266016}">mmHg</span></p><p><b>source</b>: <a href="Device-PhysioMonitorMdsDevice.html">Device: extension = ,-&gt;Practitioner Alice B. Careful ,8760,156,Dmo; identifier = urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680#01-23-45-67-89-AB-CD-EF; status = active; manufacturer = MyCompany; serialNumber = 123456; modelNumber = PM1; type = MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS</a></p><p><b>parent</b>: <a href="Device-NBPChannelDevice.html">Device: status = active; type = MDC_DEV_PRESS_BLD_NONINV_CHAN</a></p><p><b>operationalStatus</b>: On</p><p><b>color</b>: Color Red</p><p><b>category</b>: Measurement</p><p><b>measurementPeriod</b>: Once per 15 minutes</p></div>
      </text>
      <extension
                 url="http://hl7.org/fhir/uv/pocd/StructureDefinition/metric-availability">
        <valueCode value="intr"/>
      </extension>
      <type>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="150020"/>
          <display value="MDC_PRESS_BLD_NONINV"/>
        </coding>
        <text value="NBP"/>
      </type>
      <unit>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="266016"/>
          <display value="MDC_DIM_MMHG"/>
        </coding>
        <text value="mmHg"/>
      </unit>
      <source>🔗
        <reference value="Device/PhysioMonitorMdsDevice"/>
      </source>
      <parent>🔗
        <reference value="Device/NBPChannelDevice"/>
      </parent>
      <operationalStatus value="on"/>
      <color value="red"/>
      <category value="measurement"/>
      <measurementPeriod>
        <repeat>
          <frequency value="1"/>
          <period value="15"/>
          <periodUnit value="min"/>
        </repeat>
      </measurementPeriod>
    </DeviceMetric>