Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Resource Profile: VmdDevice - Detailed Descriptions

Page standards status: Trial-use | Maturity Level: 2

Definitions for the VmdDevice resource profile.

- Key Elements Table
- Differential Elements Table
- Snapshot Elements Table

Guidance on how to interpret the contents of this table can be foundhere

0. Device
Definition | A type of a manufactured item that is used in the provision of healthcare without being substantially changed through that activity. The device may be a medical or non-medical device.
Short | Item used in healthcare
Control | 0..*
Is Modifier | false
Summary | false
Invariants | dom-2: If the resource is contained in another resource, it SHALL NOT contain nested Resources (contained.contained.empty()) dom-3: If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource (contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()) dom-4: If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated (contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()) dom-5: If a resource is contained in another resource, it SHALL NOT have a security label (contained.meta.security.empty()) dom-6: A resource should have narrative for robust management (text.`div`.exists())
2. Device.implicitRules
Definition | A reference to a set of rules that were followed when the resource was constructed, and which must be understood when processing the content. Often, this is a reference to an implementation guide that defines the special rules along with other profiles etc.
Short | A set of rules under which this content was created
Comments | Asserting this rule set restricts the content to be only understood by a limited set of trading partners. This inherently limits the usefulness of the data in the long term. However, the existing health eco-system is highly fractured, and not yet ready to define, collect, and exchange data in a generally computable sense. Wherever possible, implementers and/or specification writers should avoid using this element. Often, when used, the URL is a reference to an implementation guide that defines these special rules as part of it's narrative along with other profiles, value sets, etc.
Control | 0..1
Type | uri
Is Modifier | true because This element is labeled as a modifier because the implicit rules may provide additional knowledge about the resource that modifies it's meaning or interpretation
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
4. Device.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the resource. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | ExtensionAdditional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
Slicing | This element introduces a set of slices on `Device.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
6. Device.extension:instance
Slice Name | instance
Definition | Instance number or label for multiple components of the same type.
Short | Instance number or label
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Device Instance extension) (Complex Extension)
Is Modifier | false
Must Support | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
8. Device.extension:instance.extension:number
Slice Name | number
Definition | An Extension
Short | Instance numberAdditional content defined by implementations
Control | 0..1*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
10. Device.extension:instance.extension:number.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `number`
12. Device.extension:instance.extension:number.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on `Device.extension.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
14. Device.extension:instance.extension:number.value[x]:valueUnsignedInt
Slice Name | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
16. Device.extension:instance.extension:label
Slice Name | label
Definition | An Extension
Short | Instance labelAdditional content defined by implementations
Control | 0..1*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
18. Device.extension:instance.extension:label.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `label`
20. Device.extension:instance.extension:label.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | string, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on `Device.extension.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
22. Device.extension:instance.extension:label.value[x]:valueString
Slice Name | valueString
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | string, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
24. Device.extension:instance.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance`
26. Device.extension:instance.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..01
Type | Choice of: base64Binary, boolean, canonical, code, date, dateTime, decimal, id, instant, integer, markdown, oid, positiveInt, string, time, unsignedInt, uri, url, uuid, Address, Age, Annotation, Attachment, Coding, ContactPoint, Count, Distance, Duration, HumanName, Identifier, Money, Period, Quantity, Range, Ratio, Reference, SampledData, Signature, Timing, ContactDetail, Contributor, DataRequirement, Expression, ParameterDefinition, RelatedArtifact, TriggerDefinition, UsageContext, Dosage, Meta, CodeableConcept
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
28. Device.extension:approvedJurisdictions
Slice Name | approvedJurisdictions
Definition | List of regions in which a device is approved to be operated.
Short | Approved jurisdictions
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Approved Jurisdictions extension) (Complex Extension)
Is Modifier | false
Must Support | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`) apj-1: When noApprovedJurisdictions is present, there shall be no approvedJurisdiction extensions. (`extension('noApprovedJurisdictions').exists() implies extension('approvedJurisdiction').empty()`)
30. Device.extension:approvedJurisdictions.extension:approvedJurisdiction
Slice Name | approvedJurisdiction
Definition | National state, territory, or region where the device is approved to be operated. If the list does not contain any entries, then the device or component is not approved for any region.
Short | Approved jurisdictionAdditional content defined by implementations
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
32. Device.extension:approvedJurisdictions.extension:approvedJurisdiction.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `approvedJurisdiction`
34. Device.extension:approvedJurisdictions.extension:approvedJurisdiction.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..1
Type | CodeableConcept, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on `Device.extension.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
36. Device.extension:approvedJurisdictions.extension:approvedJurisdiction.value[x]:valueCodeableConcept
Slice Name | valueCodeableConcept
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..1
Binding | Unless not suitable, these codes SHALL be taken from For codes, see Jurisdiction ValueSet (extensible to `http://hl7.org/fhir/ValueSet/jurisdiction` ) Codes for country, country subdivision and region
Type | CodeableConcept, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
38. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions
Slice Name | noApprovedJurisdictions
Definition | Explicit indication that the device has no approved jurisdictions. A value of false signals that the device is not approved for any region, as opposed to the jurisdiction being unknown. When this extension is present, there are no approved jurisdictions (yet).
Short | No approved jurisdictionsAdditional content defined by implementations
Control | 0..1*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
40. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `noApprovedJurisdictions`
42. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..1
Type | boolean, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on `Device.extension.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
44. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions.value[x]:valueBoolean
Slice Name | valueBoolean
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..1
Type | boolean, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Fixed Value | `true`
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
46. Device.extension:approvedJurisdictions.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/uv/pocd/StructureDefinition/approved-jurisdictions`
48. Device.extension:approvedJurisdictions.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..01
Type | Choice of: base64Binary, boolean, canonical, code, date, dateTime, decimal, id, instant, integer, markdown, oid, positiveInt, string, time, unsignedInt, uri, url, uuid, Address, Age, Annotation, Attachment, Coding, ContactPoint, Count, Distance, Duration, HumanName, Identifier, Money, Period, Quantity, Range, Ratio, Reference, SampledData, Signature, Timing, ContactDetail, Contributor, DataRequirement, Expression, ParameterDefinition, RelatedArtifact, TriggerDefinition, UsageContext, Dosage, Meta, CodeableConcept
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on `Device.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
50. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept
Slice Name | valueCodeableConcept
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..01
Type | CodeableConcept, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
52. Device.extension:operatingHours
Slice Name | operatingHours
Definition | Optional amount of operating hours (e.g., an OR light).
Short | Operating hours
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Operating hours extension) (Extension Type: unsignedInt)
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
54. Device.extension:operatingHours.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | ExtensionAdditional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..0*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
Slicing | This element introduces a set of slices on `Device.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
56. Device.extension:operatingHours.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours`
58. Device.extension:operatingHours.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on `Device.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
60. Device.extension:operatingHours.value[x]:valueUnsignedInt
Slice Name | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
62. Device.extension:operatingCycles
Slice Name | operatingCycles
Definition | Optional amount of operating cycles, e.g., the number of measurements taken within the component.
Short | Operating cycles
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Operating cycles extension) (Extension Type: unsignedInt)
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
64. Device.extension:operatingCycles.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | ExtensionAdditional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..0*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
Slicing | This element introduces a set of slices on `Device.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
66. Device.extension:operatingCycles.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles`
68. Device.extension:operatingCycles.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
Slicing | This element introduces a set of slices on `Device.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
70. Device.extension:operatingCycles.value[x]:valueUnsignedInt
Slice Name | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | unsignedInt, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
72. Device.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the resource and that modifies the understanding of the element that contains it and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer is allowed to define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the resource that contains them
Summary | false
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
74. Device.identifier
Definition | Unique instance identifiers assigned to a device by manufacturers other organizations or owners.
Short | Instance identifier
Comments | The barcode string from a barcode present on a device label or package may identify the instance, include names given to the device in local usage, or may identify the type of device. If the identifier identifies the type of device, Device.type element should be used.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 0..*
Type | Identifier
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
76. Device.identifier.use
Definition | The purpose of this identifier.
Short | usual | official | temp | secondary | old (If known)
Comments | Applications can assume that an identifier is permanent unless it explicitly says that it is temporary.
Control | 0..1
Binding | The codes SHALL be taken from IdentifierUse http://hl7.org/fhir/ValueSet/identifier-use|4.0.1 (required to `http://hl7.org/fhir/ValueSet/identifier-use|4.0.1` ) Identifies the purpose for this identifier, if known .
Type | code
Is Modifier | true because This is labeled as "Is Modifier" because applications should not mistake a temporary id for a permanent one.
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Allows the appropriate identifier for a particular context of use to be selected from among a set of identifiers.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
78. Device.identifier.system
Definition | Establishes the namespace for the value - that is, a URL that describes a set values that are unique.
Short | The namespace for the identifier value
Comments | Identifier.system is always case sensitive.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | There are many sets of identifiers. To perform matching of two identifiers, we need to know what set we're dealing with. The system identifies a particular set of unique identifiers.
Example | General: http://www.acme.com/identifiers/patient
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
80. Device.identifier.value
Definition | The portion of the identifier typically relevant to the user and which is unique within the context of the system.
Short | The value that is unique
Comments | If the value is a full URI, then the system SHALL be urn:ietf:rfc:3986. The value's primary purpose is computational mapping. As a result, it may be normalized for comparison purposes (e.g. removing non-significant whitespace, dashes, etc.) A value formatted for human display can be conveyed using the Rendered Value extension. Identifier.value is to be treated as case sensitive unless knowledge of the Identifier.system allows the processer to be confident that non-case-sensitive processing is safe.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Example | General: 123456
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
82. Device.udiCarrier
Definition | Unique device identifier (UDI) assigned to device label or package. Note that the Device may include multiple udiCarriers as it either may include just the udiCarrier for the jurisdiction it is sold, or for multiple jurisdictions it could have been sold.
Short | Unique Device Identifier (UDI) Barcode string
Comments | UDI may identify an unique instance of a device, or it may only identify the type of the device. See UDI mappings for a complete mapping of UDI parts to Device. UDI may identify an unique instance of a device, or it may only identify the type of the device. See UDI mappings for a complete mapping of UDI parts to Device.
Control | 0..*
Type | BackboneElement
Is Modifier | false
Must Support | true
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
84. Device.udiCarrier.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
86. Device.udiCarrier.deviceIdentifier
Definition | The device identifier (DI) is a mandatory, fixed portion of a UDI that identifies the labeler and the specific version or model of a device.
Short | Mandatory fixed portion of UDI
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | DI
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
88. Device.udiCarrier.issuer
Definition | Organization that is charged with issuing UDIs for devices. For example, the US FDA issuers include : GS1: http://hl7.org/fhir/NamingSystem/gs1-di, HIBCC: http://hl7.org/fhir/NamingSystem/hibcc-dI, ICCBBA for blood containers: http://hl7.org/fhir/NamingSystem/iccbba-blood-di, ICCBA for other devices: http://hl7.org/fhir/NamingSystem/iccbba-other-di.
Short | UDI Issuing Organization
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Barcode System
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
90. Device.udiCarrier.jurisdiction
Definition | The identity of the authoritative source for UDI generation within a jurisdiction. All UDIs are globally unique within a single namespace with the appropriate repository uri as the system. For example, UDIs of devices managed in the U.S. by the FDA, the value is http://hl7.org/fhir/NamingSystem/fda-udi.
Short | Regional UDI authority
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Requirements | Allows a recipient of a UDI to know which database will contain the UDI-associated metadata.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
92. Device.udiCarrier.carrierHRF
Definition | The full UDI carrier as the human readable form (HRF) representation of the barcode string as printed on the packaging of the device.
Short | UDI Human Readable Barcode String
Comments | If separate barcodes for DI and PI are present, concatenate the string with DI first and in order of human readable expression on label.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | Human Readable Form
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
94. Device.status
Definition | Status of the Device availability.
Short | active | inactive | entered-in-error | unknown
Comments | This element is labeled as a modifier because the status contains the codes inactive and entered-in-error that mark the device (record)as not currently valid.
Control | 0..1
Binding | The codes SHALL be taken from FHIRDeviceStatus http://hl7.org/fhir/ValueSet/device-status|4.0.1 (required to `http://hl7.org/fhir/ValueSet/device-status|4.0.1` ) The availability status of the device.
Type | code
Is Modifier | true because This element is labelled as a modifier because it is a status element that contains status entered-in-error which means that the resource should not be treated as valid
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
96. Device.statusReason
Definition | Reason for the dtatus of the Device availability.
Short | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off
Control | 0..*
Binding | Unless not suitable, these codes SHALL be taken from FHIRDeviceStatusReason http://hl7.org/fhir/ValueSet/device-status-reason|4.0.1 (extensible to `http://hl7.org/fhir/ValueSet/device-status-reason|4.0.1` ) The availability status reason of the device.
Type | CodeableConcept
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
98. Device.manufacturer
Definition | A name of the manufacturer.
Short | Name of device manufacturer
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
100. Device.manufactureDate
Definition | The date and time when the device was manufactured.
Short | Date when the device was made
Control | 0..1
Type | dateTime
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
102. Device.expirationDate
Definition | The date and time beyond which this device is no longer valid or should not be used (if applicable).
Short | Date and time of expiry of this device (if applicable)
Control | 0..1
Type | dateTime
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
104. Device.lotNumber
Definition | Lot number assigned by the manufacturer.
Short | Lot number of manufacture
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
106. Device.serialNumber
Definition | The serial number assigned by the organization when the device was manufactured.
Short | Serial number assigned by the manufacturer
Comments | Alphanumeric Maximum 20.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
108. Device.deviceName
Definition | This represents the manufacturer's name of the device as provided by the device, from a UDI label, or by a person describing the Device. This typically would be used when a person provides the name(s) or when the device represents one of the names available from DeviceDefinition.
Short | The name of the device as given by the manufacturer
Control | 0..*
Type | BackboneElement
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
110. Device.deviceName.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
112. Device.deviceName.name
Definition | The name of the device.
Short | The name of the device
Control | 1..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Σ
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
114. Device.deviceName.type
Definition | The type of deviceName. UDILabelName | UserFriendlyName | PatientReportedName | ManufactureDeviceName | ModelName.
Short | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other
Control | 1..1
Binding | The codes SHALL be taken from DeviceNameType http://hl7.org/fhir/ValueSet/device-nametype|4.0.1 (required to `http://hl7.org/fhir/ValueSet/device-nametype|4.0.1` ) The type of name the device is referred by.
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
116. Device.modelNumber
Definition | The model number for the device.
Short | The model number for the device
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
118. Device.partNumber
Definition | The part number of the device.
Short | The part number of the device
Comments | Alphanumeric Maximum 20.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
120. Device.type
Definition | The kind or type of device.
Short | The kind or type of device
Control | 10..1
Binding | Unless not suitable, these codes SHALL be taken from For example codes, see MDC Object infrastructure and Device nomenclature http://hl7.org/fhir/ValueSet/device-type|4.0.1 (extensible to `http://terminology.hl7.org/ValueSet/11073MDC-object` )
Type | CodeableConcept
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
122. Device.type.coding
Definition | A reference to a code defined by a terminology system.
Short | Code defined by a terminology system
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Control | 0..*
Type | Coding
Is Modifier | false
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
124. Device.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Short | Identity of the terminology system
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
126. Device.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Short | Version of the system - if relevant
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
128. Device.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Short | Symbol in syntax defined by the system
Control | 0..1
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
130. Device.type.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Short | Plain text representation of the concept
Comments | Very often the text is the same as a displayName of one of the codings.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
132. Device.version
Definition | The actual design of the device or software version running on the device.
Short | The actual design of the device or software version running on the device
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..*
Type | BackboneElement
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
134. Device.version.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
136. Device.version.type
Definition | The type of the device version.
Short | The type of the device version
Control | 0..1
Type | CodeableConcept
Is Modifier | false
Summary | false
Alternate Names | Σ
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
138. Device.version.type.coding
Definition | A reference to a code defined by a terminology system.
Short | Code defined by a terminology system
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Control | 0..*
Type | Coding
Is Modifier | false
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
140. Device.version.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Short | Identity of the terminology system
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
142. Device.version.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Short | Version of the system - if relevant
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
144. Device.version.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Short | Symbol in syntax defined by the system
Control | 0..1
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
146. Device.version.component
Definition | A single component of the device version.
Short | A single component of the device version
Control | 0..1
Type | Identifier
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
148. Device.version.value
Definition | The version text.
Short | The version text
Control | 1..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
150. Device.patient
Definition | Patient information, If the device is affixed to a person.
Short | Patient to whom Device is affixed
Control | 0..01
Type | Reference(Patient)
Is Modifier | false
Summary | false
Requirements | If the device is implanted in a patient, then need to associate the device to the patient.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
152. Device.location
Definition | The place where the device can be found.
Short | Where the device is found
Control | 0..01
Type | Reference(Location)
Is Modifier | false
Summary | false
Requirements | Device.location can be used to track device location.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
154. Device.safety
Definition | Provides additional safety characteristics about a medical device. For example devices containing latex.
Short | Safety Characteristics of Device
Control | 0..*
Type | CodeableConcept
Is Modifier | false
Must Support | true
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
156. Device.safety.coding
Definition | A reference to a code defined by a terminology system.
Short | Code defined by a terminology system
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Control | 0..*
Type | Coding
Is Modifier | false
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
158. Device.safety.coding.system
Definition | http://terminology.hl7.org/ValueSet/safety-classification The identification of the code system that defines the meaning of the symbol in the code.
Short | Identity of the terminology system
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
160. Device.safety.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Short | Symbol in syntax defined by the system
Control | 0..1
Binding | The codes SHALL be taken from For codes, see Safety Classification (required to `http://terminology.hl7.org/ValueSet/safety-classification` ) Safety classification
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
162. Device.parent
Definition | The parent device.
Short | The parent device
Control | 10..1
Type | Reference(MDS Device profile, Device)
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))

Guidance on how to interpret the contents of this table can be foundhere

0. Device
2. Device.extension
Slicing | This element introduces a set of slices on `Device.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
4. Device.extension:instance
Slice Name | instance
Definition | Instance number or label for multiple components of the same type.
Short | Instance number or label
Control | 0..1
Type | Extension(Device Instance extension) (Complex Extension)
Must Support | true
6. Device.extension:instance.extension:number
Slice Name | number
Short | Instance number
8. Device.extension:instance.extension:number.valueUnsignedInt
10. Device.extension:instance.extension:label
Slice Name | label
Short | Instance label
12. Device.extension:instance.extension:label.valueString
14. Device.extension:approvedJurisdictions
Slice Name | approvedJurisdictions
Definition | List of regions in which a device is approved to be operated.
Short | Approved jurisdictions
Type | Extension(Approved Jurisdictions extension) (Complex Extension)
Must Support | true
16. Device.extension:approvedJurisdictions.valueCodeableConcept
18. Device.extension:approvedJurisdictions.valueCodeableConcept.coding
20. Device.extension:approvedJurisdictions.valueCodeableConcept.coding.system
22. Device.extension:approvedJurisdictions.valueCodeableConcept.coding.code
24. Device.extension:operatingHours
Slice Name | operatingHours
Definition | Optional amount of operating hours (e.g., an OR light).
Short | Operating hours
Control | 0..1
Type | Extension(Operating hours extension) (Extension Type: unsignedInt)
Must Support | true
26. Device.extension:operatingHours.valueUnsignedInt
28. Device.extension:operatingCycles
Slice Name | operatingCycles
Definition | Optional amount of operating cycles, e.g., the number of measurements taken within the component.
Short | Operating cycles
Control | 0..1
Type | Extension(Operating cycles extension) (Extension Type: unsignedInt)
Must Support | true
30. Device.extension:operatingCycles.valueUnsignedInt
32. Device.identifier
Note | This is a business identifier, not a resource identifier (see discussion)
Must Support | true
34. Device.identifier.system
36. Device.identifier.value
38. Device.udiCarrier
Must Support | true
40. Device.udiCarrier.deviceIdentifier
42. Device.udiCarrier.issuer
44. Device.udiCarrier.jurisdiction
46. Device.udiCarrier.carrierHRF
48. Device.status
Must Support | true
50. Device.statusReason
Must Support | true
52. Device.manufacturer
Must Support | true
54. Device.manufactureDate
56. Device.expirationDate
58. Device.lotNumber
60. Device.serialNumber
Must Support | true
62. Device.deviceName
Must Support | true
64. Device.modelNumber
Must Support | true
66. Device.partNumber
Must Support | true
68. Device.type
Control | 1..?
Binding | Unless not suitable, these codes SHALL be taken from MDC Object infrastructure and Device nomenclature (extensible to `http://terminology.hl7.org/ValueSet/11073MDC-object` )
Must Support | true
70. Device.type.coding
72. Device.type.coding.system
74. Device.type.coding.version
Note | This is a business version Id, not a resource version Id (see discussion)
76. Device.type.coding.code
78. Device.type.text
80. Device.version
Note | This is a business version Id, not a resource version Id (see discussion)
Must Support | true
82. Device.version.type
84. Device.version.type.coding
86. Device.version.type.coding.system
88. Device.version.type.coding.version
Note | This is a business version Id, not a resource version Id (see discussion)
90. Device.version.type.coding.code
92. Device.version.component
94. Device.version.value
96. Device.patient
Control | 0..0
98. Device.location
Control | 0..0
100. Device.safety
Must Support | true
102. Device.safety.coding
104. Device.safety.coding.system
Definition | http://terminology.hl7.org/ValueSet/safety-classification
106. Device.safety.coding.code
Binding | The codes SHALL be taken from Safety Classification (required to `http://terminology.hl7.org/ValueSet/safety-classification` ) Safety classification
108. Device.parent
Control | 1..?
Type | Reference(MDS Device profile)
Must Support | true

Guidance on how to interpret the contents of this table can be foundhere

0. Device
Definition | A type of a manufactured item that is used in the provision of healthcare without being substantially changed through that activity. The device may be a medical or non-medical device.
Short | Item used in healthcare
Control | 0..*
Is Modifier | false
Summary | false
Invariants | dom-2: If the resource is contained in another resource, it SHALL NOT contain nested Resources (`contained.contained.empty()`) dom-3: If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource (`contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`) dom-4: If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated (`contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`) dom-5: If a resource is contained in another resource, it SHALL NOT have a security label (`contained.meta.security.empty()`) dom-6: A resource should have narrative for robust management (`text.`div`.exists()`)
2. Device.id
Definition | The logical id of the resource, as used in the URL for the resource. Once assigned, this value never changes.
Short | Logical id of this artifact
Comments | The only time that a resource does not have an id is when it is being submitted to the server using a create operation.
Control | 0..1
Type | id
Is Modifier | false
Summary | true
4. Device.meta
Definition | The metadata about the resource. This is content that is maintained by the infrastructure. Changes to the content might not always be associated with version changes to the resource.
Short | Metadata about the resource
Control | 0..1
Type | Meta
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
6. Device.implicitRules
Definition | A reference to a set of rules that were followed when the resource was constructed, and which must be understood when processing the content. Often, this is a reference to an implementation guide that defines the special rules along with other profiles etc.
Short | A set of rules under which this content was created
Comments | Asserting this rule set restricts the content to be only understood by a limited set of trading partners. This inherently limits the usefulness of the data in the long term. However, the existing health eco-system is highly fractured, and not yet ready to define, collect, and exchange data in a generally computable sense. Wherever possible, implementers and/or specification writers should avoid using this element. Often, when used, the URL is a reference to an implementation guide that defines these special rules as part of it's narrative along with other profiles, value sets, etc.
Control | 0..1
Type | uri
Is Modifier | true because This element is labeled as a modifier because the implicit rules may provide additional knowledge about the resource that modifies it's meaning or interpretation
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
8. Device.language
Definition | The base language in which the resource is written.
Short | Language of the resource content
Comments | Language is provided to support indexing and accessibility (typically, services such as text to speech use the language tag). The html language tag in the narrative applies to the narrative. The language tag on the resource may be used to specify the language of other presentations generated from the data in the resource. Not all the content has to be in the base language. The Resource.language should not be assumed to apply to the narrative automatically. If a language is specified, it should it also be specified on the div element in the html (see rules in HTML5 for information about the relationship between xml:lang and the html lang attribute).
Control | 0..1
Binding | The codes SHOULD be taken from CommonLanguages (preferred to `http://hl7.org/fhir/ValueSet/languages|4.0.1` ) A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
10. Device.text
Definition | A human-readable narrative that contains a summary of the resource and can be used to represent the content of the resource to a human. The narrative need not encode all the structured data, but is required to contain sufficient detail to make it "clinically safe" for a human to just read the narrative. Resource definitions may define what content should be represented in the narrative to ensure clinical safety.
Short | Text summary of the resource, for human interpretation
Comments | Contained resources do not have narrative. Resources that are not contained SHOULD have a narrative. In some cases, a resource may only have text with little or no additional discrete data (as long as all minOccurs=1 elements are satisfied). This may be necessary for data from legacy systems where information is captured as a "text blob" or where text is additionally entered raw or narrated and encoded information is added later.
Control | 0..1
Type | Narrative
Is Modifier | false
Summary | false
Alternate Names | narrative, html, xhtml, display
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
12. Device.contained
Definition | These resources do not have an independent existence apart from the resource that contains them - they cannot be identified independently, and nor can they have their own independent transaction scope.
Short | Contained, inline Resources
Comments | This should never be done when the content can be identified properly, as once identification is lost, it is extremely difficult (and context dependent) to restore it again. Contained resources may have profiles and tags In their meta elements, but SHALL NOT have security labels.
Control | 0..*
Type | Resource
Is Modifier | false
Summary | false
Alternate Names | inline resources, anonymous resources, contained resources
14. Device.extension
Definition | An Extension
Short | Extension
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
16. Device.extension:instance
Slice Name | instance
Definition | Instance number or label for multiple components of the same type.
Short | Instance number or label
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Device Instance extension) (Complex Extension)
Is Modifier | false
Must Support | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
18. Device.extension:instance.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
20. Device.extension:instance.extension
Definition | An Extension
Short | Extension
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
22. Device.extension:instance.extension:number
Slice Name | number
Definition | An Extension
Short | Instance number
Control | 0..1
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
24. Device.extension:instance.extension:number.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
26. Device.extension:instance.extension:number.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
28. Device.extension:instance.extension:number.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `number`
30. Device.extension:instance.extension:number.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | unsignedInt
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
Slicing | This element introduces a set of slices on `Device.extension.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
32. Device.extension:instance.extension:number.value[x]:valueUnsignedInt
Slice Name | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | unsignedInt
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
34. Device.extension:instance.extension:label
Slice Name | label
Definition | An Extension
Short | Instance label
Control | 0..1
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
36. Device.extension:instance.extension:label.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
38. Device.extension:instance.extension:label.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
40. Device.extension:instance.extension:label.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `label`
42. Device.extension:instance.extension:label.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | string
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
Slicing | This element introduces a set of slices on `Device.extension.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
44. Device.extension:instance.extension:label.value[x]:valueString
Slice Name | valueString
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | string
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
46. Device.extension:instance.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/uv/pocd/StructureDefinition/device-instance`
48. Device.extension:instance.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..0
Type | Choice of: base64Binary, boolean, canonical, code, date, dateTime, decimal, id, instant, integer, markdown, oid, positiveInt, string, time, unsignedInt, uri, url, uuid, Address, Age, Annotation, Attachment, Coding, ContactPoint, Count, Distance, Duration, HumanName, Identifier, Money, Period, Quantity, Range, Ratio, Reference, SampledData, Signature, Timing, ContactDetail, Contributor, DataRequirement, Expression, ParameterDefinition, RelatedArtifact, TriggerDefinition, UsageContext, Dosage, Meta
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
50. Device.extension:approvedJurisdictions
Slice Name | approvedJurisdictions
Definition | List of regions in which a device is approved to be operated.
Short | Approved jurisdictions
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Approved Jurisdictions extension) (Complex Extension)
Is Modifier | false
Must Support | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`) apj-1: When noApprovedJurisdictions is present, there shall be no approvedJurisdiction extensions. (`extension('noApprovedJurisdictions').exists() implies extension('approvedJurisdiction').empty()`)
52. Device.extension:approvedJurisdictions.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
54. Device.extension:approvedJurisdictions.extension
Definition | An Extension
Short | Extension
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
56. Device.extension:approvedJurisdictions.extension:approvedJurisdiction
Slice Name | approvedJurisdiction
Definition | National state, territory, or region where the device is approved to be operated. If the list does not contain any entries, then the device or component is not approved for any region.
Short | Approved jurisdiction
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
58. Device.extension:approvedJurisdictions.extension:approvedJurisdiction.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
60. Device.extension:approvedJurisdictions.extension:approvedJurisdiction.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
62. Device.extension:approvedJurisdictions.extension:approvedJurisdiction.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `approvedJurisdiction`
64. Device.extension:approvedJurisdictions.extension:approvedJurisdiction.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..1
Type | CodeableConcept
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
Slicing | This element introduces a set of slices on `Device.extension.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
66. Device.extension:approvedJurisdictions.extension:approvedJurisdiction.value[x]:valueCodeableConcept
Slice Name | valueCodeableConcept
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..1
Binding | Unless not suitable, these codes SHALL be taken from Jurisdiction ValueSet (extensible to `http://hl7.org/fhir/ValueSet/jurisdiction` ) Codes for country, country subdivision and region
Type | CodeableConcept
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
68. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions
Slice Name | noApprovedJurisdictions
Definition | Explicit indication that the device has no approved jurisdictions. A value of false signals that the device is not approved for any region, as opposed to the jurisdiction being unknown. When this extension is present, there are no approved jurisdictions (yet).
Short | No approved jurisdictions
Control | 0..1
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
70. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
72. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
74. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `noApprovedJurisdictions`
76. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..1
Type | boolean
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
Slicing | This element introduces a set of slices on `Device.extension.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
78. Device.extension:approvedJurisdictions.extension:noApprovedJurisdictions.value[x]:valueBoolean
Slice Name | valueBoolean
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..1
Type | boolean
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Fixed Value | `true`
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
80. Device.extension:approvedJurisdictions.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/uv/pocd/StructureDefinition/approved-jurisdictions`
82. Device.extension:approvedJurisdictions.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..0
Type | Choice of: base64Binary, boolean, canonical, code, date, dateTime, decimal, id, instant, integer, markdown, oid, positiveInt, string, time, unsignedInt, uri, url, uuid, Address, Age, Annotation, Attachment, Coding, ContactPoint, Count, Distance, Duration, HumanName, Identifier, Money, Period, Quantity, Range, Ratio, Reference, SampledData, Signature, Timing, ContactDetail, Contributor, DataRequirement, Expression, ParameterDefinition, RelatedArtifact, TriggerDefinition, UsageContext, Dosage, Meta
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
Slicing | This element introduces a set of slices on `Device.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
84. Device.extension:approvedJurisdictions.value[x]:valueCodeableConcept
Slice Name | valueCodeableConcept
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 0..0
Type | CodeableConcept
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
97. Device.extension:operatingHours
Slice Name | operatingHours
Definition | Optional amount of operating hours (e.g., an OR light).
Short | Operating hours
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Operating hours extension) (Extension Type: unsignedInt)
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
99. Device.extension:operatingHours.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
101. Device.extension:operatingHours.extension
Definition | An Extension
Short | Extension
Control | 0..0
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
103. Device.extension:operatingHours.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-hours`
105. Device.extension:operatingHours.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | unsignedInt
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
Slicing | This element introduces a set of slices on `Device.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
107. Device.extension:operatingHours.value[x]:valueUnsignedInt
Slice Name | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | unsignedInt
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
109. Device.extension:operatingCycles
Slice Name | operatingCycles
Definition | Optional amount of operating cycles, e.g., the number of measurements taken within the component.
Short | Operating cycles
Control | 0..1 This element is affected by the following invariants: ele-1
Type | Extension(Operating cycles extension) (Extension Type: unsignedInt)
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
111. Device.extension:operatingCycles.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
113. Device.extension:operatingCycles.extension
Definition | An Extension
Short | Extension
Control | 0..0
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
115. Device.extension:operatingCycles.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/uv/pocd/StructureDefinition/operating-cycles`
117. Device.extension:operatingCycles.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | unsignedInt
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
Slicing | This element introduces a set of slices on `Device.extension.value[x]`. The slices areUnordered and Closed, and can be differentiated using the following discriminators: type @ $this
119. Device.extension:operatingCycles.value[x]:valueUnsignedInt
Slice Name | valueUnsignedInt
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | unsignedInt
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
121. Device.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the resource and that modifies the understanding of the element that contains it and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer is allowed to define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the resource that contains them
Summary | false
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
123. Device.identifier
Definition | Unique instance identifiers assigned to a device by manufacturers other organizations or owners.
Short | Instance identifier
Comments | The barcode string from a barcode present on a device label or package may identify the instance, include names given to the device in local usage, or may identify the type of device. If the identifier identifies the type of device, Device.type element should be used.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 0..*
Type | Identifier
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
125. Device.identifier.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
127. Device.identifier.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.identifier.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
129. Device.identifier.use
Definition | The purpose of this identifier.
Short | usual | official | temp | secondary | old (If known)
Comments | Applications can assume that an identifier is permanent unless it explicitly says that it is temporary.
Control | 0..1
Binding | The codes SHALL be taken from IdentifierUse (required to `http://hl7.org/fhir/ValueSet/identifier-use|4.0.1` ) Identifies the purpose for this identifier, if known .
Type | code
Is Modifier | true because This is labeled as "Is Modifier" because applications should not mistake a temporary id for a permanent one.
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Allows the appropriate identifier for a particular context of use to be selected from among a set of identifiers.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
131. Device.identifier.type
Definition | A coded type for the identifier that can be used to determine which identifier to use for a specific purpose.
Short | Description of identifier
Comments | This element deals only with general categories of identifiers. It SHOULD not be used for codes that correspond 1..1 with the Identifier.system. Some identifiers may fall into multiple categories due to common usage. Where the system is known, a type is unnecessary because the type is always part of the system definition. However systems often need to handle identifiers where the system is not known. There is not a 1:1 relationship between type and system, since many different systems have the same type.
Control | 0..1
Binding | Unless not suitable, these codes SHALL be taken from Identifier Type Codes (extensible to `http://hl7.org/fhir/ValueSet/identifier-type|4.0.1` ) A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
Type | CodeableConcept
Is Modifier | false
Summary | true
Requirements | Allows users to make use of identifiers when the identifier system is not known.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
133. Device.identifier.system
Definition | Establishes the namespace for the value - that is, a URL that describes a set values that are unique.
Short | The namespace for the identifier value
Comments | Identifier.system is always case sensitive.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | There are many sets of identifiers. To perform matching of two identifiers, we need to know what set we're dealing with. The system identifies a particular set of unique identifiers.
Example | General: http://www.acme.com/identifiers/patient
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
135. Device.identifier.value
Definition | The portion of the identifier typically relevant to the user and which is unique within the context of the system.
Short | The value that is unique
Comments | If the value is a full URI, then the system SHALL be urn:ietf:rfc:3986. The value's primary purpose is computational mapping. As a result, it may be normalized for comparison purposes (e.g. removing non-significant whitespace, dashes, etc.) A value formatted for human display can be conveyed using the Rendered Value extension. Identifier.value is to be treated as case sensitive unless knowledge of the Identifier.system allows the processer to be confident that non-case-sensitive processing is safe.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Example | General: 123456
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
137. Device.identifier.period
Definition | Time period during which identifier is/was valid for use.
Short | Time period when id is/was valid for use
Control | 0..1
Type | Period
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
139. Device.identifier.assigner
Definition | Organization that issued/manages the identifier.
Short | Organization that issued id (may be just text)
Comments | The Identifier.assigner may omit the .reference element and only contain a .display element reflecting the name or other textual information about the assigning organization.
Control | 0..1
Type | Reference(Organization)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
141. Device.definition
Definition | The reference to the definition for the device.
Short | The reference to the definition for the device
Control | 0..1
Type | Reference(DeviceDefinition)
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
143. Device.udiCarrier
Definition | Unique device identifier (UDI) assigned to device label or package. Note that the Device may include multiple udiCarriers as it either may include just the udiCarrier for the jurisdiction it is sold, or for multiple jurisdictions it could have been sold.
Short | Unique Device Identifier (UDI) Barcode string
Comments | UDI may identify an unique instance of a device, or it may only identify the type of the device. See UDI mappings for a complete mapping of UDI parts to Device.
Control | 0..*
Type | BackboneElement
Is Modifier | false
Must Support | true
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
145. Device.udiCarrier.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
147. Device.udiCarrier.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
149. Device.udiCarrier.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
151. Device.udiCarrier.deviceIdentifier
Definition | The device identifier (DI) is a mandatory, fixed portion of a UDI that identifies the labeler and the specific version or model of a device.
Short | Mandatory fixed portion of UDI
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | DI
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
153. Device.udiCarrier.issuer
Definition | Organization that is charged with issuing UDIs for devices. For example, the US FDA issuers include : GS1: http://hl7.org/fhir/NamingSystem/gs1-di, HIBCC: http://hl7.org/fhir/NamingSystem/hibcc-dI, ICCBBA for blood containers: http://hl7.org/fhir/NamingSystem/iccbba-blood-di, ICCBA for other devices: http://hl7.org/fhir/NamingSystem/iccbba-other-di.
Short | UDI Issuing Organization
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Barcode System
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
155. Device.udiCarrier.jurisdiction
Definition | The identity of the authoritative source for UDI generation within a jurisdiction. All UDIs are globally unique within a single namespace with the appropriate repository uri as the system. For example, UDIs of devices managed in the U.S. by the FDA, the value is http://hl7.org/fhir/NamingSystem/fda-udi.
Short | Regional UDI authority
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Requirements | Allows a recipient of a UDI to know which database will contain the UDI-associated metadata.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
157. Device.udiCarrier.carrierAIDC
Definition | The full UDI carrier of the Automatic Identification and Data Capture (AIDC) technology representation of the barcode string as printed on the packaging of the device - e.g., a barcode or RFID. Because of limitations on character sets in XML and the need to round-trip JSON data through XML, AIDC Formats SHALL be base64 encoded.
Short | UDI Machine Readable Barcode String
Comments | The AIDC form of UDIs should be scanned or otherwise used for the identification of the device whenever possible to minimize errors in records resulting from manual transcriptions. If separate barcodes for DI and PI are present, concatenate the string with DI first and in order of human readable expression on label.
Control | 0..1
Type | base64Binary
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | Automatic Identification and Data Capture
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
159. Device.udiCarrier.carrierHRF
Definition | The full UDI carrier as the human readable form (HRF) representation of the barcode string as printed on the packaging of the device.
Short | UDI Human Readable Barcode String
Comments | If separate barcodes for DI and PI are present, concatenate the string with DI first and in order of human readable expression on label.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Alternate Names | Human Readable Form
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
161. Device.udiCarrier.entryType
Definition | A coded entry to indicate how the data was entered.
Short | barcode | rfid | manual +
Control | 0..1
Binding | The codes SHALL be taken from UDIEntryType (required to `http://hl7.org/fhir/ValueSet/udi-entry-type|4.0.1` ) Codes to identify how UDI data was entered.
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Requirements | Supports a way to distinguish hand entered from machine read data.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
163. Device.status
Definition | Status of the Device availability.
Short | active | inactive | entered-in-error | unknown
Comments | This element is labeled as a modifier because the status contains the codes inactive and entered-in-error that mark the device (record)as not currently valid.
Control | 0..1
Binding | The codes SHALL be taken from FHIRDeviceStatus (required to `http://hl7.org/fhir/ValueSet/device-status|4.0.1` ) The availability status of the device.
Type | code
Is Modifier | true because This element is labelled as a modifier because it is a status element that contains status entered-in-error which means that the resource should not be treated as valid
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
165. Device.statusReason
Definition | Reason for the dtatus of the Device availability.
Short | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off
Control | 0..*
Binding | Unless not suitable, these codes SHALL be taken from FHIRDeviceStatusReason (extensible to `http://hl7.org/fhir/ValueSet/device-status-reason|4.0.1` ) The availability status reason of the device.
Type | CodeableConcept
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
167. Device.distinctIdentifier
Definition | The distinct identification string as required by regulation for a human cell, tissue, or cellular and tissue-based product.
Short | The distinct identification string
Comments | For example, this applies to devices in the United States regulated under Code of Federal Regulation 21CFR§1271.290(c).
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Distinct Identification Code (DIC)
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
169. Device.manufacturer
Definition | A name of the manufacturer.
Short | Name of device manufacturer
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
171. Device.manufactureDate
Definition | The date and time when the device was manufactured.
Short | Date when the device was made
Control | 0..1
Type | dateTime
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
173. Device.expirationDate
Definition | The date and time beyond which this device is no longer valid or should not be used (if applicable).
Short | Date and time of expiry of this device (if applicable)
Control | 0..1
Type | dateTime
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
175. Device.lotNumber
Definition | Lot number assigned by the manufacturer.
Short | Lot number of manufacture
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
177. Device.serialNumber
Definition | The serial number assigned by the organization when the device was manufactured.
Short | Serial number assigned by the manufacturer
Comments | Alphanumeric Maximum 20.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
179. Device.deviceName
Definition | This represents the manufacturer's name of the device as provided by the device, from a UDI label, or by a person describing the Device. This typically would be used when a person provides the name(s) or when the device represents one of the names available from DeviceDefinition.
Short | The name of the device as given by the manufacturer
Control | 0..*
Type | BackboneElement
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
181. Device.deviceName.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
183. Device.deviceName.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
185. Device.deviceName.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
187. Device.deviceName.name
Definition | The name of the device.
Short | The name of the device
Control | 1..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Alternate Names | Σ
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
189. Device.deviceName.type
Definition | The type of deviceName. UDILabelName | UserFriendlyName | PatientReportedName | ManufactureDeviceName | ModelName.
Short | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other
Control | 1..1
Binding | The codes SHALL be taken from DeviceNameType (required to `http://hl7.org/fhir/ValueSet/device-nametype|4.0.1` ) The type of name the device is referred by.
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
191. Device.modelNumber
Definition | The model number for the device.
Short | The model number for the device
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
193. Device.partNumber
Definition | The part number of the device.
Short | The part number of the device
Comments | Alphanumeric Maximum 20.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
195. Device.type
Definition | The kind or type of device.
Short | The kind or type of device
Control | 1..1
Binding | Unless not suitable, these codes SHALL be taken from MDC Object infrastructure and Device nomenclature (extensible to `http://terminology.hl7.org/ValueSet/11073MDC-object` )
Type | CodeableConcept
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
197. Device.type.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
199. Device.type.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.type.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
201. Device.type.coding
Definition | A reference to a code defined by a terminology system.
Short | Code defined by a terminology system
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Control | 0..*
Type | Coding
Is Modifier | false
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
203. Device.type.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
205. Device.type.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.type.coding.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
207. Device.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Short | Identity of the terminology system
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
209. Device.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Short | Version of the system - if relevant
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
211. Device.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Short | Symbol in syntax defined by the system
Control | 0..1
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
213. Device.type.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Short | Representation defined by the system
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
215. Device.type.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Short | If this coding was chosen directly by the user
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Control | 0..1
Type | boolean
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
217. Device.type.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Short | Plain text representation of the concept
Comments | Very often the text is the same as a displayName of one of the codings.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
219. Device.specialization
Definition | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication.
Short | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
Control | 0..*
Type | BackboneElement
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
221. Device.specialization.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
223. Device.specialization.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
225. Device.specialization.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
227. Device.specialization.systemType
Definition | The standard that is used to operate and communicate.
Short | The standard that is used to operate and communicate
Control | 1..1
Type | CodeableConcept
Is Modifier | false
Summary | false
Alternate Names | Σ
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
229. Device.specialization.version
Definition | The version of the standard that is used to operate and communicate.
Short | The version of the standard that is used to operate and communicate
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
231. Device.version
Definition | The actual design of the device or software version running on the device.
Short | The actual design of the device or software version running on the device
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..*
Type | BackboneElement
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
233. Device.version.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
235. Device.version.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
237. Device.version.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
239. Device.version.type
Definition | The type of the device version.
Short | The type of the device version
Control | 0..1
Type | CodeableConcept
Is Modifier | false
Summary | false
Alternate Names | Σ
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
241. Device.version.type.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
243. Device.version.type.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.version.type.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
245. Device.version.type.coding
Definition | A reference to a code defined by a terminology system.
Short | Code defined by a terminology system
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Control | 0..*
Type | Coding
Is Modifier | false
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
247. Device.version.type.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
249. Device.version.type.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.version.type.coding.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
251. Device.version.type.coding.system
Definition | The identification of the code system that defines the meaning of the symbol in the code.
Short | Identity of the terminology system
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
253. Device.version.type.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Short | Version of the system - if relevant
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
255. Device.version.type.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Short | Symbol in syntax defined by the system
Control | 0..1
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
257. Device.version.type.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Short | Representation defined by the system
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
259. Device.version.type.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Short | If this coding was chosen directly by the user
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Control | 0..1
Type | boolean
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
261. Device.version.type.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Short | Plain text representation of the concept
Comments | Very often the text is the same as a displayName of one of the codings.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
263. Device.version.component
Definition | A single component of the device version.
Short | A single component of the device version
Control | 0..1
Type | Identifier
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
265. Device.version.value
Definition | The version text.
Short | The version text
Control | 1..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
267. Device.property
Definition | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties.
Short | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
Control | 0..*
Type | BackboneElement
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
269. Device.property.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
271. Device.property.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
273. Device.property.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
275. Device.property.type
Definition | Code that specifies the property DeviceDefinitionPropetyCode (Extensible).
Short | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
Control | 1..1
Type | CodeableConcept
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
277. Device.property.valueQuantity
Definition | Property value as a quantity.
Short | Property value as a quantity
Control | 0..*
Type | Quantity
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
279. Device.property.valueCode
Definition | Property value as a code, e.g., NTP4 (synced to NTP).
Short | Property value as a code, e.g., NTP4 (synced to NTP)
Control | 0..*
Type | CodeableConcept
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
281. Device.patient
Definition | Patient information, If the device is affixed to a person.
Short | Patient to whom Device is affixed
Control | 0..0
Type | Reference(Patient)
Is Modifier | false
Summary | false
Requirements | If the device is implanted in a patient, then need to associate the device to the patient.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
283. Device.owner
Definition | An organization that is responsible for the provision and ongoing maintenance of the device.
Short | Organization responsible for device
Control | 0..1
Type | Reference(Organization)
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
285. Device.contact
Definition | Contact details for an organization or a particular human that is responsible for the device.
Short | Details for human/organization for support
Comments | used for troubleshooting etc.
Control | 0..*
Type | ContactPoint
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
287. Device.location
Definition | The place where the device can be found.
Short | Where the device is found
Control | 0..0
Type | Reference(Location)
Is Modifier | false
Summary | false
Requirements | Device.location can be used to track device location.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
289. Device.url
Definition | A network address on which the device may be contacted directly.
Short | Network address to contact device
Comments | If the device is running a FHIR server, the network address should be the Base URL from which a conformance statement may be retrieved.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
291. Device.note
Definition | Descriptive information, usage information or implantation information that is not captured in an existing element.
Short | Device notes and comments
Control | 0..*
Type | Annotation
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
293. Device.safety
Definition | Provides additional safety characteristics about a medical device. For example devices containing latex.
Short | Safety Characteristics of Device
Control | 0..*
Type | CodeableConcept
Is Modifier | false
Must Support | true
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
295. Device.safety.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
297. Device.safety.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.safety.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
299. Device.safety.coding
Definition | A reference to a code defined by a terminology system.
Short | Code defined by a terminology system
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Control | 0..*
Type | Coding
Is Modifier | false
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
301. Device.safety.coding.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
303. Device.safety.coding.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Device.safety.coding.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
305. Device.safety.coding.system
Definition | http://terminology.hl7.org/ValueSet/safety-classification
Short | Identity of the terminology system
Comments | The URI may be an OID (urn:oid:...) or a UUID (urn:uuid:...). OIDs and UUIDs SHALL be references to the HL7 OID registry. Otherwise, the URI should come from HL7's list of FHIR defined special URIs or it should reference to some definition that establishes the system clearly and unambiguously.
Control | 0..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be unambiguous about the source of the definition of the symbol.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
307. Device.safety.coding.version
Definition | The version of the code system which was used when choosing this code. Note that a well-maintained code system does not need the version reported, because the meaning of codes is consistent across versions. However this cannot consistently be assured, and when the meaning is not guaranteed to be consistent, the version SHOULD be exchanged.
Short | Version of the system - if relevant
Comments | Where the terminology does not clearly define what string should be used to identify code system versions, the recommendation is to use the date (expressed in FHIR date format) on which that version was officially published as the version date.
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
309. Device.safety.coding.code
Definition | A symbol in syntax defined by the system. The symbol may be a predefined code or an expression in a syntax defined by the coding system (e.g. post-coordination).
Short | Symbol in syntax defined by the system
Control | 0..1
Binding | The codes SHALL be taken from Safety Classification (required to `http://terminology.hl7.org/ValueSet/safety-classification` ) Safety classification
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to refer to a particular code in the system.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
311. Device.safety.coding.display
Definition | A representation of the meaning of the code in the system, following the rules of the system.
Short | Representation defined by the system
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Need to be able to carry a human-readable meaning of the code for readers that do not know the system.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
313. Device.safety.coding.userSelected
Definition | Indicates that this coding was chosen by a user directly - e.g. off a pick list of available items (codes or displays).
Short | If this coding was chosen directly by the user
Comments | Amongst a set of alternatives, a directly chosen code is the most appropriate starting point for new translations. There is some ambiguity about what exactly 'directly chosen' implies, and trading partner agreement may be needed to clarify the use of this element and its consequences more completely.
Control | 0..1
Type | boolean
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | This has been identified as a clinical safety criterium - that this exact system/code pair was chosen explicitly, rather than inferred by the system based on some rules or language processing.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
315. Device.safety.text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Short | Plain text representation of the concept
Comments | Very often the text is the same as a displayName of one of the codings.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
317. Device.parent
Definition | The parent device.
Short | The parent device
Control | 1..1
Type | Reference(MDS Device profile)
Is Modifier | false
Must Support | true
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)