Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Rhythm Status Enumeration observation example - TTL Representation

Page standards status: Informative

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdf: <http://www.w3.org/1999/02/22-rdf-syntax-ns#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:Observation ;
      fhir:nodeRole fhir:treeRoot ;
      fhir:id [ fhir:v "RhythmStatusEnumerationObservation"] ; #
      fhir:meta [
        ( fhir:profile [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/EnumerationObservation"^^xsd:anyURI ;
    fhir:l <http://hl7.org/fhir/uv/pocd/StructureDefinition/EnumerationObservation>     ] )
      ] ; #
      fhir:text [
    fhir:status [ fhir:v "generated" ] ;
    fhir:div [ fhir:v "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p class=\"res-header-id\"><b>Generated Narrative: Observation RhythmStatusEnumerationObservation</b></p><a name=\"RhythmStatusEnumerationObservation\"> </a><a name=\"hcRhythmStatusEnumerationObservation\"> </a><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\"/><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-EnumerationObservation.html\">Enumeration Observation profile</a></p></div><p><b>status</b>: Final</p><p><b>code</b>: <span title=\"Codes:{urn:iso:std:iso:11073:10101 184327}\">MDC_ECG_STAT_RHY</span></p><p><b>subject</b>: <a href=\"Patient-SomePatient.html\">John Doe  Male, DoB: 1967-05-04 ( Medical record number)</a></p><p><b>effective</b>: 2021-07-09 11:33:24+0200</p><p><b>value</b>: <span title=\"Codes:{urn:iso:std:iso:11073:10101 147474}\">Sinus rhythm</span></p><p><b>device</b>: <a href=\"DeviceMetric-RhythmStatusEnumerationDeviceMetric.html\">DeviceMetric: type = MDC_ECG_STAT_RHY; operationalStatus = on; category = measurement</a></p></div>"^^rdf:XMLLiteral ]
      ] ; #
      fhir:status [ fhir:v "final"] ; #
      fhir:code [
        ( fhir:coding [
    fhir:system [
    fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ;
    fhir:l <urn:iso:std:iso:11073:10101>       ] ;
    fhir:code [ fhir:v "184327" ] ;
    fhir:display [ fhir:v "MDC_ECG_STAT_RHY" ]     ] )
      ] ; #
      fhir:subject [
    fhir:l fhir:Patient/SomePatient ;
    fhir:reference [ fhir:v "Patient/SomePatient" ]
      ] ; #
      fhir:effective [
    a fhir:DateTime ;
    fhir:v "2021-07-09T11:33:24+02:00"^^xsd:dateTime
      ] ; #
      fhir:value [
    a fhir:CodeableConcept ;
        ( fhir:coding [
    fhir:system [
    fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ;
    fhir:l <urn:iso:std:iso:11073:10101>       ] ;
    fhir:code [ fhir:v "147474" ] ;
    fhir:display [ fhir:v "MDC_ECG_SINUS_RHY" ]     ] ) ;
    fhir:text [ fhir:v "Sinus rhythm" ]
      ] ; #
      fhir:device [
    fhir:l fhir:DeviceMetric/RhythmStatusEnumerationDeviceMetric ;
    fhir:reference [ fhir:v "DeviceMetric/RhythmStatusEnumerationDeviceMetric" ]
      ] . #